
D 3 7 6 1    NEC
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders        |  915|     |
Capacity form/unform   114/      MB        Heads            |    7|     |
Seek time   / track  20.0/     ms          Sector/track     |   35|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate    1.250 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle           8.0 W     Shock        g                 |
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
NEC      D3761  APPLICATION NOTE

 Jumper Settings
 ===============

 x = Factory default setting


 Drive Switching
 ---------------

        +------+
  x MSI | xxxx | Drive C: (Master)
    SLV | o  o | Drive D: (Slave)
    BSC | o  o |
  x TRS | xxxx | Native/Translation mode
    FC  | o  o | FC- mode with 776 cylinder, 8 heads,
        +------+ 33 sectors


 Logical Parameter
 -----------------
 BIOS Typ depending



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
NEC      D3761  APPLICATION NOTE

 INSTALLATION PROCEDURE
 ======================


 System Embedded Controller

 - Set up Type:
   AMI-BIOS: 31 (98MB)
   AWARD-BIOS: 30 (109MB)
   PHOENIX-BIOS: 35 (80MB) or
   USER Type 48/49 with physical parameters
   (not for NOVELL 2.15 / ELS
 - FDISK
 - FORMAT C:/S


 External Adapter
 ----------------
 Adapter with no BIOS see above

 Adapter with BIOS: NCL 538/539
  - Set up Type: Typ 3 (114MB)
  - FDISK
  - FORMAT C:/S


 SOFTWARE
 --------
 DOS 3.30 and up

 NOVELL ELS I/II
 NOVELL 2.15
 NOVELL 386

 UNIX/XENIX

 Drive needs to be low level formatted if you do not work with
 physical parameter.

 Programs can be:
 - HDFORMAT
 - HARDPREP
 - INITFIX
 - WDFMT



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
NEC      NEC DRIVES  INSTALLATION GUIDE DEC. 92 REV. A

 NEC drives
 -----------
 The NEC IDE/SCSI drives are designed to work in the IBM AT and
 compatible systems and gurantee the operation with any standard IDE
 and SCSI Controller. Further, the NEC drives provide compatibility to
 the ATA/SCSI CAM and ANSI (X3-131-199x) standard as well as to all
 known operating systems.


