
2 5 1 3 5 0 A       M O B I L E   M A X    MAXTOR
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        | 2616|     |
Capacity form/unform  1350/      MB        Heads           8|   16|     |
Seek time   / track  13.0/ 4.5 ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate    6.000 MB/S int       Bytes/Sector      512
                     13.300 MB/S ext PIO4
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 71
Power: sleep          0.1 W     Humidity     %         5 95    |      5 95
       standby        0.2 W     Altitude    km    -0.061  3.048|
       idle           0.9 W     Shock        g       100       |    300
       seek           1.7 W     Rotation   RPM      4464
       read/write     1.9 W     Acoustic   dBA        35
       spin-up        4.4 W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   251350/251010/250840  JUMPER SETTING


                            Back of Drive
    +----------------------------------------------------------+
    |      Pin 41 +5V                                          |
    |      |                                       1   C A     |
    +------+---------------------------------------------------+
    | |  o o o o o o o o o o o o o o o o o o o o o o   o o   | |
    | |  o o o o o o o o o o o o   o o o o o o o o o   o o   | |
    +------+---------------------+-----------------------------+
           |                     |                     D B
           Pin 42 +5V            Pin 20 Key










**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   251350/251010/250840  JUMPER SETTING

 Jumper Setting
 ==============

 Cable Select Option
 -------------------
 The drive can be configured so the status of a master or slave can be
 determined by the cabling from the host system. The drive can
 recognize it self as either Drive 0 or Drive 1.

 The drive is configured as either a master (drive 0) or a slave
 (drive 1) depending on the value of the CSEL signal (pin 28). If CSEL
 is grounded, then the drive address - 0. If CSEL is open, then the
 drive address - 1.

 Special cabling is required from the system manfacturer to selectivly
 ground or open the CSEL signal.


   +-------------------------------------+---+---+---+
   |          JUMPER DESIGNATION         |D-B|A-B|C-D|
   +-------------------------------------+---+---+---+
   | Cable Select                        |   |   |   |
   | ------------                        |   |   |   |
   |  Disabled*                          | O |   |   |
   |                                     +---+---+---+
   |  Enabled                            | J |   |   |
   +-------------------------------------+---+---+---+
   | Master/Slave                        |   |   |   |
   |  Only drive in single drive system* |   | J | O |
   +-------------------------------------+---+---+---+
   |  Master in dual drive system*       |   | J | O |
   +-------------------------------------+---+---+---+
   |  Slave in dual drive system         |   | O | J |
   +-------------------------------------+---+---+---+
   J>Jumpered O>Open *>Default



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
MAXTOR    IDE INSTALLATION

            INSTALLATION PROCEDURE FOR AN IDE DRIVE
            ---------------------------------------
 1. Install a 40 pin Data Cable ensuring that pin 1, which can be
    identified by the striped edge of the cable, is closest to the
    power connector on the drive.

 2. Install a DC power cable to the back of the drive.

 3. Verify the jumper configurations for Master/Slave operation
    (Note:  Master will be the bootable drive. The slave will not
    be bootable.) Also make sure the existing C: drive is jumped
    to be the Master in a two drive system, not the only drive in
    the system.

 4. Apply power to the computer.

 4a. When memory test is complete go into your system's Standard
     CMOS set-up.
     (Note: There are various ways to get into CMOS set-up, please
     refer to system's manual for instructions.)

 4b. If your system's BIOS supports a user programmable drive
     type, program the BIOS with the default parameters of your
     drive. If your system does not support a user programmable
     drive type choose parameters that closely match but do not
     exceed the drives MegaByte capacity. Escape from set-up
     then choose write to CMOS and exit.

 5. Boot from a DOS diskette that has FDISK.EXE and FORMAT.COM on
    it. At the A> prompt type in FDISK. At the menu options select
    option 1 to create a DOS partition. Another menu will appear
    and from those options choose 1 to create a Primary DOS
    partition. Select yes to make 1 large partition and it will
    automatically become active. Then escape from FDISK.

 6. At the A> prompt type in FORMAT C:/S This does a high-level
    format on the drive and transfers the system files in order for
    the drive to be bootable. (Note: IDE drives are low-level
    formatted from the manufacturer and only need a high-level
    format).

    To configure the drive as a slave drive repeat steps 1-4 and
    proceed with steps 5a. and 6a. as follows:

  5a. At the C> prompt type in FDISK. When the menu options appear
      select option 5 to switch to the second drive. Enter fixed
      disk drive number 2. Then choose option 1 to create a DOS
      partition, then select option 1 again to create a Primary DOS
      partition or option 2 to create an Extended DOS partition.
      (Note: C and D drives will always be the Primary partitions
      but only the Primary partition on C: will have a status of
      active).

  6a. Proceed with a high-level format on the drive by typing FORMAT
      D: (Note: Make sure the correct drive letter has been selected
      for format).

 7. The drive is now bootable. As a test remove the DOS diskette
    from A and press reset to reboot the computer,  a  C> should be
    displayed, the drive is now ready for operation.


