
M 3 1 3 0 S    MINISCRIBE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/HH              Cylinders    1255|     |     |
Capacity form/unform   112/  131 MB        Heads           5|     |     |
Seek time   / track  17.0/ 3.5 ms          Sector/track   35|     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate    1.250 MB/S int       Bytes/Sector      512
                      4.000 MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C        10 50    |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      3600
       read/write    15.0 W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      35000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MINISC.  3130S

 Jumper Setting
 ==============

 SCSI ADDRESS SETTINGS (J601)
 ----------------------------
                    J601-1,2       J601-3,4       J601-5,6
                    --------       --------       --------
 SCSI ADDRESS  0      OFF            OFF            OFF
 SCSI ADDRESS  1      OFF            OFF            ON
 SCSI ADDRESS  2      OFF            ON             OFF
 SCSI ADDRESS  3      OFF            ON             ON
 SCSI ADDRESS  4      ON             OFF            OFF
 SCSI ADDRESS  5      ON             OFF            ON
 SCSI ADDRESS  6      ON             ON             ON


 THESE JUMPERS ARE THE FACTORY DEFAULT SETTINGS
 ----------------------------------------------
 J-510, J-21, J-20, J-14, J-27, J-2, J-13, J-24, J-30, J-29.


 SECTOR CONFIGURATION
 --------------------

 S.P.T.              J-12       J-13
 ------              ----       ----
 34                  ON         OFF
 35                  OFF        OFF
 36                  OFF        ON

 TERMINATORS
 -----------
 RP-701, RP-702.


