
9 0 2 5 6 D 2     D I A M O N D   M A X    MAXTOR
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 4960|     |
Capacity form/unform  2560/      MB        Heads           2|   16|     |
Seek time   / track   9.0/ 1.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA4 ULTRA      Precompensation
Cache/Buffer           256 KB SDRAM        Landing Zone
Data transfer rate   15.200 MB/S int       Bytes/Sector      512
                     33.000 MB/S ext
Recording method     PRML                           operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 71
Power: sleep          0.8 W     Humidity     %         5 95    |      5 95
       standby        1.3 W     Altitude    km    -0.061  3.048| -0.061 12.192
       idle           4.1 W     Shock        g        20       |    200
       seek           9.0 W     Rotation   RPM      5400
       read/write     4.3 W     Acoustic   dBA        36
       spin-up       20.2 W     ECC        Bit   SMART
                                MTBF         h     500000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates     EPA GREEN PC                 

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   DIAMOND MAX  INSTALLATION SHEET

 Jumper Setting
 ==============

                                        +---+---+---+---+---+
                                        |J50|J48|J46|J44|J42|
  +-------------------------------------+---+---+---+---+---+
  | Master/Slave                        |   |   |   |   |   |
  |  Only Drive in single drive system* | J |   |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  |  Master in a dual drive system*     | J |   |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  |  Slave in a dual drive system       | O |   |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  | Cable Select                        |   |   |   |   |   |
  |  Disabled*                          |   | O |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  |  Enabled                            |   | J |   |   |   |
  +-------------------------------------+---+---+---+---+---+
    J=Jumpered O=Open *=Default



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
-ANY DIREC.

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
MAXTOR    IDE INSTALLATION

            INSTALLATION PROCEDURE FOR AN IDE DRIVE
            ---------------------------------------
 1. Install a 40 pin Data Cable ensuring that pin 1, which can be
    identified by the striped edge of the cable, is closest to the
    power connector on the drive.

 2. Install a DC power cable to the back of the drive.

 3. Verify the jumper configurations for Master/Slave operation
    (Note:  Master will be the bootable drive. The slave will not
    be bootable.) Also make sure the existing C: drive is jumped
    to be the Master in a two drive system, not the only drive in
    the system.

 4. Apply power to the computer.

 4a. When memory test is complete go into your system's Standard
     CMOS set-up.
     (Note: There are various ways to get into CMOS set-up, please
     refer to system's manual for instructions.)

 4b. If your system's BIOS supports a user programmable drive
     type, program the BIOS with the default parameters of your
     drive. If your system does not support a user programmable
     drive type choose parameters that closely match but do not
     exceed the drives MegaByte capacity. Escape from set-up
     then choose write to CMOS and exit.

 5. Boot from a DOS diskette that has FDISK.EXE and FORMAT.COM on
    it. At the A> prompt type in FDISK. At the menu options select
    option 1 to create a DOS partition. Another menu will appear
    and from those options choose 1 to create a Primary DOS
    partition. Select yes to make 1 large partition and it will
    automatically become active. Then escape from FDISK.

 6. At the A> prompt type in FORMAT C:/S This does a high-level
    format on the drive and transfers the system files in order for
    the drive to be bootable. (Note: IDE drives are low-level
    formatted from the manufacturer and only need a high-level
    format).

    To configure the drive as a slave drive repeat steps 1-4 and
    proceed with steps 5a. and 6a. as follows:

  5a. At the C> prompt type in FDISK. When the menu options appear
      select option 5 to switch to the second drive. Enter fixed
      disk drive number 2. Then choose option 1 to create a DOS
      partition, then select option 1 again to create a Primary DOS
      partition or option 2 to create an Extended DOS partition.
      (Note: C and D drives will always be the Primary partitions
      but only the Primary partition on C: will have a status of
      active).

  6a. Proceed with a high-level format on the drive by typing FORMAT
      D: (Note: Make sure the correct drive letter has been selected
      for format).

 7. The drive is now bootable. As a test remove the DOS diskette
    from A and press reset to reboot the computer,  a  C> should be
    displayed, the drive is now ready for operation.


