
N P 0 4 - 1 3 T    NEC
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders        |     |     |
Capacity form/unform    10/   13 MB        Heads            |     |     |
Seek time   / track  85.0/ 5.0 ms          Sector/track   17|     |     |
Controller           MFM / ST506           Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate    0.625 MB/S int       Bytes/Sector      512
                      0.625 MB/S ext
Recording method     MFM                            operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     NO           Certificates


**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


