
M K - 1 3 0 1 M A V    TOSHIBA
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders    3650|     |     |
Capacity form/unform  1350/      MB        Heads           6|     |     |
Seek time   / track  13.0/ 3.0 ms          Sector/track     |     |     |
Controller           IDE / ATA3 EMBEDDED   Precompensation
Cache/Buffer           128 KB READ-AHEAD   Landing Zone
Data transfer rate    6.800 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method     RLL 8/9                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -20 60
Power: sleep          0.2 W     Humidity     %                 |
       standby        0.3 W     Altitude    km    -0.300  3.000| -0.400 15.000
       idle           0.9 W     Shock        g       100       |    200
       seek           2.7 W     Rotation   RPM      4200
       read/write     2.8 W     Acoustic   dBA        36
       spin-up        3.5 W     ECC        Bit   168BIT
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,IEC801-4,TUV,UL1950


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
TOSHIBA  MK1301MAV  PRODUCT SPECIFICATION 71Y102941 JUNE 1996



                                                    +-J2 MASTER/SLAVE
      43--------------------------------------------+1+-+
      |* * * * * * * * * * * * * * * * * * * * * * *|*|*|
   ---+* * * * * * * * * * * *   * * * * * * * * * *|*|*+-----
      44-----------------------+--------------------+2+-J1 RESERVED
                               |                    +-+
                        Polarity Key












**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TOSHIBA  MK1301MAV  PRODUCT SPECIFICATION 71Y102941  JUNE 96

 Jumper Setting
 ==============

 Master/Slave Configuration
 --------------------------
 By using the CSEL pin (PIN 28) and the optional jumper J2 beside the
 interface connector, two units can be connected on a cable in a daisy
 chain.

 When J2 is open, the drive runs as master drive and CSEL does not
 affect the definition. When J2 is closed, CSEL affects the
 definition. If CSEL is negated then the drive runs as master drive.
 If CSEL is asserted the the drive runs as slave drive.

 In case of two drive connection, one should be a master and another
 should be a slave. In case of single drive connection, it should be
 defined as master.

 Both master and slave drive are allocated onto same I/O area and
 identified by Drive bit in DRVH register. Host system writes into
 register on both drives but reads register only from a selected
 drive.

 Only the selected drive can execute the command except Diagnose
 command. Diagnose is executed on both drives and the result of slave
 drive is transferred to master drive through PDIAG line. Master
 drive reports both results to host system.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
TOSHIBA  MK1301MAV  PRODUCT DESCRIPTION  71Y102941  JUNE 96

 Notes On Installation
 =====================

 Installation
 ------------
 The drive should be mounted carefully on the surface of 0.1 mm
 flatness or less to avoid excessive distortion. It is recommended
 the space greater than 1 mm is kept under the PCB and it is important
 to check enough for safe design to prevent short- circuit under any
 circumstances. Enough room to avoid any mechanical interference
 when receiving shock or vibration is required especially around the
 convex portion in the HDA. The temperature of the top cover and the
 base must be kept under 60*C at any moment to maintain the desired
 reliability. (When the drive is running frequently, the temperature
 of the top cover may be rising by 15*C maximum. If the drive is used
 in 45*C or more ambient temperature, it is advisable to maintain
 adequate ventilation to keep top cover under 60*C.)

 The M3 mounting screw holes are tapped directly on the aluminium
 portion of HDA for electrical ground. The other are tapped on the
 plastic portion for electrical insulation. Screw holes for mounting
 can be determined by the evaluation results of the electromagnetic
 noise emitted from the host system to drive. The breathing hole
 should be kept open after mounting. A maximum force of 2N should be
 allowed on the top cover to avoid the drive damage.

 The drive is using several parts which can be easily damaged by ESD
 (Electric Static Discharge), so do not touch the interface
 connector pins and the surface of PCB.


 Screwing
 --------
 Four screws should be tightened equally with 0.3N.m (3 kgf.cm)
 torque. The depth should be 3.0 mm min. 3.5mm maximum.


 Cable Connection
 ----------------
 +------------------------+---------------------------------------+
 |Interface Connector     |                                       |
 |Drive side connector    |   Yamainchi GAP050K11617              |
 +------------------------+---------------------------------------+
 |Recommended host        |                                       |
 |side connector          |                                       |
 |for board               |  right angle type: Berg 88333-044     |
 |                        |  straight type:    AMP 8-176135-2     |
 |    --------------------+---------------------------------------+
 |for cable               |  Berg 89361-044                       |
 |                        |  AMP 1-111-624-0                      |
 +------------------------+---------------------------------------+


 Cable
 Twisted pair type cable is recommended as follows:
 Standard diameter           0.32mm (28 AWG)
 Characteristic impedance    100-132

 Cable length and capacitance
 0.46 MAX. 35pF MAX.


 Grounding
 ---------
 HDA (Head Disk Assembly) and DC ground (ground pins on interface)
 are electrically connected each other.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
TOSHIBA  MK-1301MAV  PRODUCT SPECIFICATION 71Y102941  JUNE 96

 General Description
 -------------------
 The MK1301MAV comprises a series of intelligent disk drives,
 hereinafter referred to as the MK1301MAV or simply as the drive.

 The drive features an ATA-2/ATA-3 interface embedded controller that
 requires a simplified adapter board for interfacing to an AT or AT
 compatible bus. The drives employ Winchester technology and a cloosed
 loop servo control system to realize recording density of 1.35 Mbit/
 mm  (874 Mbit/inch ) and average access time of 13 msec with highest
 reliability of 300,000 hours for MTTF (Mean Time to Failuree).

 It features smallest and lightest drive with 12.7mm height half foot-
 print of market standard 3.5" type micro FDD and 150 grams of weight.

 The MK1301MAV consists of an HDA (Head Disk Assembly) and a printed
 circuit board. The HDA is a sealed module and contains a disk
 spindle assembly, a head actuator assembly and an air filtration
 system. Reliability is enhanced through the use of Winchester
 technology. The actuator is a rotary voice coil motor and provides
 high-speed access.

 The disk is driven directly by a DC spindle motor. Air filtration is
 provided by means of a high performance air filtration system using
 both breather and circulation filters.

 The drive provides a carriage lock mechanism which is activated
 automatically upon power down, thus preventing head/media damage
 during non-operating or transportation conditions.

 The printed circuit board is located externally to the HDA and
 contains all the electric circuitry necessary to operate the drive
 except the head drivers. This board contains the power supply and
 interface signal connectors. Only the head control IC's are located
 within the HDA. The circuitry perform the following functions:

 Read/Write, Task File Control, Spindle Motor Control, Seek and Head
 Positioning Servo Control, Abnormal Condition Detection and Shock
 Sensor Control.


