
S T 3 2 4 3 A    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 1024|     |
Capacity form/unform   214/      MB        Heads           4|   12|     |
Seek time   / track  16.0/ 5.0 ms          Sector/track     |   34|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            32 KB SEGMENTED    Landing Zone
Data transfer rate    2.800 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 70
Power: sleep              W     Humidity     %                 |
       standby        1.3 W     Altitude    km                 |
       idle           2.5 W     Shock        g        10       |     75
       seek           4.6 W     Rotation   RPM      3811
       read/write     4.1 W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     250000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates



**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST3290 FAMILY  INSTALLATION GUIDE 36237-002, REV. A 6/1993

  +---------------------------------------------------------+
  |                                               +----+J5  |XX J1
  |  ++LED                                        +----1    |XX
  |  ++2-pin                                                |XX
  |                                                         |XX I
  |                                                         |XX N
  |                                                         |XX T
  |                                                         |XX E
  |                                                         |XX R
  |                                                         |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |X1 E
  |                                                         |
  |                                                         |XX J3
  |                                                         |XX Power
  +---------------------------------------------------------+  1




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST3290 FAMILY  INSTALLATION GUIDE 36237-002, REV. A, 6/1993

 Jumper Setting
 ==============


 J5 Master/Slave Jumper Block
 ----------------------------

      +8-6-4-2+
      |o o o o|   The drive is a master; there is no slave.
      |o o o o|
      +7-5-3-1+

      +8-6-4-2+
      |o o X o|   Master in a two drive system
      |o o X o|
      +7-5-3-1+

      +8-6-4-2+
      |o o o X|   The drive is a slave to a ATA compatible master.
      |o o o X|   NOTE: Do not configure the drive as a slave to a
      +7-5-3-1+   non-ATA-compatible master.

      +8-6-4-2+
      |o o    |   Pins 5 & 6, and 7 & 8 are factory reserved.
      |o o    |   Don't use them! (OPEN)
      +7-5-3-1+


 J3   DC Power and pin connector assignments
 -------------------------------------------
 -------------------+
 --+  +-----J3-----+|  pin 1    +12 VDC
  1|  | 4  3  2  1 ||  pin 2    +12 Volts Return
  -+  \------------/|  pin 3    + 5 Volts Return
  ------------------+  pin 4    + 5 VDC



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SEAGATE  ST3290 FAMILY  INSTALLATION GUIDE 36237-002, REV. A, 6/1993

 Notes on Installation
 =====================

 Mounting the drive
 ------------------
 Mount the drive securely in any orientation using either the bottom
 or side mounting holes.

 NOTE
 Make sure you mount the drive so that you do not strain the cables.


 Bottom mounting holes
 ---------------------
 Insert four 6-32 UNC-2A screws not more than 0.20 inches (6 turns)
 into the drive frame.


 Side mounting holes
 -------------------
 Insert four 6-32 UNC-2A screws not more than 0.13 inches (4 turns)
 into the drive frame.

 CAUTION
 If you use a screw that is too long, you cold damage the drive.


 Attaching cables
 ----------------
 1. Turn off the system power

 2. Put on a grounded wrist strap.

 3. Attach the 40-pin AT interface cable. Attach one end of the cable
    to the drive interface connector and the other end to the
    interface connector on the host adapter or the host system mother-
    board. If you are installing two drives, use a daisy-chain cable.

    Verify that pin 1 of the interface cable is matched to pin 1 of
    the interface connector on the drive and on the host computer. Pin
    1 is usually deenoted by a stripe on the side of the ribbon cable.

 4. Attach the power cable. Attach a system power cable to the drive
    power connector.


