
C F P - 4 2 0 7 S V   C A Y M A N   A V    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    4016|     |     |
Capacity form/unform  4294/      MB        Heads          20|     |     |
Seek time   / track   8.5/ 2.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST/AV      Precompensation
Cache/Buffer           512 KB              Landing Zone
Data transfer rate    6.700 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %         5 95    |      5 95
       standby            W     Altitude    km    -0.061  3.048|        12.192
       idle          12.8 W     Shock        g         5       |     50
       seek          14.3 W     Rotation   RPM      7200
       read/write    13.2 W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h    1000000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CFP-4207S  QUICK REFERENCE GUIDE REV. C, 12/1994

  +---------------------------------------------------------+
  |      +-J1                                            ++ |XX J2
  |      | |                                             || |XX
  |      | |                                             || |XX
  |      | |                                             || |XX I
  |      +-+                                             || |XX N
  |                                                      *+ |XX T
  |                                                    E8++ |XX E
  |                                                      ++ |XX R
  |                                             (Fuse)F1 xx |XX F
  |  J3                                                  ++ |XX A
  | +-+ SS                         ++++++++              || |XX C
  | | | LED                        ++++++++              || |XX E
  | | |                          E1 ****** E7            || |XX
  | +-+                          E4 RESERVED             || |
  |J6+0E1                                                *+ |xx
  || |                                                      |XX J4
  |+-+0E6                                                   |XX Power
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CFP-4207S  QUICK REFERENCE GUIDE 12/1994, REV. C

 Jumper Setting
 ==============


 Setting the SCSI Bus Address
 ----------------------------
 There are three jumpers available for configuration of the SCSI ID:
 E1, E2, and E3.

 OPTIONAL HEADER
      |     +-+
  0E1 | ----+ +-*  SCSI ID 1
  0E2 | ----+ +-*  SCSI ID 2
  0E3 | ----+ +-*  SCSI ID 4
  0E5 | ----+ +-*  Disable Spin
  0E6 | ----+ +-*  LED Driver
      |     +-J6
      |     PCB
      +---------------


 An optional 2mm pin pitch right angle header is located on the front
 of the PCBA (opposite the SCSI interface connector) which allows
 changing the SCSI IDs while the drive is mounted in the system. The
 header includes three pins, 0E1, 0E2 and 0E3 which can alternatively
 be used to select the SCSI Bus address. This connector may also be
 used to cable the SCSI ID select to a remote switch. A receptable
 connector AMP P/N 111622-1 or equivalent can be used to connect a
 ribbon cable to this header.

   +----------+-----------------------+
   | SCSI ID  | 0E3     0E2     0E1   |
   |          | E3    | E2    | E1    |
   +----------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    2     | OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    3     | OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+
   |    4     | CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    5     | CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    6     | CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+

 NOTE
 When controlling the SCSI ID remotely, IN (CLOSED) = Ground or TTL
 Low and OUT (OPEN) = Open or TTL High.


 Disabling Spin-Up at Power On
 -----------------------------
 A jumper in the E5 location, disables spin up after power-on for
 applications where spin up sequencing is necessary. An optional 2mm
 pin pitch right angle header is located on the front of the PCBA
 (opposite the SCSI interface connector) which can alternatively be
 used to disable spin up. Disabling spin up on application of power
 can also be enabled by setting the DSPN bit in MODE SELECT page 00H
 (Operating Parameters). The Host must issue a Start UNIT command to
 cause the drive to spin up.

   +---------+------+---------------------+
   |E5 or 0E5| DSPN | Result              |
   +---------+------+---------------------+
   |   IN    |  0   | Spin Disabled       |
   +---------+------+---------------------+
   |   IN    |  1   | Spin Disabled       |
   +---------+------+---------------------+
   |   OUT   |  0   | Spin up on Power On |
   +---------+------+---------------------+
   |   OUT   |  1   | Spin Disabled       |
   +---------+------+---------------------+
 NOTE
 IN = Ground or TTL Low and OUT = Open or TTL High.


 Delaying Spin Up at Power On
 ----------------------------
 A jumper in the E6 location, delays spin up on power-up by the value
 of the drive's SCSI ID multiplied by 4 seconds (i.e. SCSI ID 4 will
 delay 16 seconds). Delaying spin up on application of power can also
 be enabled by setting the SDLY bit in MODE SELECT page 00H (Operating
 Parameters.)

   +---------+------+---------------------+
   |   E6    | SDLY | Result              |
   +---------+------+---------------------+
   |   IN    |  0   | Spin Delayed        |
   +---------+------+---------------------+
   |   IN    |  1   | Spin Delayed        |
   +---------+------+---------------------+
   |   OUT   |  0   | Spin up on Power On |
   +---------+------+---------------------+
   |   OUT   |  1   | Spin Delayed        |
   +---------+------+---------------------+


 Disabling the SCSI Bus Parity
 -----------------------------
 SCSI parity is always enabled in both directions, unless the E7
 Parity disable jumper is installed. Installing the jumper will cause
 the drive to ignore SCSI bus Parity In but it will continue to
 generate SCSI bus Parity Out.


 Disabling SCSI Bus Terminator Power (TERMPWR)
 ---------------------------------------------
 Power to the on-board terminators is provided by the higher of the
 voltage supplied at Pin #26, J2 or the voltage level at the 5 Volt
 power input to the drive minus one diode drop. Termination Power to
 external terminators can be supplied by the drive through Pin #26,
 J2. The TERMPWR line can be disconnected from the drive by removing
 Jumper E8.


 Jumper E8   Result
   IN        TERMPWR (J2, Pin #26) connected to the drive's internal
             termination power.

   OUT       TERMPWR (J2, Pin #26) open circuit.


 Setting the Bus Termination
 ---------------------------
 This drive provides on-board Alternative 2 active termination for the
 SCSI bus. The termination resistors, which are contained in two
 Single Inline Packs (SIPs) should be removed from the drive unless it
 is a SCSI device at the physical end of the bus.

 NOTE
 The TERMPWR output of the drive is protected by a 1 Ampere fuse (F1).
 If external terminators are being powered from the drive and SCSI bus
 problems are suspected, verify that the fuse is still operational
 using a meter.


