
D E S K S T A R 5   3 4 3 3 0    IBM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 8400| 8400|
Capacity form/unform  4330/      MB        Heads           5|   16|   15|
Seek time   / track      /     ms          Sector/track     |   63|   63|
Controller           IDE / ATA3            Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                     33.300 MB/S ext DMA
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 65
Power: sleep              W     Humidity     %         8 90    |      5 95
       standby            W     Altitude    km    -0.300  3.048| -0.300 12.000
       idle               W     Shock        g        10       |     75
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   ON THE FLY,SMART
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
IBM      DESKSTAR 5  JUMPER SETTING


   +---------------------------------------------------------------+
   |                                                               |
   |                                                               |
   | +--------------------------------------1---G-----A-+------1-+ |
   | |* * * * * * * * * * * * * * * * * * * * * * * * * |X X X X | |
   | |* * * * * * * * *   * * * * * * * * * *+-+* * * * |X X X X | |
   +-+------AT-INTERFACE---------------------+ +-JUMPER-+-POWER--+-+













**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
IBM      DESKSTAR 5  JUMPER SETTING

 Jumper Setting
 ==============
 Interface Connector  3M 3417-7000 or equivalent


  16 Logical Head              15 Logical Head
  ---------------              ---------------
  G E C A                      G E C A
  X * * X      Device 0        X * xxx
  X * * X      (Master)        X * * *
  H F D B                      H F D B


  G E C A                      G E C A
  * * X X       Device 1       * * xxx
  * * X X       (Slave)        * * * *
  H F D B                      H F D B


  G E C A                      G E C A
  * X * X      Cable Select    * X xxx
  * X * X                      * X * *
  H F D B                      H F D B


  G E C A                      G E C A
  X * * X      Device 1        X X * *
  X * * X      (Slave)         X X * *
  H F D B      Present         H F D B

 All other jumper setting patterns are reserved. Do not make other
 settings.

 Shipping default settings:
 16 head logical architecture is enabled. Master is set to on (i.e.
 jumper on pins A-B and G-H. No other jumpers are fitted.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
IBM      DESKSTAR 5  NOTES ON INSTALLATION

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).

 Mount the drive securely, using the appropriate brackets or rails, in
 any axis, using four 6-32 UNC metric screws in either bottom or side
 mounting holes.

 The max. screw insertion depth for the bottom mounting is 5.5mm
 (0.21 inch) and for side mounting 3.5 mm (0.14 inch).


