
M K - 7 2 P C    TOSHIBA
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders     830|     |     |
Capacity form/unform    72/      MB        Heads          10|     |     |
Seek time   / track  25.0/     ms          Sector/track   17|     |     |
Controller           MFM / ST506           Precompensation   512
Cache/Buffer               KB              Landing Zone      830
Data transfer rate    0.625 MB/S int       Bytes/Sector      512
                      0.625 MB/S ext
Recording method     MFM                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TOSHIBA  MK72PCX  PRODUCT DESCRIPTION




   Underside View
                        Terminator
              TP------++   |   +---Write Protect
              Model-++||   |   |+--Radial
                    ||||   |   ||+------Drive Select 4
              CHK-+ ||||   |   |||+-----Drive Select 3
              RWC+| ||||+++++++||||+----Drive Select 2
                 ** oooo*******ooooo*---Drive Select 1
                 ** oooo*******ooooo*
   --+------+--+  ++                   +----+  ++           +----
     +------+  |  ||                   |    |  ||           |
     PJ6       +--++-------------------+    +--++-----------+
     Power          Control Connector         Data Connector

    *             o
    * = Jumpered, o = Open


