
M 1 6 3 6 T A U     P I C O B I R D   9    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    6189| 2490|     |
Capacity form/unform  1284/      MB        Heads           2|   16|     |
Seek time   / track  11.0/ 3.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           128 KB FIFO BUFFER  Landing Zone
Data transfer rate    7.700 MB/S int       Bytes/Sector      512
                     16.700 MB/S ext PIO4
Recording method     PRML 8/9                       operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep          1.1 W     Humidity     %         8 80    |      5 95
       standby            W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle               W     Shock        g         5       |     75
       seek               W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA        35
       spin-up            W     ECC        Bit   SMART
                                MTBF         h     500000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  M163X/162XTAU  JUMPER SETTING








                        Jumper
               +Power-----2-6----------------------+
               |xxxxxxxx  ooo ooooooooo oooooooooo |
               |XXXXXXXX  ooo oooooooooooooooooooo |
               |1         1 5                      |
               +---------------Interface-----------+








**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  M163X/162XTAU  JUMPER SETTING

 Jumper Setting
 ==============


   2   6
   X o o
   X o o  MASTER (default)
   1   5


   2   6
   o X o
   o X o  SLAVE
   1   5


   2   6
   xxx o
   o o o  CABLE SELECT  Cable Select Mode gives an alternative method
   1   5                by which the drive may be set to MASTER or
                        SLAVE. A special cable is needed to implement
                        this feature and ahould only be used by BOTH
                        drives.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
FUJITSU  M163X/162XTAU  JUMPER SETTING

 Notes On Installation
 =====================

 Grounding
 ---------
 Sufficient grounding will be provided for correct operation when
 the drive is screwed into an electrically grounded frame.


 Orientation
 -----------
 The drive may be installed in one of three orientations; PCA down
 or on either edge.



     horizontally             vertically
   +-----------------+   +--+             +--+ +------------------+
   |                 |   |  +-----+ +-----+  | |                  | x
   |                 |   |  |     | |     |  | x+----------------+x
 +-+-----------------+-+ |  |     | |     |  | ||x              x||
 +---------------------+ |  |     | |     |  | ||  x          x  ||
                         |  |     | |     |  | ||    x      x    ||
      x           x      |  |     | |     |  | ||      x  x      ||
 +------x------x-------+ |  +-----+ +-----+  | ||       xx       ||
 +-+------x--x-------+-+ +--+             +--+ ||     x    x     ||
   |       xx        |                         ||   x        x   ||
   |     x    x      |                         || x            x ||
   +---x--------x----+                         |x                x|
     x            x                           x++----------------++x
      UNACCEPTABLE!                                UNACCEPTABLE!
      Never install PC board on the Top!


 Cooling
 -------
 Allow space above and below the drive to provide for adequate air
 flow. Fan cooling is recommended. The disk enclosure temperature,
 measured at top center, should never exceed 60*C.


 Mounting screw fixing
 ---------------------
 When the mounting screw holes on the side of the drive are used, then
 use only the two pairs of outer holes. Do not use the center hole in
 conjunction with only one of the outer holes. The screw must not
 penetrate the drive.
 Screws: 6-32UNC


