
Q M   3 1 7 0 0 S         S I R O C C O    QUANTUM
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform  1700/      MB        Heads           4|     |     |
Seek time   / track  11.0/ 2.5 ms          Sector/track     |     |     |
Controller           SCSI3 SI/FA           Precompensation
Cache/Buffer           128 KB ADAP./SEGMEN Landing Zone
Data transfer rate    5.500 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     PRML 16/17                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 65
Power: sleep              W     Humidity     %         5 85    |      5 95
       standby        0.8 W     Altitude    km            2.137|        12.192
       idle           4.2 W     Shock        g        10       |     70
       seek           6.5 W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA        33
       spin-up            W     ECC        Bit   160BIT REED SOLO.,ON THE FLY
                                MTBF         h     400000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


