
8 3 8 4 0 A 6     D I A M O N D   M A X    MAXTOR
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform  3840/      MB        Heads           6|     |     |
Seek time   / track  10.0/ 1.0 ms          Sector/track     |     |     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate    8.000 MB/S int       Bytes/Sector      512
                     16.700 MB/S ext PIO4
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle           4.3 W     Shock        g                 |
       seek               W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA
       spin-up       14.4 W     ECC        Bit
                                MTBF         h     500000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MAXTOR   85120A/83840A/82560A/81280A DIAMOND  JUMPER SETTING



     J1 IDE Connector                   J2 Power
  +----------- --------1-++-----------+
  | .................... || * * *   * |/---------\
  | .......... ......... || * * * * * || O O O O |
  +----------------------++-----------++---------+
                            | | | | |    | | | |
                            | | | | |    | | | |
        J50 Master/Slave ---+ | | | |    | | | +-+12V        (Yellow)
        J48 Cable Select -----+ | | |    | | +---+12V Return (Black)
        J46 4092 Cyl Limitation-+ | |    | +----- +5V Return (Black)
        J44 Factory Reserved -----+ |    +------- +5V        (Red)
        J42 Factory Reserved -------+







**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MAXTOR   85120A/83840A/82560A/81280A  DIAMOND  JUMPER SETTING

 Jumper Setting
 ==============


                                        +---+---+---+---+---+
                                        |J50|J48|J46|J44|J42|
  +-------------------------------------+---+---+---+---+---+
  | Master/Slave                        |   |   |   |   |   |
  |  Only Drive in single drive system* | J |   |   |   |   |
  |  Master in a dual drive system*     | J |   |   |   |   |
  |  Slave in a dual drive system       | O |   |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  | Cable Select                        |   |   |   |   |   |
  |  Disabled*                          |   | O |   |   |   |
  |  Enabled                            |   | J |   |   |   |
  +-------------------------------------+---+---+---+---+---+
  | 4092 Cylinder Option                |   |   |   |   |   |
  |  Disabled*                          |   |   | O |   |   |
  |  Enabled                            |   |   | J |   |   |
  +-------------------------------------+---+---+---+---+---+
  | Factory Reserved                    |   |   |   | O |   |
  +-------------------------------------+---+---+---+---+---+
  | Factory Reserved                    |   |   |   |   | O |
  +-------------------------------------+---+---+---+---+---+
    J=Jumpered O=Open *=Default



 Systems Using Cable Select
 --------------------------
 Most systems do not use this feature. Unless you are sure that the
 system that the Maxtor hard drive is being installed in uses Cables
 Select, do not set up the drive with this feature enabled.

 Maxtor hard drives support Cable Select - which allows the system
 to identify Devuce 0 and Device 1 drives on the interface cable. If
 your system manufacturer for specific procedures for installing hard
 drives.

 On Maxtor DiamondMax hard drives, the Cable Select is enabled by
 installing a jumper on J48. When J48 is installed, remove the jumper
 from J50.


