
F I R E B A L L   S E   4 3 0 0 S    QUANTUM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders   14848|     |     |
Capacity form/unform  4300/      MB        Heads           9|     |     |
Seek time   / track   9.5/     ms          Sector/track   63|     |     |
Controller           SCSI3 SI/ULTRA        Precompensation
Cache/Buffer           512 KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     EPRML                          operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit   224BIT,SMART
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
-ANY DIREC.

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).


