
M 2 2 6 2 E    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders    1658|     |     |
Capacity form/unform   448/  570 MB        Heads          11|     |     |
Seek time   / track  16.0/ 4.0 ms          Sector/track   53|     |     |
Controller           ESDI                  Precompensation 65535
Cache/Buffer               KB              Landing Zone
Data transfer rate    1.875 MB/S int       Bytes/Sector      512
                      5.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 45    |    -40 60
Power: sleep              W     Humidity     %        20 80    |      5 95
       standby            W     Altitude    km            3.000|        12.000
       idle               W     Shock        g         2       |     20
       seek               W     Rotation   RPM      3600
       read/write    28.0 W     Acoustic   dBA
       spin-up            W     ECC        Bit   -
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  M2261E/M2262E/M2263E  OEM MANUAL 41FH5031E-02

  +---------------------------------------------------------+
  |                           16+----+2                     |XX 20 Pin
  |                           15+CNH7+1                     |XX
  | +---+CN4                  16+----+2                     |XX
  | +---+CN5                  15+CNH6+1  15+-+16            |XX
  | +---+CN6                               | |   +--------+ |
  | +---+                                CNH5|   +Terminat+ |XX 34 Pin
  |                                       1+-+2             |XX
  |                                      15+-+16            |XX
  |                                      CNH2|              |XX
  |                                        | |              |XX
  |                            16+----+2  1+-+2             |XX
  |     16+----+2              15+CNH1+1                    |XX
  |     15+CNH3+1                                      1+-+2|XX
  |                                                   CN7 | |
  |                                                     | | |
  |              16+----+2   3210                      5+-+6|XX Power
  |              15+CNH4+1   **** Fault Lamp                |XX
  +---------------------------------------------------------+


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  M2261E/M2262E/M2263E  OEM MANUAL 41FH5031E-02

 Fault Lamps and Setting Plugs
 =============================
 Selectable by user side: Terminator
                          CNH5, CNH6, CNH7
 Fixed at factory:        CN4, CN5, CN6, CN7
                          CNH1, CNH2, CNH3, CNH4


 Jumper Settings
 ===============
 x = Jumpers are set from factory


 CNH3  Offtrack Compensation
 ---------------------------
       15-16 OPEN    Enable
             CLOSE   Disable


 CNH5  READY LED lighting conditions
 -----------------------------------
 x     15-16 OPEN    Drive select signal not gated
             CLOSE   Drive select signal gated


 CNH6  Drive select
 ------------------
        Drive    1         2     3     4         5         6     7
        ------+-----+-----+-----+-----+-----+-----+-----
 x      1- 2  |CLOSE|OPEN |OPEN |OPEN |OPEN |OPEN |OPEN
        3- 4  |OPEN |CLOSE|OPEN |OPEN |OPEN |OPEN |OPEN
        5- 6  |OPEN |OPEN |CLOSE|OPEN |OPEN |OPEN |OPEN
        7- 8  |OPEN |OPEN |OPEN |CLOSE|OPEN |OPEN |OPEN
        9-10  |OPEN |OPEN |OPEN |OPEN |CLOSE|OPEN |OPEN
       11-12  |OPEN |OPEN |OPEN |OPEN |OPEN |CLOSE|OPEN
       13-14  |OPEN |OPEN |OPEN |OPEN |OPEN |OPEN |CLOSE

 CNH6  Signal gate or not (Select signal)
 ----------------------------------------
 x     15-16  OPEN   Gate (daisy)
              CLOSE      No gate (radial)

       When the pins are shorted, the drive output signals are always
       enabled, regardless of Drive Select signal. Without a jumper
       here, the output signals are enabled only when the drive is
       selected.


 CNH7  Motor start control from interface
 ----------------------------------------
        1- 2  OPEN       Yes
 x            CLOSE  No

 CNH7  Device Type selection (model specific)
 --------------------------------------------
        Device M2261 M2262 M2263
        ------+-----+-----+-----
        3- 4  |OPEN |OPEN |CLOSE
        5- 6  |OPEN |CLOSE|OPEN

 CNH7  Sector setting
 --------------------
        Sectors/Track   24        27    28        48    51        53    54        96
        Bytes/Sector |1304 |1159 |1117 | 652 | 613 | 590 | 579 | 362
        -------------+-----+-----+-----+-----+-----+-----+-----+-----
 x      7- 8         |OPEN |OPEN |OPEN |OPEN |CLOSE|CLOSE|CLOSE|CLOSE
 x      9-10         |OPEN |OPEN |CLOSE|CLOSE|OPEN |OPEN |CLOSE|CLOSE
 x     11-12         |OPEN |CLOSE|OPEN |CLOSE|OPEN |CLOSE|OPEN |CLOSE

       Valid only in hard sector mode

 CNH7  Sector mode setting
 -------------------------
       13- 14 OPEN       Drive hard sector
              CLOSE  Controller soft sector

 CNH7  Power ON Reset Condition
 ------------------------------
 x     15- 16 OPEN       ATTENTION signal and bit 8 of Status byte are
                     set at the READY state just after power-on.
              CLOSE  ATTENTION signal and bit 8 of Status byte are
                     not set at the READY state just after power-on.


 Fault lamps
 ===========
        Drive fault states are displayed by the fault lamps (0,1,2,3)

        Fault lamp| Drive State
         3 2 1 0  |
        ----------+--------------------------------------------------
         x x x o  |     Spindle motor rotation less than 90% of standard
         x x o x  | VCM over current
         x x o o  | Initial seek time out
         x o x x  | Write command during seek operation
         x o x o  | +12V/+5V less than 80% of standard
         x o o x  |     Off track during Write operation
         x o o o  |     Write Echo check
         o x x x  | Two or more head ICs selected during
                  |  operation
         o x x o  | Seek time out
         o x o x  | Guard band detection during Seek operation
         o x o o  | Guard band detection during linear mode
         o o x x  | Overshoot check
         o o x o  | Seek command without ONTRACK signal true
         o o o x  | Head load signal lost after READY
         o o o o  |     Read and Write commands simultaneously issued or
                  | other miscellaneous faults
         x x x *  | Invalid or unimplemented command fault
         x x * x  | Interface time out fault
         x x * *  | Command data parity fault
         x * x x  | Spindle sync error

         o = On    x = Off    * = Blinking


**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
FUJITSU  M2261E/M2262E/M2263E  OEM MANUAL 41FH5031E-02

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
      x           x                |  |     |           |     |  |
 +------x------x-------+           |  +-----+           +-----+  |
 +-+------x--x-------+-+           +--+                       +--+
   |       xx        |
   |     x    x      |
   +---x--------x----+
     x            x


 There are three possible installation directions, and the mounting
 angle must be   5* from the horizontal.

 Ambient temperature
 -------------------
 The operating temperature range of the drive is specified at a dis-
 tance of 3 cm from the drive. Note, temperature specifications are
 for the outside air surrounding the drive.

 Multi-drive connection
 ----------------------
 In serial mode, up to 7 drives can be connected. The termination of
 the control signals must be performed only at the last drive. The
 terminator must be removed from all but the last drive.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
FUJITSU  M2261E/2262E/2263E  OEM MANUAL 41FH5031E-02

 Defect list
 ===========
 When the unit leaves the factory, a printed media defect list for
 each drive is sent with it. This information is also written on the
 media.
 Cylinder 0, Head 0 and 1 are defect free!

