
S D - 3 2 1 0 - 3 0    TEAC
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    1695| 1024|     |
Capacity form/unform   215/      MB        Heads           4|    8|     |
Seek time   / track  17.0/ 7.0 ms          Sector/track   62|   57|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            64 KB LOOK-AHEAD   Landing Zone
Data transfer rate    2.500 MB/S int       Bytes/Sector      512
                      4.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 60
Power: sleep          0.1 W     Humidity     %         8 80    |      8 80
       standby        0.5 W     Altitude    km                 |
       idle           3.2 W     Shock        g         5       |     70
       seek           5.1 W     Rotation   RPM      3600
       read/write     3.4 W     Acoustic   dBA        45
       spin-up            W     ECC        Bit
                                MTBF         h     100000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,TUV,UL478



**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
TEAC     SD-3210-30  HARD DISK DRIVE SPECIFICATION 10530648-00 REV. B

  +---------------------------------------------------------++-+Strap
  |                                                         || |SP
  |                                                         |+-+S0 3
  |                                                         |1X
  |                                                         |XX Inter-
  |                                                         |XX face
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |++LED                                                    |XX
  |++                                                       |XX
  |                                                         |XX
  |                                                         |xx
  |                                                         |XX Power
  |                                                         |
  |                                                         |XX Power
  |                                                         |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TEAC     SD-3210-30  HARD DISK DRIVE SPECIFICATION 10530648-00 REV. B

 Jumper Setting
 ==============

 Indicator LED
 -------------
 The indicator (LED) on the front bezel lights up while the HDD
 executes a command. An external LED can also be lighted through the
 -SLV/ACT signal terminal on the same condition by setting the strap
 SP to ON.


 Straps
 ------
 The setting method for the straps, S2 and S3, should be changed
 according to the number of the HDDs connected as shown in the
 following table.

 Functions of straps
  +----------+-------------------------------------------------------+
  | Strap No.| Function                                              |
  +----------+-------------------------------------------------------+
  | SP       | Changes over the function of the -SLV/ACT output      |
  |          | signal.                                               |
  |          | ON  : The -ACTIVE signal is selected. The external LED|
  |          |       can be lighted up at the -SLV/ACT signal        |
  |          |       terminal.                                       |
  |          | OFF : The -SLAVE PRESENT signal is selected.          |
  +----------+-------------------------------------------------------+
  | S0       | (Not used)                                            |
  +----------+-------------------------------------------------------+
  | S1       | Changes over the -I/O CH RDY output signal.           |
  |          | OFF : The -I/O CH RDY signal is not output.           |
  |          | ON  : The -I/O CH RDY signal is output.               |
  +----------+-------------------------------------------------------+
  | S2       | Selects the master drive or slave drive.              |
  |          | OFF : Only one unit used, or master drive with two    |
  |          |       units used.                                     |
  |          | ON  : Slave drive with two units used.                |
  +----------+-------------------------------------------------------+
  | S3       | Selects whether one HDD is used singly, or two HDDs   |
  |          | are used in daisy chain connection.                   |
  |          | ON  : Two HDDs are used.                              |
  |          | OFF : Only one HDD is used.                           |
  +----------+-------------------------------------------------------+
 Notes: 1. ON  : Strap short
           OFF : Strap open

        2. At the shipping of the HDD, the strap SP is set to ON, S0
           to OFF, S1 to OFF, S2 to OFF, S3 to OFF.


 How to set the straps, S2 and S3
 --------------------------------
  +-------------------------+--------------+-----+-----+
  |Number of HDDs connected | Master/Slave |  S2 | S3  |
  +-------------------------+--------------+-----+-----+
  |           1             |      -       | OFF | OFF |
  +-------------------------+--------------+-----+-----+
  |           2             |    Master    | OFF | ON  |
  |                         |    Slave     | ON  | ON  |
  +-------------------------+--------------+-----+-----+



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
TEAC     SD-3210-30  HARD DISK DRIVE SPECIFICATION 10530648-00 REV. B

 Notes on Installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 Any of the four directions can be used.
 The mounting cabinet for the HDD should be constructed so that no
 distortion may be produced in the chassis.
 A space of at least 1.5mm must be allowed between the mounting
 cabinet and the PCBA of the HDD.

 An insulation sheet should be stuck to the PCBA mounting face of the
 HDD mounting cabinet, as required.
 In each mounted position, the front can be raised by up to 30*.
 Mounting positions other than those shown must be discussed
 separately.


 Screws
 ------
 The HDD is fixed with screws through the mounting holes at the
 3-#6-32UNC 4 deep each side.
 4-#6-32UNC 4 deep bottom.


 Auto shipping lock function
 ---------------------------
 The auto shipping lock is designed to protect the media against the
 risk of damage due to vibration and shock during transport. When the
 power is turned off, the head carriage is locked automatically at the
 shipping zone, within the inside limit of the work zone, to protect
 your important stored data.


 Automatic self-diagnosis
 ------------------------
 When the power is switched on, the SD-3210 and SD-3240 automatically
 performs a selfcheck sequence, checking program ROM, buffer RAM, and
 interface register.


