
C F N - 3 4 0 S    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders    1598|     |     |
Capacity form/unform   344/      MB        Heads           6|     |     |
Seek time   / track  13.0/ 3.0 ms          Sector/track     |     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation
Cache/Buffer            32 KB              Landing Zone
Data transfer rate    3.000 MB/S int       Bytes/Sector      512
                      6.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 60
Power: sleep          0.2 W     Humidity     %         5 90    |      5 90
       standby        0.2 W     Altitude    km    -0.061  3.048| -0.061  4.500
       idle           0.9 W     Shock        g        10       |    200
       seek           1.1 W     Rotation   RPM      4000
       read/write     1.4 W     Acoustic   dBA        34
       spin-up            W     ECC        Bit
                                MTBF         h     150000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   QUICK INSTALLATION GUIDE L-511-1008 11/93 SCSI

 QUICK INSTALLATION GUIDE
 ========================
 SCSI

    Chart AA
         +----+----+----+-----+
         | ID |E-1 |E-3 | E-4 |
         +----+----+----+-----+
         | 0  |OUT |OUT |OUT  |
         +----+----+----+-----+
         | 1  |IN  |OUT |OUT  |
         +----+----+----+-----+
         | 2  |OUT |IN  |OUT  |
         +----+----+----+-----+
         | 3  |IN  |IN  |OUT  |
         +----+----+----+-----+
         | 4  |OUT |OUT |IN   |
         +----+----+----+-----+
         | 5  |IN  |OUT |IN   |
         +----+----+----+-----+
         | 6  |OUT |IN  |IN   |
         +----+----+----+-----+
         | 7  |IN  |IN  |IN   |
         +----+----+----+-----+


 Partity is always enabled with the following exceptions:

 CP3180:  Jumper E4 to disable
 CP3100:  Jumper E4 to disable
 CFP1060: Jumper E7 to disable


 LED Configuration Table
 -----------------------
 Letter  Connector  LED+   LED-
   A       J-4      Pin 1  Pin 2
   B       J-1      Pin 3  Pin 4
   C       J-5      Pin 3  Pin 4
   D       J-3      Pin 3  Pin 4
   E       J-7      Pin 1  Pin 2
   F       J-5      Pin 7  Pin 8


