
D K 5 1 1 - 8    HITACHI
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders     823|     |     |
Capacity form/unform    68/      MB        Heads          10|     |     |
Seek time   / track  23.0/     ms          Sector/track   17|     |     |
Controller           MFM / ST506           Precompensation   400
Cache/Buffer               KB              Landing Zone      822
Data transfer rate    0.625 MB/S int       Bytes/Sector      512
                      0.625 MB/S ext
Recording method     MFM                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     NO           Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
HITACHI  DK511  PRODUCT MANUAL K6600061 REV. 7 10/01/1985




  +---------------------------------------------------------+
 ++LED                    xxJP164  +-----+9      4--3       |XX
 ++               JP155            1-----8       |  |JP117  |XX
  |            16------9           JP123         6--1       |XX J2
  |            1+------+            PLO          Write Prot.|XX
  |             Velocity                                    |XX
  |             Gain                              6--5      |XX
  |                                      Write    |  |JP113 |
  |                                      Protect  |  |      |XX
  |  SZ073 PCB REV. 3                             +--1      |XX
  |  Component Side                              +--4       |XX J1
  |                            General  xxJP70   |  |JP68   |XX
  |                            Reset             8--1Drive  |XX
  |                                                  Select |XX
  |       +-------+                     +-------+Term.      |
  |       +  5A   |                     + IC    |           |xx
  |       +-------+                     +-------+           |XX
  |  (POSN-P) TP27Ax  xTP10A (GND)                          |XX J3
  +---------------------------------------------------------+












  +---------------------------------------------------------+
 ++LED                    xxJP164  +-----+9      4--3       |XX
 ++               JP155            1-----8       |  |JP117  |XX
  |            16------9           JP123         6--1       |XX J2
  |            1+------+                                    |XX
  |                                                         |XX
  |                                               6--5      |XX
  |                                               |  |JP113 |
  |                                               |  |      |XX
  |  SZ073 PCB REV. 4 or 5                        +--1      |XX
  |  Component Side                              +--4       |XX J1
  |                                   1xxx3      |  |JP68   |XX
  |                                    JP70      8--1       |XX
  |                                                         |XX
  |       +-------+                     +-------+Term.      |
  |       +  5A   |                     + IC    |           |xx
  |       +-------+                     +-------+           |XX
  |  (POSN-P) TP27Ax  xTP10A (GND)                          |XX J3
  +---------------------------------------------------------+






  +---------------------------------------------------------+
 ++LED xxx JP182A         xxJP164  +-----+9      4--3       |XX
 ++    1  3       JP155            1-----8       |  |JP117  |XX
  |            16------9           JP123         6--1       |XX J2
  |            1+------+                                    |XX
  |                                                         |XX
  |                                               6--5      |XX
  |                                               |  |JP113 |
  |                                               |  |      |XX
  |  SZ073 PCB REV. 6                             +--1      |XX
  |  Component Side                              +--4       |XX J1
  |                                   1xxx3      |  |JP68   |XX
  |                                      JP70    8--1       |XX
  |                                                         |XX
  |       +-------+                     +-------+Term.      |
  |       +  5A   |                     + IC    |           |xx
  |       +-------+                     +-------+           |XX
  |  (POSN-P) TP27Ax  xTP10A (GND)                          |XX J3
  +---------------------------------------------------------+








  +---------------------------------------------------------+
  |                                                     +--+|
  |                                                     |  ||
  |                                 Head Sel #7   3xxx1 |J7||
  |     SZ074 PCB                   Fault Jumper > JP4A |  ||
  |                                 Switch              +--+|
  |                                                    +---+|
  |                                                    |   ++---
  |                                   +----+           | J4||
  |                                   |    |           |   ++-----
  |                                   | J8 |           +---+|
  |                                   |    |             +-+|
  |                                   +----+           J5| ||
  |                                                      | ||
  |                                                      | ||
  |                                                      +-+|
  |                                                  J6+--+ |
  |                                                    +--+ |
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
HITACHI  DK511  PRODUCT MANUAL K6600061 REV. 7, 10/01/1985

 Jumper Setting
 ==============

 Adjustment
 ----------
 There are two types of jumper switches for DK511 as follows:

 CAUTION
 1. Jumper Switches with GREEN connectors: to be used for an assign-
    ment of unit address and for selection of optional functions, and
    to be arranged when installing the unit or replacing the PC board.

 2. Jumper Switches with BLACK connectors; to be used for adjusting
    servo control circuits. These need not be readjusted when
    installing the unit or replacing to a spare PC board since they
    have already been adjusted at shipment. Even if a readjustment is
    needed by all means, be sure to make a record of their preset
    status prior to readjust them for the capability of recovery.


 Setting of GREEN Jumper Switches
 --------------------------------

 JP68 Drive Select Jumper Switch
 -------------------------------
 There is the jumper switch to select the drive address number. Set up
 the switch as follows:

    8 7 6 5   8 7 6 5   8 7 6 5   8 7 6 5
   +-------+ +-------+ +-------+ +-------+
   |X o o o| |o X o o| |o o X o| |o o o X|
   |X o o o| |o X o o| |o o X o| |o o o X|
   +-------+ +-------+ +-------+ +-------+
    1 2 3 4   1 2 3 4   1 2 3 4   1 2 3 4
    Drive 0   Drive 1   Drive 2   Drive 3

 As shipped, the jumper pins 1 to 8 is shorted for Drive 0.


 Jumper for Optional Functions
 -----------------------------
 General Reset Jumper Switch
 As an optional feature, there is General Reset signal (J1-2 pin)
 which can be available by the jumper switch (JP70 on SZ073 PCB REV. 3
 SZ073 PCB REV. 4 or 5, SZ073 PCB REV. 6 ).

 Set up the jumper switch as follows:

 General Reset Jumper Switch SZ073 PCB REV. 3

   JP70                      JP70
    +-+                      +-+
    |o| J1-2 pin is OPEN     |X| General Reset Signal is available
    |o|                      |X|
    +-+                      +-+
 Primary                   Optional

 When shipped the jumper is set to the primary position.


 General Reset Jumper Switch SZ073 PCB REV. 4

   JP70                      JP70
    +-+                      +-+
    |X|1 J1-2 pin is OPEN    |o| General Reset Signal is available
    |X|2                     |X|
    |o|3                     |X|
    +-+                      +-+
 Primary                   Optional

 When shipped the jumper is set to the primary position.


 Write Protect Jumper Switch
 ---------------------------
 As an optional feature, there are WRITE PROTECT (J2-7 Pin) and
 WRITE PROTECTED signal (J2-11 pin) which can be available by the
 jumper switches (JP113 and JP117). Setting up these jumper switches
 are as follows:

        Primary
        -------
     JP113     JP117
  10-------6+ +6---4+   JP113 J2-7 pin is connected to J1-16 pin.
  |o X o o o| |o o o|   JP117 J2-11 pin is GND.
  |o X o o o| |o xxx|
  +1-------5+ +1---3+

        Optional
        --------
     JP113     JP117
  10-------6+ +6---4+   JP113 Write Protect signal is available.
  |o o o o o| |o X o|   JP117 Write Protected signal is available.
  |xxx o o o| |o X o|
  +1-------5+ +1---3+

 When shipped, these jumpers are set in the primary position.


 JP182A LED Jumper Switch
 ------------------------
 There is the jumper switch (SZ073 PCB REV. 6 ) deactivating the
 green LCD.

   Primary                 Optional
   -------                 --------
    +-+                       +-+
   1|X| LED activated        1|o| LED deactivated (OFF)
   2|X|                      2|X|
   3|o|                      3|X|
    +-+                       +-+

 When shipped, this jumper is set in the primary position.


 Terminator
 ----------
 If the multiple drives are connected in the daisy chain mode, only
 the last drive must be terminated with a terminator module. When
 shipped, the terminator module (IC#IC) is installed. Remove it all
 but the last drive (if the multiple drives in the daisy chain mode).


 Adjustment Specification (BLACK Jumper)
 ---------------------------------------
 NOTE
 Since adjustment portions are already adjusted when the device is
 shipped, don't move them unless understanding the prior "CAUTION"
 of this chapter.


 JP4A Head Sel #7 Fault Jumper Switch
 ------------------------------------
 (This jumper is available from SZ073 Rev. 7)

 Write Fault caused by invalid head selection is ignored by this
 option. If this option doesn't use, the selection of HD#7 causes
 Write Fault. This option is available on and after SZ073 REV. 7.


   Primary                 Optional
   -------                 --------
    +-+ JP4A                  +-+ JP4A
   1|o| HD#7 selection       1|x| HD#7 selection doesn't
   2|X| causes Write         2|X| causes Write Fault.
   3|X| Fault.               3|o|
    +-+                       +-+

 When shipped, this jumper is set in the primary position.


 PLO free-running frequency
 --------------------------
 - Pull J6 Connector and insert Jumper socket in JP164 for allowing
   the error signal to set at zero.

 - Turn the power on, and adjust the value of JP117-6 pin within the
   range of 10 MHz   1% using JP123.

 - After completion of aforementioned adjustment, turn the power off,
   insert J6 Connector in the original position, and then pull Jumper
   Socket out of JP164.

 - Turn the power on again and ensure that an operation is in normal
   status (device in READY status).


