
C P - 3 0 0 0    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    1045|  980|     |
Capacity form/unform    42/      MB        Heads           2|    5|     |
Seek time   / track  28.0/11.0 ms          Sector/track   40|   17|     |
Controller           IDE / AT              Precompensation
Cache/Buffer             8 KB LOOK-AHEAD   Landing Zone
Data transfer rate    1.500 MB/S int       Bytes/Sector      512
                      4.500 MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep          0.4 W     Humidity     %         8 80    |      8 80
       standby        0.5 W     Altitude    km    -0.061  3.050|        12.200
       idle           2.0 W     Shock        g         5       |     75
       seek           2.8 W     Rotation   RPM      3557
       read/write     4.2 W     Acoustic   dBA        40
       spin-up            W     ECC        Bit   INTERNAL
                                MTBF         h     100000
                                Warranty Month        15
Lift/Lock/Park     YES          Certificates     CSA,IEC380,IEC435,IEC950,U...


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CP3000  PRODUCT MANUAL REV. I, DECEMBER 1990

  +-------------------------------------------------------+
  | +-+J1                                  +-------+      |XX  J5
  | | |                                    +-------+      |xx1 Power
  | | |HDA                               HSP CD DSP ACT   |
  | | |                                                   |XX 40 Pin
  | +-+                                                   |XX Task
  |                                                       |XX File
  |                                                       |XX
  |                                                       |XX Inter-
  |                                                       |XX face
  | SERIAL IN/OUT                                         |XX
  | LED DRIVE                                             |XX J2
  | CAPABILITY                                            |XX
  |+--1                                                   |XX
  ||  |                                                   |  1
  ||  | J4                                                |XX Power J3
  |+--+                                                   |XX
  +-------------------------------------------------------+  1








   (AT) Adapter Card Layout          J1        1
  +-------------------------XXXXXXXXX.XXXXXXXXX-------------+
  |O                              **           2          O |
  |                                E1                       |
  |                                   E2** ***E4          O |
  |                                        E3               |
  |                                                         |
  |                                                         |
  |                                                         |
  |                                                         |
  |                                                         |
  |                                                         |
  |                                                         |
  |                                                       O |
  |                                                         |
  |                                                       O |
  +-------------+           ++                      +-------+
                +++++++++++++++++++++++++++++++++++++



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CP3000  PRODUCT MANUAL REV. I, DECEMBER 1990

 Jumper Setting
 ==============

 Customer Options
 ----------------
 There are four jumper options available for configuration:
 HSP, C/D, DSP, and ACT.

 HSP, when jumpered, connects the -HOST SLV/ACT signal on the inter-
 face to ground for systems that require the slave drive to provide
 -SLAVE PRESENT signal in a two-drive system.

 C/D is the address jumper. When jumpered, the master (or C drive), is
 selected. When open, the slave (or D drive), is selected.

 DSP, when jumpered, indicates to the master drive that a slave is
 present. In a two-drive system, this jumper option must be installed
 in the master, or C drive.

 The last jumper, ACT, connects the -ACTIVE signal to the -HOST
 SLV/ACT signal on the interface. This signal provides the capability
 to drive an external LED. An external current limiting resistor is
 required.

 As an alternative, an LED may be connected between J4, pins 1 and 2.
 This would provide both an open collector drive signal and a current
 limiting resistor connected to +5V respectively.

 The following table shows what the jumper setting should be for
 various system configurations.
   +--------------+--------+---------------+--------------+
   |Jumper        |        |               |              |
   |Configuration |1 Drive |2 Drive Master |2 Drive Slave |
   +--------------+--------+---------------+--------------+
   |    ACT       |    J   |    Note 1     |   Note 1     |
   +--------------+--------+---------------+--------------+
   |    C/D       |    J   |      J        |    NJ        |
   +--------------+--------+---------------+--------------+
   |    HSP       |   NJ   |     NJ        |   Note 2     |
   +--------------+--------+---------------+--------------+
   |    DSP       |   NJ   |      J        |    NJ        |
   +--------------+--------+---------------+--------------+

 NOTE 1:
 In a two drive system, it is possible to drive one LED with both
 drives. An external current limiting resistor is required.

 NOTE 2:
 If the drive is connected to a host that requires that the signal
 -DRIVE SLAVE PRESENT be supplied from the slave drive, via the inter-
 face signal -HOST SLV/ACT, then this jumper must be installed. If
 this jumper is installed, the ACT jumper must not be installed
 because the two jumpers are mutually exclusive.



 J3   DC Power and pin connector assignments
 -------------------------------------------
      /------------\   pin 1    +12 V
      | 4  3  2  1 |   pin 2    GND
      +------------+   pin 3    GND
                       pin 4    + 5 V


 J5   DC Power and pin connector assignments
 -------------------------------------------
      +---------+   pin 1    + 5 V
      | 1  2  3 |   pin 2    +12 V
      +---------+   pin 3    GND



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
CONNER   CP3000  PRODUCT MANUAL REV. I, DECEMBER 1990

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive may be mounted in any attitude!


 Recommended Mounting Configuration
 ----------------------------------
 The CP3000 is designed to be used in applications where the unit may
 experience shock and vibrations at greater levels than larger and
 heavier disk drives.


 Shock Tolerance Features
 ------------------------
 The design features which allow greater shock tolerance are the use
 of rugged heads and media, a dedicated landing zone, closed loop
 servo positioning and specially designed motor and actuator
 assemblies.


 Mechanically Isolated Mounting Points
 -------------------------------------
 Ten base mounting points are provided to the customer. The drive is
 mounted using 6-32 x 1/8" max. insertion for the sides, and 1/4"
 insertion for the bottom. The system integrator should allow ventila-
 tion to the drive to ensure reliable drive operation over the opera-
 ting temperature range.

 For additional vibration isolation, an external suspension system may
 be used.


 Power Connectors
 ----------------
 The CP3000 has a 4-pin DC power connector (J3) mounted on the PCB.
 The recommended mating connector is AMP part number 1-480424-0
 utilizing AMP pins (part number 350078-4 or equivalent).
 DC power may also be supplied to the drive throughh a 3 pin
 connector (J5). The recommended mating connector is Molex part number
 39-01-0033 utilizing Molex pins (part number 39-00-0031 or equiva-
 lent).

 Power is to be supplied at either J3 or J5, but not both.


 Task File Interface Connector
 -----------------------------
 The CP3000 has a 40-pin Task File Interface connector (J2) mounted on
 the printed circuit board. The recommended mating connector is Molex
 part number 10-91-2401 or equivalent. Two drives may be daisy chained
 together at this connector. Maximum cable length is two feet.


 Acoustic Noise
 --------------
 The sound pressure level will not exceed 40dBA at a distance of 1
 meter from the drive.


 Drive Mechanism
 ---------------
 A brushless DC direct drive motor rotates the spindle at 3557 rpm.
 The motor/spindle assembly is balanced to provide minimal
 mechanical runout to the disk. A dynamic brake is used to provide a
 fast stop to the spindle motor when power is removed, or upon
 initiation of STANDBY MODE.


 Air Filtration System
 ---------------------
 The head-disk assembly is a sealed enclosure with an integral 0.3
 micron filter which maintains a clean environment for the heads and
 disks.


 Installation of the Drive and Adapter Card
 ------------------------------------------

  1. Remove power to the computer

  2. If another hard disk controller is installed, it is necessary to
     prevent it from responding to the addresses 1F0-7H and 3F6-7H.
     It is also necessary to ensure that the controller is
     electrically disconnected or tri-stated from IRQ14 of the mother-
     board bus. This may be done either by removing the board, by
     electrically disconnecting the signal from the interface, or by
     setting the jumpers of the board to disable the hard disk
     controller.

  3. Insert the board into any available card slot.

  4. Configure the Host adapter for the correct configuration of your
     computer BIOS.

     Adapter Card Jumpers   E1 and E3 always not installed
                            E2 and E4 always installed

  5. Connect power to the CP3000.

  6. Run the DOS FDISK program to establish DOS partitions.

      Note: DOS 3.3 and below have limitations of 32 megabytes unless
            software utility is used to overcome this.

  7. Run the DOS format programm by typing "Format C:/S". The volume
     may be named with the addition of the "/V". The format will be
     completed and the system transferred if the "/V" option was used.
     The system will ask for a volume name.

  8. Files can then be copied to the C drive from floppy.

  9. When the system is rebooted, the system should boot from the hard
     drive (Drive C) if the floppy is removed.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
CONNER   CP3000  PRODUCT MANUAL REV. I, DECEMBER, 1990

 Key Features
 ------------
 Key features of the CP3000 include:

 - Low power requirements enabling battery operation in portable
   environments

 - High performance rotary voice coil actuator with embedded servo
   system

 - High shock resistance

 - Internal air filtration system

 - Sealed HDA

 - Automatic actuator latch against inner stop upon power down

 - Microprocessor-controlled diagnostics routines that are auto-
   matically executed at start-up

 - Automatic error correction and retries

 - Block size: 512 bytes

 - Emulates IBM Task File and supports additional commands

 - Up to two drives may be daisy-chained on this interface

 - Translate mode (17 sectors, 5 heads, 980 cylinders) is supported

 - Look Ahead Read Capability

 - AC Hysteresis on interface

 - 8K buffer


 Seek Times
 ----------

       +----------------------------------+--------+
       |Track-to-Track         msec.      |   11   |
       +----------------------------------+--------+
       |               Average msec. typ. |   28   |
       |               Average msec. max. |   50   |
       +----------------------------------+--------+
       |Latency                msec. avg. |   8.4  |
       +----------------------------------+--------+


 Functional Description
 ----------------------
 The CP3000 contains all mechanical and electronic parts necessary
 to interpret control signals, position the recording heads over the
 desired track, read and write data, and provide a contaminant free
 environment for the heads and disks.


 Read/Write and Control Electronics
 ----------------------------------
 One integrated circuit is mounted within the sealed enclosure in
 close proximity to the read/write heads. Its function is to provide
 one of two head selection, read pre-amplification, and write data
 circuitry.

 The single microprocessor-controlled circuit card provides the re-
 maining electronic functions, which include:

        - Read/Write Circuitry
        - Rotary Actuator Control
        - Interface Control
        - Spin Speed Control
        - Dynamic Braking
        - Power Management

 At power down or the starts of STANDBY MODE, the heads are
 automatically retracted to the inner diameter of the disk. There they
 are latched and parked on a landing zone that is inside the data
 tracks.


 Head Positioning Mechanism
 --------------------------
 The read/write heads are supported by a mechanism coupled to a voice
 coil actuator.


 Read/Write Heads and Disks
 --------------------------
 Data is recorded on 95mm diameter disk through 3370 type composite
 ferrite heads.


 Error Correction
 ----------------
 The CP3000 performs internal error correction. The error correction
 polynominal is capable of correcting one error bursts with a maximum
 of 8 bits per 512-byte block.


 Diagnostic Routines
 -------------------
 The microprocessor performs diagnostics upon application of power. If
 an error is detected, the CP3000 will not come ready.


 Reliability and Maintenance
 ---------------------------
 MTBF                     100,000 hours (POH)
 MTTR                     10 minutes typical
 Preventive Maintenance   None
 Component Design Life    5 years


 Execute Drive Diagnostic - 90
 -----------------------------
 This command runs the internal diagnostic tests implemented by the
 drive. The diagnostic tests shall only be executed upon receipt of
 this command.

 The drive sets BSY immediately upon receipt of this command. If the
 drive is a master (C/D jumpered) the drive performs the diagnostic
 tests and saves the results. It then checks to see if a slave drive
 is present and waits up to 5 seconds for the slave to complete its
 diagnostics. If the slave successfully completes its diagnostics, it
 asserts -HOST PDIAG.

 If the slave does not successfully complete its diagnostics, it sets
 the error register as follows. The master drive resets BSY,
 and generates an interrupt. The value in the error register should
 be viewed as a unique 8 bit code and not as the single bit flags
 defined previously. The interface registers are set to initial values
 except for the error register if error.

 The table below details the codes in the error register and a
 corresponding explanation:
 +----------+-----------------------------------+
 |Error Code|Description                        |
 +----------+-----------------------------------+
 |    01    |no error detected                  |
 |    03    |sector buffer error                |
 |    8x    |slave drive failed (see note below)|
 +----------+-----------------------------------+

 NOTE
 If the slave drive fails diagnostics, the master drive shall "OR"
 80H with its own status and load that code into the error register.
 If the slave drive passes diagostics or there is no slave drive
 connected, the master drive shall set bit 7 of the Error Register in
 the Task File to 0.


 Error Reporting
 ---------------
 In general, errors are detected in the following fashion by the
 drive microprocessor. At the start of this execution of the command,
 the command register is checked for conditions that would lead to an
 aborted command. Then the operation is attempted. Ayn subsequent
 error terminates the command at the point that is discovered. The
 errors that are valid for each command are summarized in the follow-
 ing matrix. Any subsequent error terminates the command at the point
 that it is discovered.

  +-----------------+---+---+----+----+---+----+---+---+----+---+
  |Commands         |BBK|UNC|IDNF|ABRT|TK0|DRDY|DWF|DSC|CORR|ERR|
  +-----------------+---+---+----+----+---+----+---+---+----+---+
  |Recalibrate      |   |   |    | V  | V | V  | V | V |    | V |
  |Read Sector      | V | V | V  | V  |   | V  | V | V | V  | V |
  |Read Sec. Long   | V |   | V  | V  |   | V  | V | V |    | V |
  |Write Sector     | V |   | V  | V  |   | V  | V | V |    | V |
  |Write Sec. Long  | V |   | V  | V  |   | V  | V | V |    | V |
  |Read Verify Sec. | V | V | V  | V  |   | V  | V | V | V  | V |
  |Format Track     |   |   | V  | V  |   | V  | V | V |    | V |
  |Seek             |   |   | V  | V  |   | V  | V | V |    | V |
  |Exec. Drive Diag.|   |   |    | V  |   |    |   |   |    | V |
  |Initi. Parameters|   |   |    | V  |   |    |   |   |    | V |
  |Read Buffer      |   |   |    | V  |   |    |   |   |    | V |
  |Write Buffer     |   |   |    | V  |   |    |   |   |    | V |
  |Identify Drive   |   |   |    | V  |   |    |   |   |    | V |
  |Inval.Cmnd. Codes|   |   |    | V  |   |    |   |   |    | V |
  |Look Ahead Read  |   |   |    | V  |   |    |   |   |    | V |
  +-----------------+---+---+----+----+---+----+---+---+----+---+

 Key:
 V     = Valid errors for each command
 ABRT  = Abort command error
 BBK   = Bad block detected
 CORR  = Corrected data error
 DRDY  = Drive not ready detected
 DSC   = Disk Drive seek complete not detected
 DWF   = Drive write fault detected
 ERR   = Error bit in the Status Register
 IDNF  = Requested ID not found
 TK0   = Track zero not found error
 UNC   = Uncorrectable data error


 Signal Levels
 -------------
 All signal levels are TTL compatible. A logic "1" is greater than 2.0
 volts. A logic "0" is from 0.00 volts to 0.70 volts.


