
S T 5 2 1 6 0 N   M E D A L I S . P R O    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    4968|     |     |
Capacity form/unform  2170/      MB        Heads           4|     |     |
Seek time   / track  12.0/ 3.5 ms          Sector/track   63|     |     |
Controller           SCSI3 SI/ULTRA        Precompensation
Cache/Buffer           128 KB MULTI-SEGMEN Landing Zone
Data transfer rate    5.000 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     PRML 0/4/4,ZBR                 operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 70
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g         2       |     75
       seek               W     Rotation   RPM      5397
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST52160N  MEDALIST PRO 2160N  JUMPER SETTING

 Jumper Setting
 ==============

 Front View

 J5 Option Block
 ---------------

                   +------- Parity Enable
  (TOP)            |   +--- SCSI ID
                   | +-+-+
            +------+-4-2-1-+
            |o o o o o o o1|
           -+o o o o o o o2+---------------------PWA----------
            ++-+-+---------+
  (BOTTOM)   | | +--------- Remote Start Enable
             | +----------- Terminator Disable
             +------------- Remote LED (13-,14+)

 Termination Power: The drive will provide termination power to the
 drive's terminator chips and to the SCSI bus. Termination power is
 still provided to the SCSI bus when terminators are disabled. No
 other option is available.


   +----------+-----------------------+
   | SCSI ID  |        Jumpers        |
   |          |  4    |  2    |   1   |
   +----------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    2     | OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    3     | OPEN  | CLOSED| CLOSED| default
   +----------+-------+-------+-------+
   |    4     | CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+
   |    5     | CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+
   |    6     | CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+


