
C P - 3 0 1 7 0    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    2116|     |     |
Capacity form/unform   172/      MB        Heads           2|     |     |
Seek time   / track  13.0/ 3.0 ms          Sector/track     |     |     |
Controller           SCSI2 SINGLE-ENDED    Precompensation
Cache/Buffer            32 KB              Landing Zone
Data transfer rate    3.900 MB/S int       Bytes/Sector      512
                      8.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep          0.3 W     Humidity     %         8 80    |      8 80
       standby        0.4 W     Altitude    km    -0.061  4.575|        12.200
       idle           2.5 W     Shock        g         5       |     50
       seek           3.8 W     Rotation   RPM      4500
       read/write     3.5 W     Acoustic   dBA        40
       spin-up            W     ECC        Bit
                                MTBF         h     250000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates



**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CP30340/30170 FILEPRO SCSI  CUSTOMER OPTIONS

  +---------------------------------------------------------+
  |       +-+                                             ++|XX J2
  |       | |                                             |||XX
  |       | |J1                                Terminator |||XX I
  |       | |HDA                                          |||XX N
  |       +-+                                             |||XX T
  |                                                       |||XX E
  |                                            TERMPWR-+  ++|XX R
  |+-+J3                                             +-+  ++|XX F
  ||x|RESERVED                                            |||XX A
  ||x|LED Drive                                Terminator |||XX C
  ||x|                                                    |||XX E
  |+-+                                                    |||XX
  |J4 E1                                                  |||XX
  |+-+ |                                                  ++|X1
  ||x|E3                                                    |
  ||x|DSPN                                                  |XX1 J5
  |+-+RESERVED                                              |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CP30340/30170 FILEPRO SCSI  CUSTOMER OPTIONS

 Jumper Setting
 ==============


 E1-E3 SCSI ID
 -------------
   +----------+-----------------------+
   | SCSI ID  |        Jumpers        |
   |          |   E3  |   E2  |   E1  |
   +----------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  |
   |    1     | OPEN  | OPEN  | CLOSED|
   |    2     | OPEN  | CLOSED| OPEN  |
   |    3     | OPEN  | CLOSED| CLOSED|
   |    4     | CLOSED| OPEN  | OPEN  |
   |    5     | CLOSED| OPEN  | CLOSED|
   |    6     | CLOSED| CLOSED| OPEN  |
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+
 There are three jumpers available for configuration of SCSI ID: E1,
 E2, and E3.

 Delay Spin: A jumper in the DSPN (E4) location, disables spin up on
 power-on. Disabling spin up on application of power can also be
 enabled by setting the DSPN bit in MODE SELECT page 0.

 TERMPWR Output Enable

 Terminators
 -----------
 Remove in all but last drive in chain.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
CONNER   CP30340/30170 FILEPRO SCSI  CUSTOMER OPTIONS

 Mounting Holes
 --------------
 Side:   6-32 UNC-2B .15 Max. Insertion
 Bottom: 6-32 UNC-2B .25 Max. Insertion



 J5   DC Power and pin connector assignments
 -------------------------------------------
 -------------------+
 --+  +-----J5-----+|  pin 1    +12 V
  1|  | 1  2  3  4 ||  pin 2    Ground
  -+  +------------+|  pin 3    Ground
  ------------------+  pin 4    + 5 V



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
CONNER   CFA-170S/340S  PRODUCT MANUAL REV. A, 501-058, 10/1993

 Overview of the Drives
 ----------------------
 The Conner Filepro CFA-170S and CFA-340S are high performance, low-
 profile hard disk drives that are designed to operate in a system
 with a Small Computer System Interface (SCSI). The command set is
 SCSI-2 compatible. The drives are actually two versions of the same
 basic mechanism.


 Features of the Drive
 ---------------------
 - Can be installed in a wide range of host systems

 - Supports SCSI-2 interface and commonly used SCSI-2 commands

 - High performance rotary voice coil actuator with embedded servo
   system

 - One-of-seven run-length limited code

 - High shock resistance

 - Sealed head/disk assembly

 - Internal air filtration

 - Low power consumption

 - Automatic actuator latch over data-free landing zone during shut-
   down mode or power down

 - Microprocessor-controlled diagnostic routines are automatically
   executed at start-up

 - 64K buffer

 - Reed-Solomon error detection and correction with on-the-fly single-
   burst correction

 - Automatic error correction and retries, ECC on-the-fly

 - 512-byte block size

 - 10 MB/s synchronous or 5.0 MB/s asynchronous data transfer

 - Read look-ahead buffering


 Drive Motor and Spindle
 -----------------------
 A brushless DC direct-drive motor assembly is mounted on the drive's
 base. The motor rotates the drive's spindle at 4,011 RPM. The motor/
 spindle assembly is dynamically balanced to provide minimal
 mechanical runout to the disks. A dynamic brake is used to provide a
 fast stop to the spindle motor and return the heads to the landing
 zone when power is removed.


 Firmware
 --------
 The drive's firmware includes a command set that the host uses to
 control the drive. The command set allows the host to request the
 following types for actions:

 - report drive status
 - seek a specific point on the disk
 - read and write data.


 Error Correction
 ----------------
 The drive uses a Reed-Solomon code to perform error detection and
 correction. For each 512-byte block, the software error correction
 poilynomial is capable of correcting:

 - One error burst with of up to 22 bits

 - Two error bursts of up to 11 bits each

 Single bursts of 11 bits or less are corrected on the fly (OTF) with
 no performance degradation.


 Magnetic Field
 --------------
 The disk drive will meet its specified performance while operating in
 the presence of an externally-produced magnetic field under the
 following conditions:

  Frequency Field       Intensity
  DC                    6 gauss
  To 700 kHz            7 milligauss
  700 kHz to 1.5 MHz    3 milligauss


 Acoustic Noise
 --------------
 The sound pressure level will not exceed 40 dBA in Idle Mode at a
 distance of 1 meter from the drive.


