
S T 1 4 0 0 A    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders    1475| 1018|     |
Capacity form/unform   332/  381 MB        Heads           7|   12|     |
Seek time   / track  14.0/ 2.5 ms          Sector/track     |   53|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate    3.125 MB/S int       Bytes/Sector      512
                      8.000 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 70
Power: sleep              W     Humidity     %         8 80    |      5 95
       standby            W     Altitude    km    -0.305  3.048| -0.305 12.210
       idle           9.5 W     Shock        g         2       |     50
       seek          12.0 W     Rotation   RPM      4412
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     150000
                                Warranty Month        12
Lift/Lock/Park     YES          Certificates     CSA,IEC950,UL1950,UL478,VDE  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST1480A FAMILY  PRODUCT MANUAL 77738463-B

  +---------------------------------------------------------+
  |                                          4 or 6  1---J6 |+-1
  |                                          pin     +---+  || |J5
  |                                                         || |
  |                                                         |+-+
  |                                                         |X1 Power
  |                                                         |XX
  |                                                         |
  |                                                         |X1 40 pin
  |                                                         |XX I/O
  |                                                         |XX Cable
  |                                                         |XX J4
  |                                                         |.X
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST1480A FAMILY  PRODUCT MANUAL 77738463-B

 Jumper setting
 ==============

 Note: This description of each jumper position is only valid on
 drives that have J6 with 4 pins (2x2).

 The function of the options are industry compatible. Headers used are
 the standard .1" center type. A description of the function of each
 jumper position is given below. Default jumpers are marked by "*".


 J5  Configuration Select Header
 -------------------------------

         +-------------1-+
         | E  D  C  B  A |
    -----+---------------+


 Jumper  Function
 ----------------
 *A      REFSIG: This location provides a port for external
         connection of the synchronized spindle reference signal (Pin
         1) and ground (Pin 2). The reference signal is bi-directional
         single-ended, and terminated without an external resistor. It
         is also available on J4 Pin 28 if the factory jumper is
         installed. The drive will self-determine if it is a master or
         slave for spindle synchronization.

  B      HOST DRIVE 1/ACT: When this shunt is installed, DRIVE 1
         PRESENT (provided by the output of 74HCT14) is applied to J4
         pin 39 for system that require this signal from drive 0. This
         shunt is mutually exclusive with the ACTIVE shunt. (i.e., if
         jumper "B" is installed Jumper "E" must not be installed).

 *C      DRIVE 0: When this shunt is installed, the drive is
         configured as drive 0. When not installed, the drive is drive
         1.

  D      DRIVE 1 PRESENT: When installed, this shunt indicates to
         drive 0 that drive 1 is present. This shunt must be installed
         on drive 0 in a two-drive system.

  E      ACTIVE: When this shunt is installed, DASP- is made present
         on J4 pin 39. This shunt is mutually exclusive with the HOST
         DRIVE 1/ACT shunt (i.e., if "E" is installed, "B" must not be
         installed).


 J6  LED
 -------


        +------------------  LED Driver
        |     +------------  Pin 1
       ++-----+-+
       | O    O |
       | O    O |
    ---++-----+-+--PWA
        |     +------------  Reserved Jumper Position
        +------------------  Remote LED Connection



 --------------------------------------------------------------------

 Note: This following description of each jumper position is only
 valid on drives that have J6 with 6 pins (2x3).

 The function of the options are industry compatible. Headers used are
 standard .1" center type. A description of the functions of each
 jumper position is given below. Default jumpers are marked by "*".

 J5
 --
      +-A-------------+   +-----------------+  +-----C---------+
      | x  o  o  o  o1|   |  o  o  o  o  o1 |  | o  xxxx  o  o1|
      | X  o  o  o  o |   |B xxxx  o  o  o  |  | o  o  o  o  o |
      +---------------+   +-----------------+  +---------------+

      +-------D-------+   +--------E--------+  +----------F----+
      | o  o  x  o  o1|   |  o  o  xxxx  o1 |  | o  o  o  x  o1|
      | o  o  X  o  o |   |  o  o  o  o  o  |  | o  o  o  X  o |
      +---------------+   +-----------------+  +---------------+

      +-----------G---+
      | o  o  o  xxxx1|
      | o  o  o  o  o |
      +---------------+

 Jumper      Jumper Function Description
 Position
 -----------------------------------------
 A      B
 -      -
 OFF    OFF  Drive is the slave (Drive 1).
 OFF    ON   Drive is the master (Drive 0) with slave (Drive 1)
             present.

 C
 -
 ON          Slave (Drive 1) Present is connected to J4 pin 39. This
             Jumper is mutually exclusive with jumpers "D" and "E"
             (jumper "D" or "E" cannot be installed if jumper "C" is
             installed).
 OFF         Slave Present is not connected to J4 pin 39.

 D
 -
 ON*         DASP- is connected to J4 pin 39. This jumper is mutually
             exclusive with jumpers "C", "D", "F", and "G" cannot be
             installed if jumper "E" is installed).
 OFF         DASP- is not connected to J4 pin 39.

 E
 -
 ON          REFSIG is connected to J4 pin 39. This jumper is mutually
             exclusive with jumpers "C", "D", "F", and "G" (jumper
             "C", "D", "F", or "G" cannot be installed if jumper "E"
             is installed).
 OFF         REFSIG is not connected to J4 pin 39.

 F
 -
 ON          No external reference for REFSIG. This jumper is mutually
             exclusive with jumper "E", "G", and "H" (jumper "E", "G",
             and "H" cannot be installed if jumper "F" is installed).
 OFF         This location provides a port for external connection of
             the synchronized spindle reference signal (Pin 3) and
             ground (Pin 4).

 G
 -
 ON          REFSIG is connected to J4 pin 28. This jumper is mutually
             exclusive with jumpers "E" and "F" (jumper "E" and "F"
             cannot be installed if jumper "G" is installed.
 OFF         REFSIG is not connected to J4 pin 28.



 Synchronozed Spindle Operation
 ------------------------------
 The option allows two drives operationg from the same host to operate
 their spindles at the same synchronized rotational rate. A system of
 synchronized spindle drives is self-arbitrating in establishing the
 master-slave relationship. Drives operating in a system in
 synchronized mode increase the system capacity and transfer rate in
 a cost effective manner.

 A synchronized spindle array application may contain u to 9 drives
 (max.) on one twisted pair Reference Index cable connection.

 J6  LED
 -------


      +-1--2--3-+
      | o  o  o-+---Pin 1
      | o  o  o |
    --+---------+--


 Jumper      Jumper Function Description
 Position
 ----------------------------------------
    1        Remote LED connection. Pin 6 is connected to +5V through
             a 147 ohm resistor. Pin 5 is LED driver.

    2        Conners/ATA mode. When the jumper is ON, IORDY is not
             connected to J4, DMACK- is connected to J4 pin 27, and
             DMARQ is connected to J4 pin 29. When the jumper is OFF,
             IORDY is connected to J4 pin 27, DMACK- is connected to
             J4 pin 29, and DMARQ is connected to J4 pin 21.

    3        Reserved jumper position.


 --------------------------------------------------------------------

 Note: Pins on the drive select and configuration select header (J5)
 are provided to facilitate manual drive configuration. No devices
 other than jumpers should be connected to these pins. Except for
 jumper position A. Connections to external devices (switches,
 connectors, etc.) could adversely affect drive performance. Exact
 location of these pins and headers may change without notice.


 DC Power Connector
 ------------------

              +-4----3-----2-----1--+
              |+5V  +5V  +12V  +12V |
              |      Ret  Ret       |
              +---------------------+



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SEAGATE  ST1480A FAMILY  PRODUCT MANUAL 77738463-B

 Notes on installation
 =====================

 Drive Orientation
 -----------------
 The balanced rotary arm actuator design of the drive allows it to
 be mounted in any orientation. All drive performance characterization
 however, has been done with the drive in horizontal (disc level) and
 vertical (drive on its side) orientations, and these are the two
 preferred mounting orientations.


 The drive is designed, manufactured, and tested with a "Plug-in and
 Play" installation philosophy. Basically, this philosophy minimizes
 the requirements for highly trained personnel to integrate the drive
 into an OEM's system, wether in a factory or field environment.

 - If one drive is on the AT (IDE) bus, insure that the AT (IDE) bus
   ID of the drive is set for drive 0.

 - If two devices are on the bus insure that the drive 0/ drive 1 ID
   Jumper of each drive is correct for its position on the bus
   (select a drive 0 and a drive 1).

 - If the drive is the only device on the bus it should be attached to
   end of the AT (IDE) bus cable (18 inch max length).

 - Set all appropriate option jumpers for desired operation prior to
   power on. If jumpers are changed after power has been applied the
   drive must be power cycled for the new settings to be affect.

 - In all cases where additional drives are added on the AT (IDE) bus
   it will be necessary to logically install the new drive onto the
   system.


 Mounting Holes
 --------------
 Four 6-32 UNC-2A screws are required for installation. Maximum
 mounting screw length into chassis is 0.125 inches (3.17 mm).


 Cooling
 -------
 The cabinet cooling must be designed by the customer so that the
 ambient temperature immediately surrounding the drive will not exceed
 temperature conditions. Specific consideration should be given to
 make sure adequate air circulation is present around the components
 on the PWA.


 Service Tools
 -------------
 No special tools are required for site installation or recommended
 for site maintenance. The depot repair philosophy of the drive
 precludes the necessity for special tools. Should repair of any part
 of the drive be desired, drive should be sent through purchase source
 to the factory repair depot. There are no spare parts for the drive
 avaiable. Call 1-800-468-3472 if purchase source cannot arrange for
 return of the drive.


 Air Cleanliness
 ---------------
 The driv is designed to operate in a typical office environment with
 minimal environment control.


 Interface Cabling Options
 -------------------------
 The drive is capable of operating on the AT (IDE) bus in a daisy
 chained configuration with a second drive/controller that operates
 in accordance with these specification. One drive is designated as
 master (drive 0) and the other as the slave (drive 1).


         +-----------------------------------------+
         |                  HOST                   |
         |        I/O                              |
         +---------+-------------------------------+
                   |
                   |
                   +----------------+
         +---------+--+  +----------+--+
         | AT (IDE)   |  | AT (IDE)    |
         | Drive 0    |  | Drive 1     |
         +------------+  +-------------+




 DC Cable and Connector
 ----------------------
 The drive receives DC power through a 4 pin connector mounted on the
 main circuit board. Recommended part numbers for the mating connector
 are included below, but equivalent parts may be used.

 Type of cable:      18 AWG
 Connector:          AMP 1-480424-0
 Contacts:           AMP 60619-4 (Loose Piece); AMP 61117-4 (Strip)



 I/O Cable and Connector
 -----------------------
 The I/O connector is a 40 pin connector. A key is provided by the re-
 moval of Pin 20. The corresponding pin on the cable connector should
 be plugged. Seagate recommends keying this connector to prevent the
 possibility of installing it upside down.

 Maximum I/O cable length is 18 inches (.45 metres).

 Recommended part numbers for the mating connector are included below,
 but equivalent parts may be used.

 Connector:          40 pin, 3M-3417-7000 (Strain relief 3448-2040)
 Cable:              Flat Cable (Stranded AWG 28) 3M-3365-40
                     Flat Cable (Stranded AWG 28) 3M-3517-40 (Shielded
                     Cable)


 Grounding
 ---------
 Signal ground (PWA) and HDA ground are connected together in the
 drive and cannot be separated by the user. The chassis ground is not
 connected to the HDA and PWA ground. A chassis grounding quick
 disconnect Tab is provided at the rear of the drive above the DC
 power connector. Mating connector to connect a system chassis ground
 to the grounding tab is AMPP/N 62137-2. If it is desired for the
 system chassis ground to be connected to the HDA/PWA ground, the
 systems integrator or user must provide a flexible ground strap be-
 tween HDA and chassis ground point. Such a strap must not interfere
 with the ability of the HDA to meet shock and vibration
 specifications.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
SEAGATE  ST1480A FAMILY  PRODUCT MANUAL 77738463-B

 General Description
 -------------------
 The ST1480A Family drives are members of a family of low cost, high
 performance, highly reliable, random access storage devices designed
 to meet the needs of the OEM, AT (IDE) compatible, marketplace.

 Standards
 ---------
 The ST1480A Family has been developed as system peripherals to the
 highest standards of design and construction. The ST1480A Family
 drives depends upon their host equipment to provide adequate power
 and environment in order to achieve optimum performance and
 compliance with applicable industry and governmental regualations.
 Special attention must be given in the areas of safety, power
 distribution, shielding, audible noise control, and temperature
 regulation.

 The ST1480A Family complies with Seagate standards.

 Each Member of the ST1480A Family UL Recognized component per UL 478
 or UL1950 and a CSA Certified component per CSA C22.2 No. 220-M1986
 or CAN/CSA-C22.2 No. 950-M89.It also meets the requirements of DIN
 VDE 0805/05.90, and EN 60950:1988 (IEC 950).

 The drive as delivered, is designed for system integration before
 use. It is supplied as a component or subassembly as defined in the
 FCC Rules and Regulations, Part 15, Subpart J governing EMI of
 computing devices and the Radio Interference Regulations of the
 Canadian Department of Communications. The drive is, therefore, not
 directly subject to the FCC rules and regulations or the Radio Inter-
 ference Regulations of the Canadian Department of Communications.


 The head, disc and actuator chamber (HDA) is environmentally sealed
 at the factory. Air is recirculated within the HDA and passes through
 a nonreplaceable filter to ensure the maintenance of a contamination
 free disc/actuator environment.

 The ST1480A Family uses a dedicated landing zone at the innermost
 radius of the media thus eliminating the possibility of destroying or
 degrading data by landing in the data zone. Head parking is done
 automatically by the drive. The Host need not send a command that
 sends the heads to the parking zone.

 The ST1480A Family drives incorporate an automatic shipping look
 which prevents potential damage to the heads and discs caused by
 movements during shipping and handling. The shipping lock is
 automatically disengaged when power is applied to the drive.

 The ST1480A Family drives decode Track 0 location from the dedicated
 servo surface thereby eliminating mechanical transducer adjustments
 and related reliability concerns.

 The ST1480A Family drives use a high performance actuator assembly
 consisting of a low inertia, balanced, patented, straight arm design
 which provides excellent performance with minimum power dissipation.



 Media Description
 -----------------
 The media used on the drive has a diameter of approximately 3.5
 inches (89 mm). The aluminum substrate is coated with a thin film
 magnetic material, overcoated with a proprietary protective layer for
 improved durability and environmental protection.

 Each data surface has a total of 1474 tracks and is capable of
 storing 54 Mbytes of unformatted data.

 Media defects are characterized as correctable or uncorrectable de-
 pending on the type and magnitude of the media flaw. The drive media
 certification is performed using the following standards:

            An error burst of 11 bits or less is a correctable error.

            An error burst greater than 11 bits in length is an un-
            correctable error.

 In each ot the above cases reallocation is performed during factory
 media certification testing. In other words, all known correctable or
 uncorrectable defects are reallocated at the factory.

 At the time of shipment from the point of manufacture, the drive
 recording surfaces will meet the following requirements.

       1. 1475 total physical tracks per surface.

       2. Tracks 0 to be error free on each data surface.

       3. 50 defects per surface maximum.

       4. Accumulative defects not to exceed one per megabyte, based
          on total available unformatted drive capacity.


 Defect and Error Management
 ---------------------------
 The drive, as delivered, complies with this specification. The read
 error rate and specified storage capacity are not dependent upon use
 of defect management routines by the host.

 Defect and error management in the AT system involves the drive
 internal defect/error management and AT system error considerations
 (error in communications between host and the drive). Tools for use
 in designing a defect/error management plan are briefly outlined in
 this section, with references to other sections where further details
 are given.


 Drive Internal Defect/Errors
 ----------------------------
 Identified defects are recorded on the drive defects list tracks
 (referred to as the primary or ETF defect list). These known defects
 are assigned new locations during the initial drive format operation
 at the factory. The drive internal retries and data correction by ECC
 should be enabled to recover data from additional flaws if they
 occur. If data correction by ECC is required to recover data, the
 host should immediately re-assign or mark the sector "bad block" by
 use of the Format Track command. If the drive automatic retries and
 data correction by ECC are disabled, defects are usally unrecoverable
 and need to be re-assigned or marked "bad block" as they are
 discovered.


 Logical Capacity
 -----------------
 The drive has an embedded controller that has the capability to
 translate the drive's actual, physical heads, cylinders and sectors
 values to logical, apparent values when communicating with a host
 controller. Thus a host system not having a disc drive table entry
 that fits the drive physical configuration can install the drive
 as a drive having a heads, cylinders and sectors configuration
 matching some drive that is listed in the Host's BIOS drive table.
 The host sends the Initialize Drive Parameters command to the
 embedded controller in the drive and it translates the drive's
 physical heads and sectors to whatever they need to appear to be to
 install on the host system as they selected type. The capacity
 achieved in the translate mode depends on the logical configuration
 to which the drive "translates". The Logical configuration must
 equate to less than or equal to the drives maximum specified
 capacity.

 Recommended Logical values of parameters are as follows:

    ST1480A      895 cylinders     15 heads     62 sector/track
    ST1400A     1018 cylinders     12 heads     53 sector/track
    ST1401A      726 cylinders     15 heads     61 sector/track


 Formatting
 ----------
 It is not necessary to low level format this drive. The drive is
 shipped from the factory low level formatted in 512 byte physical
 sectors. The drive translates its physical format structure to
 simulate a Logical format as required by host.



 Seek Time
 ---------
                                           ST1480A/|         |
                                          |ST1400A | ST1401A |
        ----------------------------------+--------+---------+
        Track-to-Track         msec. typ. |   2.5  |   2.5   |
                               msec. max. |   4.5  |   4.5   |
                       Average msec. typ. |  14    |  12     |
                       Average msec. max. |  16    |  14     |
        Maximum Seek Time      msec. typ. |  26    |  24     |
                               msec. max. |  32    |  28     |
        Latency                msec. avg. |   6.80 |   6.80  |
        ----------------------------------+--------+---------+


    Including Controller Overhead
    -----------------------------
                                           ST1480A/|         |
                                          |ST1400A | ST1401A |
        ----------------------------------+--------+---------+
        Track-to-Track         msec. typ. |   2.9  |   2.9   |
                               msec. max. |   4.9  |   4.9   |
                       Average msec. typ. |  14.4  |  12.4   |
                       Average msec. max. |  16.4  |  14.4   |
        Maximum Seek Time      msec. typ. |  26.4  |  24.4   |
                               msec. max. |  32.4  |  28.4   |
        Latency                msec. avg. |   6.80 |   6.80  |
        ----------------------------------+--------+---------+

 Seek time is defined as the required time from the receipt of a Seek
 Command by the drive until the completion of the seek operation.
 Average seek time is determined by dividing the sum of the time for
 all possible seek movements by the total number of seek movements.
 Drive level seek times do not include controller overhead, the time
 required by the drive controller to process the command.


 Spindle Speed and Latency
 -------------------------
 The spindle speed is 4412   0.5% r/min. The speed tolerance includes
 motor performance and motor control circuit tolerances.

 The average latency time is 6.80 milliseconds, based on a nominal
 disc speed of 4412 r/min.


 Host/Drive Interface data transfer rate
 ---------------------------------------
 Maximum instantaneous:  8.0 Mbytes/s
 Maximum average:        5.5 Mbytes/s


 Power Sequencing
 ----------------
 Power sequencing is not required for the drive. The drive protects
 against inadvertent writing during power up and down.


 Temperature
 -----------
 The drive will meet all specifications over a 41*F to 122*F (5*C to
 50*C) ambient temperature range with a maximum gradient of 36*F
 (20*C) per hour. The enclosure for the drive should be designed such
 that the temperatures at the locations are not exceeded. Air flow may
 be needed to achieve these temperature values. Operation at case
 temperatures above these values may adversely affect the drives
 ability to meet specification.


 Heat/Power Dissipation
 ----------------------
 Typical power dissipation is 12 watts (41 BTUs per hour) of DC power
 average at nominal voltages. Typical power dissipation under idle
 operating conditions is 9.5 watts (32.4 BTU's per hour).



 Reliability
 -----------
 The following reliability specifications assume correct host/drive
 operational interface has been implemented, including all interface
 timings, power supply voltages, environmental conditions, and
 appropriate data handling circuit to the host system.

 MTBF                     150,000 hours
 Service Life             5 years
 Preventive Maintenance   None required



**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
SEAGATE   SUPPORT SERVICES

 Seagate Technology
 ------------------
 Technical Support Services
 If you need assistance installing your drive, consult your dealer.
 Dealers are familiar with their unique system configurations and can
 help you with system conflicts and other technical issues. If you
 need additional assistance with your Seagate(r) drive or other
 Seagate products, use one of the Seagate technical support services
 listed below.

 SeaFONE at 1-800-SEAGATE (1-800-732-4283)
 Seagate's 800 number allows toll-free access to automated self-help
 services, providing answers to commonly asked questions,
 troubleshooting tips and specifications for disc drives and tape
 drives. This service is available 24 hours daily and requires a
 touch-tone phone. If you need to speak to a technical support
 engineer, dial this number and listen to the options for technical
 support. (International callers can also reach this automated
 self-help service by dialing 408-456-4496).


 Seagate Technology online services
 Using a modem, you can obtain troubleshooting tips, free utility
 programs, drive specifications and jumper settings for Seagate's
 entire product line. You can also download software for installing
 and analyzing your drive.

 SeaNET
 You can obtain technical information on Seagate drives, Seagate
 software and much more over the Internet from Seagate's World Wide
 Web home page (http://www.seagate.com) or Seagate's ftp server
 (ftp://ftp.seagate.com).

 You may also send E-mail with your questions to DiscSupport@
 Seagate.com or TapeSupport@Seagate.com.


 SeaBOARD
 SeaBOARD is a computer bulletin board system (BBS) that contains
 information about Seagate's disc and tape drive products and is
 available 24 hours daily. Set your communications software to eight
 data bits, no parity and one stop bit (8-N-1). SeaBOARD phone numbers
 are listed in the following table.

 BBS Location           Modem number
 United States      Disc: 408-434-1080; Tape: 408-456-4415
 England            44-1628-478011
 France                         33 1-48 25 35 95
 Germany            49-89-140-9331
 Singapore          65-292-6973
 Thailand           662-531-8111
 Australia          61-2-9756-2359
 Taiwan             886-2-719-6075

 Seagate CompuServe forum
 Online technical support for Seagate products is available on
 CompuServe. To access our technical support forum, type go seagate.
 This forum provides information similar to that found on SeaBOARD.
 In addition, you can type questions or browse through previous
 questions and answers on the forum messages.

 Seagate Technology FAX services
 SeaFAX
 You can use a touch-tone telephone to access Seagate's automated FAX
 system to receive technical support information by return FAX. This
 service is available 24 hours daily.
 Location               Telephone number
 United States          1-800-SEAGATE or 408-456-4496
 England                44-1628-894084
 Australia              61-2-9756-5170

 Seagate technical support FAX
 You can FAX questions or comments to technical support specialists 24
 hours daily. Responses are sent during business hours.
 Location               FAX number
 United States          408-944-9120
 England                        44-1628-890660
 France                 33 1-46 04 42 50
 Germany                        49-89-1430-5100
 Australia              61-2-9725-4052
 Singapore              65-293-4722
 Hong Kong              852-2368 7173
 Taiwan                 886-2-715-2923
 Korea                          82-2-556-7294/4251


 Seagate technical support
 You can talk to a technical support specialist during business hours
 Monday through Friday for one-on-one technical help.  Before calling,
 note your system configuration and drive model number (STxxxx). There
 are several technical support phone numbers available for various
 Seagate products.

 Location          Telephone  number
 United States Please dial 1-800-SEAGATE for the specific product
               telephone number.
               (6:00 A.M. to 11:15 A.M., 12:30 P.M. to 5:00 P.M.,
               Pacific time, M-F)
 England       44-1628-894083 (10:00 A.M. to 1:00 P.M., 2:00 P.M. to
               5:00 P.M., M-F)
 France        33 1-41 86 10 86 (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Germany       Disc: 49-89-140-9332; (9:30 A.M. to 12:30 P.M., 2:00
               P.M. to 4:00 P.M., M-F)
               Tape: 49-89-140-9333
 Australia     61-2-9725-3366 (9:00 A.M. to 5:00 P.M., M-F)
 Singapore     65-290-3998 (9:00 A.M. to 12:00 P.M., 2:00
               P.M. to 5:00 P.M., M-F)
 Hong Kong     852-2368 9918
 Taiwan        886-2-514-2237
 Korea         82-2-556-8241


 SeaTDD 408-944-9121
 Using a telecommunications device for the deaf (TDD), you can send
 questions or comments 24 hours daily and exchange messages with a
 technical support specialist between 6:00 A.M. to 11:15 A.M. and
 12:30 P.M. to 5:00 P.M. (Pacific time) Monday through Friday.


 Customer Service Centers
 Seagate direct OEM, Distribution, System Integrator and Retail
 customers should contact your Seagate Service Representative for
 warranty information.  Other customers contact your place of
 purchase.  Seagate offers comprehensive customer support for all
 Seagate drives.  Seagate customer service centers are the only
 facilities authorized to service Seagate drives. These services are
 available worldwide.

 Location                       Telephone number                FAX number
 United States          1-800-468-3472;                 405-949-6740
 Other Americas
 (Canada & Brazil)      405-949-6706;               405-949-6738
 Mexico                         525-546-6965;                   525-546-4888
 Europe, Middle
 East & Africa          31-2065-43300;              31-2065-34320
 Asia Pacific &
 Australia              65-485-3595;                    65-485-4980
 Japan                          81-3-5462-2904;                 81-3-3462-2979


 Seagate, Seagate Technology and the Seagate logo are registered
 trademarks of Seagate Technology, Inc. SeaFAX, SeaFONE, SeaBOARD,
 SeaTDD, SeaNET, Medalist and DiscWizard are either trademarks or
 registered trademarks of Seagate Technology, Inc. or one of its
 subsidiaries. All other trademarks or registered trademarks are the
 property of their respective owners.


