
M 2 6 7 1 P    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 8"/FH                 Cylinders        |     |     |
Capacity form/unform      / 2640 MB        Heads          15|     |     |
Seek time   / track  27.0/ 5.0 ms          Sector/track     |     |     |
Controller           IPI-2                 Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      4340
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
FUJITSU => GDT

 Tips & Hints about ICP controllers and other peripherals
 ========================================================

 Tagged queues and Fujitsu M 26xx harddisks
 ------------------------------------------
 Fujitsu Harddisks of the M26XX series do not support the SCSI-II
 feature tagged queues. You should disable this feature in the
 initialize disks menue of the GDTSetup program. An inquiry command
 shows, that the harddisk supports tagged queues (this is why you can
 enable it in the GDTSetup) but this is not true as stated by Fujitsu
 Germany.


