
S Q 3 1 0 5 A    SYQUEST
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders        |  841|     |
Capacity form/unform   105/      MB        Heads            |   16|     |
Seek time   / track  14.5/     ms          Sector/track     |   16|     |
Controller           IDE / AT              Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate    1.950 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SYQUEST  SQ3105  INSTALLATION MANUAL 104323-002 REV. A

  +---------------------------------------------------------+
  |                                                         |XX 3-PIN
  |                                                         |xx POWER
  |                                                         |XXI
  |                                            Jumper       |XXN
  |                                            ****         |XXT
  |                                            ****1        |XXE
  |                                                         |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  |                                                         |XX
  |                                                         |
  |                                                         |XX POWER
  |                                                         |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SYQUEST  SQ3105  INSTALLATION MANUAL 104323-002 REV. A

 Jumper Setting
 ==============

  -----------------+
                   |XX
                   |XX
            ...X   |XXINTERFACE
  MASTER    ...X1  |XX
                   |XX



  -----------------+
                   |XX
                   |XX
  SLAVE     ...o   |XXINTERFACE
            ...o   |XX
                   |XX


  -----------------+
   ACKNOWLEDGE     |XX
   MEDIA CHANGE    |XX
            X...   |XXINTERFACE
            X...   |XX
                   |XX


  -----------------+
   NO MEDIA CHANGE |XX
   MOTIVICATION    |XX
            o...   |XXINTERFACE
            o...   |XX
                   |XX



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SYQUEST  SQ3105  INSTALLATION MANUAL 104323-002 REV. A

 Notes On Installation
 =====================

 Drive mounting
 --------------

     horizontally             vertically
   +-----------------+   +--+             +--+ +------------------+
   |                 |   |  +-----+ +-----+  | |                  | x
   |                 |   |  |     | |     |  | x+----------------+x
 +-+-----------------+-+ |  |     | |     |  | ||x              x||
 +---------------------+ |  |     | |     |  | ||  x          x  ||
                         |  |     | |     |  | ||    x      x    ||
      x           x      |  |     | |     |  | ||      x  x      ||
 +------x------x-------+ |  +-----+ +-----+  | ||       xx       ||
 +-+------x--x-------+-+ +--+             +--+ ||     x    x     ||
   |       xx        |                         ||   x        x   ||
   |     x    x      |                         || x            x ||
   +---x--------x----+                         |x                x|
     x            x                           x++----------------++x
      UNACCEPTABLE!                                UNACCEPTABLE!
      Never install PC board on the Top!

 For best results, the cartridges should be formatted in the same
 position as the final (predominatly) mounted orientation.


 Screw Configuration
 -------------------
 Bottom Mounting: 6-32 UNC (or M4) screws, 4 places. Maximum length
 into drive frame: 0.20-inch (5.08 mm)


 Side Mounting: 6-32 UNC (or M4) screws, 4 places. Maximum length
 into drive frame: 0.13-inch (3.30 mm)



  3-PIN                          4-PIN
  +---+ +---------------------+ +----+
  |OOO+-+ oooooooooooooooooooo+-+OOOO|
  +---+ | ooooooooo oooooooooo| +----+
  POWER +---------------------+  POWER

 Pin 1 = +5V                     Pin 1 = +5V
     2 = NC                          2 = GND
     3 = GND                         3 = NC
                                     4 = NC (Not connected)

 NOTE
 Early versions of the SQ3105 3 pin power connector
 had different (Non-Conners standard) power connections.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
SYQUEST  SQ3105  INSTALLATION MANUAL 104323-002 REV. A

 READ BEFORE YOU BEGIN...
 The SQ3105 is an ATA compatible drive.

 Observe static-discharge precautions: Keep the drive in its static-
 shielded bag until you are ready to complete the installation.

 - Do not touch the PC Board or I/O connector pins.

 - Always handle the drive by the edge or frame. Never apply pressure
   to the PC Board or the top cover.

 Use a grounded wrist strap at your workstation; if unavailble, ground
 yourself frequently by touching the metal chassis of the system
 before handling any components. Provide anti-static padding on all
 work surfaces. Avoid static inducing carpeted areas.


 Drive Configuration
 -------------------
 The user must select the drive features that are appropriate for
 installation in their system. This is done by way of configuration
 jumpers found on the drive PC Board.


 CMOS Configuration (ATA Systems)
 --------------------------------
 Basic information about the drive must be entered in the host system
 CMOS. The number of heads, cylinders and sectors per track are
 specific to each drive and collectively define the drives "geometry".
 CMOS configuration is system dependent and is usually accomplished
 through a keystroke or combination of keystrokes during the POWER-ON
 sequence or a utility such as setup after the system has booted.


 Default Drive Geometry
 ----------------------
 SyQuest ATA interface drives translate their physical drive
 geometry's. If the drive types offered by the CMOS does not support
 the numbers of cylinders, heads and sectors and your system does not
 include a "user-defined" drive type, then select a drive type which
 is less than or equal to the capacity given in the "Capacity"
 section.


