
M K - 1 0 0 2 M A V     H D D - 2 7 3 1    TOSHIBA
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders    3560| 2100|     |
Capacity form/unform  1085/      MB        Heads            |   16|     |
Seek time   / track  13.0/ 3.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA3 EMBEDDED   Precompensation
Cache/Buffer           128 KB              Landing Zone
Data transfer rate    6.900 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -20 60
Power: sleep          0.1 W     Humidity     %                 |
       standby        0.3 W     Altitude    km                 |
       idle               W     Shock        g       100       |    200
       seek           2.5 W     Rotation   RPM      4635
       read/write     2.5 W     Acoustic   dBA        33
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TOSHIBA  MK1002MAV  JUMPER SETTING

 Jumper Setting
 ==============

 Master/Slave
 ------------
 Toshiba's 2,5" hard disk drives can be configured as a master or
 slave. Master configuration is used for all single drive
 applications, Master and Slave configuration (only one of each per
 I/O port) is used for two drive applications. Master configuration
 is obtained by setting Jumper J2 open (no Jumper). Slave
 configuration is obtained by installing a jumper on J2. If Pin #28
 = 0, drive = master. If Pin #28 = 1, drive = slave.

 Jumper J1 is reserved for factory use only.


