
M K - 1 3 3 F A    TOSHIBA
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders     733|     |     |
Capacity form/unform    30/   38 MB        Heads           5|     |     |
Seek time   / track  25.0/ 7.0 ms          Sector/track   32|     |     |
Controller           MFM / ST506           Precompensation   512
Cache/Buffer               KB              Landing Zone
Data transfer rate    0.625 MB/S int       Bytes/Sector      256
                      0.625 MB/S ext
Recording method     MFM                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C           40    |    -40 70
Power: sleep              W     Humidity     %         8 80    |      5 90
       standby            W     Altitude    km    -0.300  3.000| -0.400 15.000
       idle          10.0 W     Shock        g        10       |     40
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA        48
       spin-up            W     ECC        Bit   WITH 11BIT BURST COR
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
TOSHIBA  MK-130FA  PRODUCT SPECIFICATIONS 71Y101562, REV. A

  +---------------------------------------------------------+
  |                                                Factory  |XX
  |                                                +---+PJ5 |XX
  |                                                1---+    |XX J2
  |                                                         |XXData
  |                                                         |  1
  |                                                         |XX
  |                                                  1-+PJ4 |XX
  |                                                  | |    |XX J1
  |                                                  | |    |XXControl
  |                                                  | |    |XX
  |                                                  | |    |XX
  |                                                  | |    |XX
  |                                                  +-+    |XX
  |                                                         |XX
 ++                                                         |  1
 ++LED                                                  1XXXXXX Power
  +---------------------------------------------------------+   J3



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TOSHIBA  MK130FA  PRODUCT SPECIFICATIONS 71Y101562, REV. A

 Jumper Setting
 ==============

 PJ4
 ---
        +-2-----------------------------32+
        | o o o o o o o o o o o o o o o o |
        | o o o o o o o o o o o o o o o o |
        +-1-----------------------------31+

 The 32 pin connector for the selectable functions is provided on the
 printed circuit board. The specific functions are selected by the
 jumper plugs to the pins on this connector.


  Pins    Definitions      Meanings
 -------------------------------------------------------------------
 01, 02   WRITE PROTECT    Write protected when the jumper plug is
                           connected.
 03, 04   RADIAL MODE      The drive is always selected when the
                           jumper plug is connected.
 05, 06   DRIVE NO. 4      UNIT NO. 4 is assigned when the jumper
                           plug is connected.
 07, 08   DRIVE NO. 3      UNIT NO. 3 is assigned when the jumper
                           plug is connected.
 09, 10   DRIVE NO. 2      UNIT NO. 2 is assigned when the jumper
                           plug is connected.
 11, 12   DRIVE NO. 1      UNIT NO. 1 is assigned when the jumper
                           plug is connected.

 13, 14 ---+
 15, 16    |
 17, 18    +--- TERMINATOR Should be closed on the last drive on the
 19, 20    |               daisy-chain.
 21, 22    |
 23, 24 ---+

 25, 26 ---+--- FOR ADJUSTMENT USE ONLY
 27, 28 ---+

 29, 30 ---+--- DRIVE MODEL
 31, 32 ---+


 Drive ID
 --------
 Five pairs are assigned to set the drive number. By these pairs, it
 is possible to set any drive ID from 1 to 4 or to set radial
 connection.


 Write protect
 -------------
 Write protection is activated by the jumper plug to the pair of pins
 of the connector.


 Terminators
 -----------
 Terminator resistors are connected to the interface signals when
 plugged.


 Miscellanious
 -------------
 Two pairs of pins for the drive model definition and two pairs for
 the adjustment are prepaired in the connector. These pairs must not
 be changed by the customer.


 Indicator LED
 -------------
 The indicator LED and the connector for additional external
 indication are prepared at the front on the printed circuit board.
 The signal for indication becomes "ON" when the both UNIT SELECTED
 and READY signals are "TRUE".


 PJ5 FACTORY RESERVED
 --------------------
 1-3 MUST OPEN, and 4 must CLOSED



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
TOSHIBA  MK-130FA  PRODUCT DESCRIPTIONS 71Y101562, REV. A

 Notes on installation
 =====================

 Drive mounting
 --------------

     horizontally             vertically
   +-----------------+   +--+             +--+ +------------------+
   |                 |   |  +-----+ +-----+  | |                  | x
   |                 |   |  |     | |     |  | x+----------------+x
 +-+-----------------+-+ |  |     | |     |  | ||x              x||
 +---------------------+ |  |     | |     |  | ||  x          x  ||
                         |  |     | |     |  | ||    x      x    ||
      x           x      |  |     | |     |  | ||      x  x      ||
 +------x------x-------+ |  +-----+ +-----+  | ||       xx       ||
 +-+------x--x-------+-+ +--+             +--+ ||     x    x     ||
   |       xx        |                         ||   x        x   ||
   |     x    x      |                         || x            x ||
   +---x--------x----+                         |x                x|
     x            x                           x++----------------++x
      UNACCEPTABLE!                                UNACCEPTABLE!
      Never install PC board on the Top!


 Mounting Instructions
 ---------------------
 When mounting the drive, the cabinet frame should keep apart 0.1 inch
 (2.5 mm) or more distance from the outer surface of the HDA and PCB
 for vibrating space.

 Use 4 tap holes located on both sides or bottom side of the drive
 frame for fixing the drive.

 Screws should not be penetrated more than 2.5mm from the outer
 surface of drive frame to keep clearance between screw tips and PCB.

 The drive frame is isolated from the HDA (signal ground).

 Mounting screws M3X0.5, four in bottom, two in each side.


 Cooling
 -------
 Cabinet packaging designs must provide ample air circulation around
 the drive to ensure environmental limits are not exceeded.


 J1 Control Signal Connector
 ---------------------------
 Drive side connector:     Card edge (gilded)
 No. of poles and pitch:   34 poles, 0.1-inch pitch (17-pole double
                           side, even numbered on the component side)
 Porality key slot:        Between pin No. 4 and 6
 Cable-side applicable
 connector:                AMP ribbon connector P/N 88373-3 or
                           Molex P/N 15-35-1341

 Flat cable or twisted pair 6m max.


 J2 Data Signal Connector
 ------------------------
 Drive side connector:      Card edge (gilded)
 No. of poles and pitch:    20 poles, 0.1-inch pitch (10-pole double
                            side, even numbered on the component side)
 Porality key slot:         Between pin No. 4 and
 Cable-side applicable
 connector:                 AMP ribbon connector P/N 88373-6 or
                            Molex P/N 15-35-1201

 Flat Cable or twisted pair 6m max.


 J3 Power Input Connector
 ------------------------
 Drive side connector:     AMP P/N 350211-1 or equivalent
 No. of poles:             4 poles
 Porality:                 Poralized by the form of the connector
                           housing
 Cable-side applicable:    AMP P/N 1-480424-0 and pin P/N 350078-4
                           (chain type) or 61173-4 (loose type)
 Power cable:              Must meet the maximum current consumption
                           of the drive an dthe voltage at the
                           connector end.


 J4 Frame Ground Connector
 -------------------------
 The HDA module (head/disk assembly container) and DC ground (signal
 0V) are short-circuited at the time of factory shipment. However, the
 frame (the part where the mounting tap holes are provided) is
 isolated from DC ground.

 DC ground connector
 Drive side        : Faston terminal AMP P/N 61761-2
 Mating connector  : Faston terminal AMP P/N 62187-1


 DC Power and pin connector assignments
 --------------------------------------
 pin 1    +12 VDC
 pin 2    +12 Volts Return
 pin 3    + 5 Volts Return
 pin 4    + 5 VDC


 Cable Interconnection - 4 Drive System
 --------------------------------------

       HOST
  +-----------+                                +-----------------+
  |           +---o---Control------------------+J1     Drive 1   |
  |           |   |    +-------Data------------+J2               |
  |           |   |    |             +-Power---+J3  GROUND TAB   |+-+
  |           |   |    |             |         +-----+-----------+  |
  |           |   |    |             |    +-Frame----+              |
  |           |   |    |             |    |    +-----------------+  |
  |Controller |   o----+-------------+----+----+J1     Drive 2   |  |
  |           |   |    | +-----------+----+----+J2               |  |
  |           |   |    | |           o----+----+J3  GROUND TAB   |+-+
  |           |   |    | |           |    |    +----+------------+  |
  |           |   |    | |           |    o---------+               |
  |           |   |    | |           |    |    +-----------------+  |
  +-----------+   o----+-+-----------+----+----+J1     Drive 3   |  |
  |           |   |    | | +---------+----+----+J2               |  |
  |           +---+----+ | |         o----+----+J3  GROUND TAB   |+-+
  |           +---+------+ |         |    |    +-----+-----------+  |
  |           |   |        |         |    o----------+              |
  |Data       +---+--------+         |    |    +-----------------+  |
  |Separator  |   +------------------+----+----+J1     Drive 4   |  |
  |           +----------------------+----+----+J2               |  |
  |           |                      o----+----+J3  GROUND TAB   |+-+
  +-----------+                      |    |    +-----+-----------+  |
                      DC voltages ---+    o----------+              |
                                          |                         |
                      Signal Ground ------+                         |
                                                                    |
                      Frame Ground ---------------------------------+

 NOTE
 It is necessary to set ON the terminator by the jumper plug at the
 last drive in connection. Terminator resistance networks for the
 other drives must be set to OFF.

 The total length of control signal cables for four drives must not
 exceed 6 meters. The maximum cable length of a data signal cable is
 6 meters.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
TOSHIBA  MK-130FA  PRODUCT SPECIFICATIONS 71Y101562, REV. A


 General Description
 -------------------
 The MK130FA magnetic disk drive is a fixed magnetic disk drive with
 standard 3.5-inch magnetic disks as recording media. The size and
 mounting details are identical to the industry standard mini floppy
 disk drives.

 The MK130FA is a high-performance magnetic disk drive featuring
 high-speed access, a recording capacity of 23 to 54 Megabytes and
 high reliability employing the Winchester technologies and closed
 loop servo control.

 The disks are driven directly by a DC spindle motor. Air filtration
 is provided by means of a high performance air circulation filter
 system using breather and circulation filters. The drive provides an
 automatic carriage lock mechanism to prevent the damage during non-
 operating and transportation. The printed circuit board contains all
 the electronic circuitry necessary to drive the equipment.

 The circuit board is provided outside outside the HDA and has power
 input and interface signal connectors. The circuit board contains an
 interface circuit read/write circuit, spindle motor control circuit,
 access (seek) and head positioning servo control circuit and abnormal
 condition detecting circuit.

 Options
 -------
 1. Control signal cable
 2. Data transmission signal cable
 3. Front panel


 Write Precompensation
 ---------------------
 Cylinders to be compensated: Cyl. 512 to cyl. 732
 Compensation time:             12ns


 Media Defect
 ------------
 A media defect is a physical defect on media (disk). Such a defect
 causes read errors repeatedly even if this drive is properly adjusted
 and operated in a normal environmental condition. Valid data must not
 be written deallocation or skip displacement techniques must be
 utilized.

 1. Number of defects
    +-----------------+---------+---------+---------+
    |Model            | MK132FA | MK133FA | MK134FA |
    +-----------------+---------+---------+---------+
    |Max. per drive   |    30   |    40   |    50   |
    |Max. per surface |    15   |    15   |    15   |
    +-----------------+---------+---------+---------+

 2. Defect-free tracks
    Head 0 and head 1 of cylinder 000 have no defect for all models at
    the time of factory shipment.

 3. At the time of factory shipment, there does not exist any defect
    that causes an error of 11 and more consecutive bits. Therefore,
    almost all defects may be corrected if ECC (Error Correction Code)
    that can correct a 11-bit error is used.


 Defective Sector Flag
 ---------------------
 At the time of factory shipment, a data sheet is attached to the
 drive, indicating the positions of defective sectors or sectors with
 poor recording quality. The defective positions are indicated by the
 head numbers and the byte address from the INDEX.


