
S T 3 3 2 3 2 A   M E D A L I . 3 2 3 2    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 6253|     |
Capacity form/unform  3200/      MB        Heads           8|   16|     |
Seek time   / track  12.0/ 2.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA3 ULTRA      Precompensation
Cache/Buffer           128 KB MULTI-SEGMEN Landing Zone
Data transfer rate   10.000 MB/S int       Bytes/Sector      512
                     33.300 MB/S ext DMA33
Recording method     2/3 RLL1,7                     operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %                 |
       standby        1.0 W     Altitude    km                 |
       idle           5.4 W     Shock        g         5       |     75
       seek           7.4 W     Rotation   RPM      4500
       read/write     5.5 W     Acoustic   dBA        34
       spin-up            W     ECC        Bit   SMART
                                MTBF         h     300000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST31082A/ST31276A/ST31720A  MEDIALIST 1082/1720/1276A  LAPAZ

 Jumper Setting
 ==============


               J2                   5  12
  +----------------------------+--1+V--V+
  |XXXXXXXXXXXXXXXXXXXXXXXXXXXX|:::|OOOO|POWER
  +----------------------------+++++----+
   Pin 20 removed               ||+--- RESERVED
                                |+-+-- Slave Present (when Master ON)
                                |  +-- Cable Select (when Slave OFF)
                                +----- Master ON, Slave OFF


