
M K - 1 3 4 F A   ( R L L )    TOSHIBA
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders     733|     |     |
Capacity form/unform    65/      MB        Heads           7|     |     |
Seek time   / track  25.0/ 7.0 ms          Sector/track   26|     |     |
Controller           RLL / ST506           Precompensation   512
Cache/Buffer               KB              Landing Zone
Data transfer rate    0.938 MB/S int       Bytes/Sector      512
                      0.938 MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C           40    |    -40 70
Power: sleep              W     Humidity     %         8 80    |      5 90
       standby            W     Altitude    km    -0.300  3.000| -0.400 15.000
       idle               W     Shock        g        10       |     40
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA        48
       spin-up            W     ECC        Bit   WITH 11BIT BURST COR
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
TOSHIBA  MK-130FA  PRODUCT SPECIFICATIONS 71Y101562, REV. A

  +---------------------------------------------------------+
  |                                                Factory  |XX
  |                                                +---+PJ5 |XX
  |                                                1---+    |XX J2
  |                                                         |XXData
  |                                                         |  1
  |                                                         |XX
  |                                                  1-+PJ4 |XX
  |                                                  | |    |XX J1
  |                                                  | |    |XXControl
  |                                                  | |    |XX
  |                                                  | |    |XX
  |                                                  | |    |XX
  |                                                  +-+    |XX
  |                                                         |XX
 ++                                                         |  1
 ++LED                                                  1XXXXXX Power
  +---------------------------------------------------------+   J3



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TOSHIBA  MK130FA  PRODUCT SPECIFICATIONS 71Y101562, REV. A

 Jumper Setting
 ==============

 PJ4
 ---
        +-2-----------------------------32+
        | o o o o o o o o o o o o o o o o |
        | o o o o o o o o o o o o o o o o |
        +-1-----------------------------31+

 The 32 pin connector for the selectable functions is provided on the
 printed circuit board. The specific functions are selected by the
 jumper plugs to the pins on this connector.


  Pins    Definitions      Meanings
 -------------------------------------------------------------------
 01, 02   WRITE PROTECT    Write protected when the jumper plug is
                           connected.
 03, 04   RADIAL MODE      The drive is always selected when the
                           jumper plug is connected.
 05, 06   DRIVE NO. 4      UNIT NO. 4 is assigned when the jumper
                           plug is connected.
 07, 08   DRIVE NO. 3      UNIT NO. 3 is assigned when the jumper
                           plug is connected.
 09, 10   DRIVE NO. 2      UNIT NO. 2 is assigned when the jumper
                           plug is connected.
 11, 12   DRIVE NO. 1      UNIT NO. 1 is assigned when the jumper
                           plug is connected.

 13, 14 ---+
 15, 16    |
 17, 18    +--- TERMINATOR Should be closed on the last drive on the
 19, 20    |               daisy-chain.
 21, 22    |
 23, 24 ---+

 25, 26 ---+--- FOR ADJUSTMENT USE ONLY
 27, 28 ---+

 29, 30 ---+--- DRIVE MODEL
 31, 32 ---+


 Drive ID
 --------
 Five pairs are assigned to set the drive number. By these pairs, it
 is possible to set any drive ID from 1 to 4 or to set radial
 connection.


 Write protect
 -------------
 Write protection is activated by the jumper plug to the pair of pins
 of the connector.


 Terminators
 -----------
 Terminator resistors are connected to the interface signals when
 plugged.


 Miscellanious
 -------------
 Two pairs of pins for the drive model definition and two pairs for
 the adjustment are prepaired in the connector. These pairs must not
 be changed by the customer.


 Indicator LED
 -------------
 The indicator LED and the connector for additional external
 indication are prepared at the front on the printed circuit board.
 The signal for indication becomes "ON" when the both UNIT SELECTED
 and READY signals are "TRUE".


 PJ5 FACTORY RESERVED
 --------------------
 1-3 MUST OPEN, and 4 must CLOSED


