
M K - 3 0 0 3 M A N    TOSHIBA
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        |     |     |
Capacity form/unform  3080/      MB        Heads            |     |     |
Seek time   / track  13.0/     ms          Sector/track     |     |     |
Controller           IDE / ATA3            Precompensation
Cache/Buffer           128 KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C         5 55    |
Power: sleep              W     Humidity     %         8 80    |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA        35
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
TOSHIBA  MK3003MAN  HDD-2619  JUMPER SETTING







                                                    +-+
      43-------------------------------------------1+C+A+
      |* * * * * * * * * * * * * * * * * * * * * * *|*|*|
   ---+* * * * * * * * * * * *   * * * * * * * * * *|*|*+-----
      44-----------------------+-------------------2+D+B+
                               |                    +-+
                        Polarity Key








**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
TOSHIBA  MK3003MAN HDD-2619  JUMPER SETTING

 Jumper Setting
 ==============

 Master/Slave Configuration
 --------------------------
 Drive address is set by the optional jumper of the interface
 connector.

 If jumper is open, drive is set to be Master.

 If jumper plug is inserted into position C - D, drive is set to be
 Slave.

 If jumper plug is set with position B - D and P28 (CSEL) signal is
 low, drive is Master drive.

 If jumper plug is set with position B - D and P28 (CSEL) signal is
 high, drive is Slave drive.

 In case of using 2 Drives one must set as Master and  the other is
 set to Slave.

 In case of using single Drive, drive must be set as Master.


 PROHIBIT!!
 A-B JUMPER
 A-C JUMPER


