
M 2 9 5 2 R A U    FUJITSU
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    5713|     |     |
Capacity form/unform  2420/      MB        Heads           5|     |     |
Seek time   / track   9.0/ 0.8 ms          Sector/track     |     |     |
Controller           SCSI2 DI/WI/FAST      Precompensation
Cache/Buffer           506 KB MULTI-SEGMEN Landing Zone
Data transfer rate    9.900 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     PR4ML                          operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 60
Power: sleep              W     Humidity     %        20 80    |      5 95
       standby            W     Altitude    km            3.000|        12.000
       idle               W     Shock        g         5       |     50
       seek               W     Rotation   RPM      7200
       read/write         W     Acoustic   dBA        34
       spin-up       11.5 W     ECC        Bit   ON THE FLY
                                MTBF         h    1000000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  M2952/2954R  JUMPER SETTING N1CA01407-0115

  +---------------------------------------------------------+
  |                                                         |
  |                                                         |XX I
  |                                                         |XX N
  |                                            1-+          |XX T
  |                                            | |          |XX E
  1-+                                          +-+CN12      |XX R
  xx|CN7                                                    |XX F
  xx|                                          1-+CN6       |XX A
  +-16                                         | |          |XX C
  |                                            +-+          |XX E
  |                                                         |XX
  |                                                         |XX
  |                                                         |xx
  |                                                         |
  |                                                         |XX Power
  |                                                         |XX
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  M2952R/2954R  JUMPER SETTING

 Jumper Setting
 ==============

 CN6 Spindle motor/Bus parity/Self-diagnostics
 ---------------------------------------------
 Spindle motor control
 ---------------------
 Pin 1/2 CLOSED Auto Start on power up (default)
         OPEN   Controlled by START/STOP UNIT command


 SCSI BUS Parity checking
 ------------------------
 Pin 3/4 CLOSED Enabled (default)
         OPEN   Disabled


 Offline Self-diagnostics
 ------------------------
 Pin 5/6 OPEN   Normal (default)
         CLOSED Execute


 CN7  SCSI ID setting
 ---------------------
   +----------+-------------------------------+
   | SCSI ID  |       Jumper Location         |
   |          |             PINS              |
   |          |  7-8  |  5-6  |  3-4  |  1-2  |
   +----------+-------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |    2     | OPEN  | OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |    3     | OPEN  | OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |    4     | OPEN  | CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    5     | OPEN  | CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |    6     | OPEN  | CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |    7     | OPEN  | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |    8     | CLOSED| OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    9     | CLOSED| OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |   10     | CLOSED| OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |   11     | CLOSED| OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |   12     | CLOSED| CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |   13     | CLOSED| CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |   14     | CLOSED| CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |   15     | CLOSED| CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+

 Set the SCSI ID so that there are no duplicates between SCSI devices
 on the same SCSI bus.


 CN7 Pin 13-14  Write protection
 -------------------------------
 Pin 13-14 SHORT  Enabled
           OPEN   Disabled (default)


 CN7 Pin 09 Ground
         10 Spindle Synchronization Pulse Signal
         11 No Connect
         12 IDD Reset Signal

 CN7 15-16 Remote LED


 CN12 Terminal Setting
 ---------------------
 1-2 CLOSED Enable SCSI Transeiver upper bit



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
FUJITSU  M2952/2954  JUMPER SETTING

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions). Inclination from
 vertical or horizontal should not exceed 5".


 Mounting screw fixing
 ---------------------
 When the mounting screw holes on the side of the drive are used, then
 only use two pairs of outer holes. Do not use the center hole in
 conjunction with only one of the outer holes. The screws must not
 penetrate the drive by more than 4 millimeters.


 Cooling
 -------
 Allow space above and below the  drive to provide for adequate air
 flow. Fan cooling is recommended. The disk enclosure temperature
 measured at top center, should never exceed 55*C.


 Grounding
 ---------
 This drive uses MR (Magneto Resistive) Heads. The disk enclosure (DE)
 must not be connected to ground. The mounting frame is isolated from
 the DE and this should be connected to ground via the mounting
 screws.


 Termination
 -----------
 A terminating resistor should be installed at both ends of the SCSI
 bus. When shipped from the factory, this drive is terminated. If the
 drive is to be used in the middle of the SCSI cable with other
 terminated devices at the ends, or if external termination is to be
 used, then the terminating resistor on the drive must be disabled.


 Termination Power
 -----------------
 TMPWR must be supplied to the terminating resistor for correct
 operation. This can be supplied from either the drive or the SCSI
 bus. If external termination is to be used then TRMPWR should be
 supplied to the SCSI bus.

 Users must ensure that the Disk Enclosure casing is NEVER shorted to
 the computer system's Frame or DC Ground.

 Magneto-Resistive Read heads are a significant factor in the
 achievement of very high capacities in small form factor hard disk
 drives. The M2952 and M2954 drives use Magneto-Resistive (MR) heads
 and therefore requires special handling considerations. The MR head
 must be electrically biased in order to function, and Fujitsu uses
 +5.5 VDC on thes drives. The voltage is generated by the drive
 electronics from normal +5VDC and +12VDC rails, so standard power
 supplies and connectors may be used.

 With the MR heads biased in this way, it becomes importatnt to avoid
 the possibility of discharge between the head and the media, so, in
 order to ensure operational reliability, the disk enclosure (DE)
 and hence the platters themselves are also biased to +5.5VDC rather
 than DC Ground as would be the case on a conventional drive. Fujitsu
 has taken steps to minimise the possibility of accidental shorting
 by coating the DE with an electrically insulating material and by
 removing the earthing tag that would normally by present. Also the
 drive is protected against damage in the event of accidental shorting
 through the use of a protection circuit in the head IC. This works by
 quickly shutting off the bias voltage when it detects a voltage drop.
 Any read or write operation during this time will result in a hard
 data error.

 When the short is removed the bias voltage is automatically restored
 and read/write operations will again work normally. Pay close
 attention to the mounting specifications of the drive ensuring that
 no component of the system is likely to abrade the disk enclosure
 surface.


