
7 0 7 0 - 2 0    MICROSCIENCE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders     960|     |     |
Capacity form/unform    94/      MB        Heads           5|     |     |
Seek time   / track  18.0/     ms          Sector/track   40|     |     |
Controller           IDE / AT              Precompensation   960
Cache/Buffer               KB              Landing Zone      960
Data transfer rate    1.000 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      36000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
MICROSC. 7070-20/7100-00/-20/-21/7200-00  PRODUCT DESCRIPTION

  +---------------------------------------------------------+
  |                                                 +----+J4|XX
  |                                                 1----8  |XX Power
  |                                                         |1
  |                                                         |
  |                                                         |1
  |                                                         |XX I
  |                                                         |XX N
  |                                                         |XX T
  |                                                         |XX E
  |                                                         |XX R
  |                                                         |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |XX E
  |                                                         |XX
  +---------------------------------------------------------+




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
MICROSC. 7070-20/7100-00/20/21/7200-00  PRODUCT DESCRIPTION

 Jumper Setting
 ==============

 J4 Master/Slave Select
 ----------------------

 Pins 1-2  OPEN    Single drive only
 Pins 7-8  OPEN

 Pins 1-2  CLOSED  Master drive in a two drive system
 Pins 7-8  OPEN

 Pins 1-2  OPEN    Slave drive in a two drive system
 Pins 7-8  CLOSED

 The other pins are not used!



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
MICROSC. 7XXX/8XXX SERIES  JUMPER SETTINGS 280095-004, REV. A

 Installation Procedure
 ----------------------

 1. Installation precautions
 ---------------------------
 Four (4) 6-32UNC screws, with 3/16" (4.78mm) maximum screw length,
 are required for installation. Use caution when installing the
 mounting screws to ensure no contact is made with drive's printed
 circuit board.


 2. In the CMOS (System BIOS) setup, select drive type as follows
 ----------------------------------------------------------------
 Select a hard drive type that is equal to or less than the formatted
 capacity of the drive.

 NOTE
 Drive parameters cannot exceed the specified capacity.

 - Use user defined type or manually enter the drive parameters.


 3. Disk partion options
 -----------------------
 Use DOS "FDISK" to create the partition table.
 Utility software such as Disk Manager or Speedstor may be used.


 4. High Level Format Options
 ----------------------------
 If DOS "FDISK" is used to create the partitions, then use DOS
 "FORMAT" to do the high level format.

 If Disk Manager is used to create the partitions, then use Disk
 Manager to do the high level format.

 If Speedstor is used to create partitions, then use Speedstor to do
 the high level format.


 Always low-level formatted at the factory!


