
C F S - 5 4 1 A                 C A B O    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 1048|  524| 1024
Capacity form/unform   540/      MB        Heads           2|   16|   32|   16
Seek time   / track  14.0/ 3.0 ms          Sector/track     |   63|   63|   63
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            64 KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                     16.600 MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep          1.0 W     Humidity     %         8 80    |      8 80
       standby            W     Altitude    km    -0.061  3.048| -0.061 12.192
       idle           3.8 W     Shock        g         5       |     75
       seek           5.7 W     Rotation   RPM      3600
       read/write     4.9 W     Acoustic   dBA        34
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST3541A STINGRAY  QUICK REFERENCE GUIDE

 Jumper Setting
 ==============

 C/D Master/Slave Configuration
 ------------------------------
 CLOSED  Single Drive
 CLOSED  Master Drive
 OPEN    Slave Drive


 CS Cable Select
 ---------------
 OPEN    Cable select option disabled
 CLOSED  Cable select option enabled

 NOTE
 When using the CS option, the C/D jumper must be open.


 Front View                      +----  NOT USED
                                 | +--  Master ON, Slave OFF (C/D)
                                 | |
     (TOP)         o o o o o   o o o1
 Option Block   ---  o o o o---o o o2------------------
    (BOTTOM)       +---+---+   |
                       |       |
           RESERVED ---+       |
           Cable Select  ------+


 The C/D jumper is used to determine whether the drive is a master
 (drive C) or a slave (drive D). The drive is configured as a master,
 when jumpered, and a slave when not jumpered.

 When using CS option, the C/D jumper MUST be open


 Master/Slave Configuration
 --------------------------
 When two drives are daisy-chained on the host interface, one must be
 designated at the master drive (C: drive) and one as the slave drive
 (D: drive). Commands from the host are written in parallel to both
 drives.

 When the C/D jumper on the drive is closed, the drive will assume the
 role of a master. When C/D is open, the drive will act as a slave. In
 single-drive configurations, C/D must remain in the closed (master)
 position.


 Cable Select
 ------------
 This optional method of drive master/slave designation can be enabled
 by jumper selection as described below. If used, special cabling can
 be used to selectively ground the CSEL interface signal of the
 drive intended to be drive C (0). This drive will then function as
 the master. If CSEL is allowed to float the drive will recognize it-
 self as drive D (1) and function as the slave.


