
C P - 3 0 5 4 0    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    2243|     |     |
Capacity form/unform   545/      MB        Heads           6|     |     |
Seek time   / track  10.0/ 2.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST         Precompensation
Cache/Buffer           256 KB              Landing Zone
Data transfer rate    1.250 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %         5 95    |      5 95
       standby            W     Altitude    km    -0.061  3.048| -0.061 12.192
       idle           5.2 W     Shock        g         5       |     75
       seek           9.0 W     Rotation   RPM      5400
       read/write     6.5 W     Acoustic   dBA        40
       spin-up            W     ECC        Bit
                                MTBF         h     250000
                                Warranty Month        24
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
CONNER   CP30540 AEGEAN SCSI  CUSTOMER OPTIONS

  +---------------------------------------------------------+
  |                                                         |XX J2
  |       +-+                                               |XX
  |       | |J1                                             |XX
  |       | |HDA                                            |XX I
  |       | |                                        TERMPWR|XX N
  |       +-+                                            ++ |XX T
  |                                                      ++ |XX E
  |                                                         |XX R
  |                                                         |XX F
  |J3                                                       |XX A
  |+-+Spindle Sync                                          |XX C
  ||x|LED Drive                     E1++++++E5              |XX E
  ||x|                                ++++++                |X1
  |+-+                                                      |  1
  |+-+0E1                                                   |XX J4
  ||x| |                                                    |XX Power
  |+-+0E5 (Alternate LED Drive)                             |
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   CP30540 AEGEAN SCSI  CUSTOMER OPTIONS

 Jumper Setting
 ==============


 E1/0E1-E3/0E3 SCSI ID
 ---------------------
   +----------+-----------------------+
   | SCSI ID  |        Jumpers        |
   |          | E3/0E3| E2/0E2| E1/0E1|
   +----------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  |
   |    1     | OPEN  | OPEN  | CLOSED|
   |    2     | OPEN  | CLOSED| OPEN  |
   |    3     | OPEN  | CLOSED| CLOSED|
   |    4     | CLOSED| OPEN  | OPEN  |
   |    5     | CLOSED| OPEN  | CLOSED|
   |    6     | CLOSED| CLOSED| OPEN  |
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+
 There are three jumpers available for configuration of SCSI ID: E1,
 E2, and E3.

 Use either but not both: E1 to E3 OR 0E1 to 0E3. The 0E header is not
 installed on drive configurations with a LED on the PCBA.

 Delay Spin: A jumper in the E4 location, disables spin up on power-
 on. Disabling spin up on application of power can also be enabled by
 setting the DSPN bit in MODE SELECT page 0.

 E4 Disable Spin on Power on

 E5/0E5 Terminators on


 TERMPWR Output Enable



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
CONNER   CP31370  BAJA SCSI/CP30540 AEGEAN SCSI  CUSTOMER OPTIONS 1993

 Mounting Holes
 --------------
 Side:   6-32 UNC-2B .15 Max. Insertion
 Bottom: 6-32 UNC-2B .25 Max. Insertion



 J4   DC Power and pin connector assignments
 -------------------------------------------
 -------------------+
 --+  +-----J4-----+|  pin 1    +12 V
  1|  | 1  2  3  4 ||  pin 2    +12 Volts Return
  -+  +------------+|  pin 3    + 5 Volts Return
  ------------------+  pin 4    + 5 V


