
Q - 5 1 0    QUANTUM
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders     512|     |     |
Capacity form/unform     9/   11 MB        Heads           2|     |     |
Seek time   / track  45.0/10.0 ms          Sector/track   17|     |     |
Controller           MFM / ST412           Precompensation   256
Cache/Buffer               KB              Landing Zone
Data transfer rate    0.625 MB/S int       Bytes/Sector      512
                      0.625 MB/S ext
Recording method     MFM                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C        10 50    |    -40 62
Power: sleep              W     Humidity     %        20 80    |     10 95
       standby            W     Altitude    km            3.048| -0.305  9.144
       idle               W     Shock        g         5       |     30
       seek               W     Rotation   RPM      3529
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h      10000
                                Warranty Month        12
Lift/Lock/Park     -            Certificates     CSA,UL1950                   

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
QUANTUM  Q500  PRODUCT DESCRIPTION  OEM MANUAL 81-50125 REV. E DEC. 83

  +---------------------------------------------------------+
  |                                                         |XX
  |                                                         |XX J2
  |                                                         |XX
  |                                                         |XX
  |                                                     +-+ |
  |                                              Drive  | | |
  |+-+                                           Select | | |
  || |                                                  1-+ |XX
  || |P4                                        +--RN3---+  |XX
  || |                                          +--------+  |XX J1
  || |                                          Terminator  |XX
  |+-+                                                      |XX
  |                                                         |XX
  | +--E4                                                   |X1
  | +--+                                                    |
  |                 +---------P5                            |XX P3
  |                 +---------+                             |XX Power
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
QUANTUM  Q500 PRODUCT DESCRIPTION  OEM MANUAL 81-50125 REV. E, DEC. 83

 Jumper Setting
 ==============

 Drive Select
 ------------
 Five jumpers are provided for logical drive number assignment. DS1,
 DS2, DS3, DS4 cause the drive to be selected when the active drive
 select line matches the installed jumper. Jumper G, when installed,
 causes the drive to be selected constantly. The Quantum part number
 for the jumper plug is 22-10036.

   +-------+----------------------------+
   |Drive  |        Jumper              |
   |Select |   1      2      3      4   |
   +-------+-------+------+------+------+
   |  1    | CLOSED|OPEN  |OPEN  |OPEN  |
   +-------+-------+------+------+------+
   |  2    | OPEN  |CLOSED|OPEN  |OPEN  |
   +-------+-------+------+------+------+
   |  3    | OPEN  |OPEN  |CLOSED|OPEN  |
   +-------+-------+------+------+------+
   |  4    | OPEN  |OPEN  |OPEN  |CLOSED|
   +-------+-------+------+------+------+


 Control Cable Termination
 -------------------------
 If the Model Q500 is the last drive at the end of the control signal
 cable, a 220/330 ohm terminator pack must be installed at PCB
 location RN3. The terminator must be removed from RN3 is the drive is
 not at the end of a string of drives. The Quantum part number for the
 terminator pack is 13-12302.


