
R O 5 1 8 0 S    RODIME
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/HH              Cylinders    1219|     |     |
Capacity form/unform   144/  178 MB        Heads           7|     |     |
Seek time   / track  24.0/ 4.0 ms          Sector/track   33|     |     |
Controller           SCSI1 SINGLE-ENDED    Precompensation 65535
Cache/Buffer             4 KB FIFO BUFFER  Landing Zone
Data transfer rate    1.250 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |    -40 70
Power: sleep          7.0 W     Humidity     %        10 85    |
       standby       16.0 W     Altitude    km    -0.305  1.830|
       idle               W     Shock        g         2       |     30
       seek          23.0 W     Rotation   RPM      3600
       read/write         W     Acoustic   dBA        48
       spin-up            W     ECC        Bit   32
                                MTBF         h      30000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
RODIME   RO 5000S SERIES DISK DRIVE  PRODUCT SPECIFICATION PRO-21911

  +---------------------------------------------------------+
  |                                                         |XX P1
  |                                                  ++++++ |XX Power
  |                                       Terminators|||||| |
  |                                                  |||||| |
  |                                                  +1+1+1 |
  |                                                      6-5|
  |                                                   P3 | ||
  |                                                      2-1|
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                               SCSI      |XX P2
  |                                               Connector |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  +---------------------------------------------------------+2 1



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
RODIME   RO 5000S SERIES DISK DRIVE  PRODUCT SPECIFICATION PRO-21911

 Jumper Setting
 ==============


 P3  SCSI ID
 -----------
   +----------+-----------------------+
   | SCSI ID  |        Jumpers        |       +-2--4--6-+
   |          |  1-2  |  3-4  |  5-6  |       | o  o  o |
   +----------+-------+-------+-------+       | o  o  o |
   |    0     | OPEN  | OPEN  | OPEN  |       +-1--3--5-+
   |    1     | OPEN  | OPEN  | CLOSED|
   |    2     | OPEN  | CLOSED| OPEN  |    ID bit 2  Pin 2
   |    3     | OPEN  | CLOSED| CLOSED|    ID bit 1  Pin 4
   |    4     | CLOSED| OPEN  | OPEN  |    ID bit 0  Pin 6
   |    5     | CLOSED| OPEN  | CLOSED|  Pins 1, 3, and 5 are ground.
   |    6     | CLOSED| CLOSED| OPEN  |
   |    7     | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+


 DC Power and pin connector assignments
 --------------------------------------
 pin 1    +12 VDC
 pin 2    Ground
 pin 3    Ground
 pin 4    + 5 VDC



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
RODIME   RO 5000S SERIES DISK DRIVE  PRODUCT SPECIFICATION PRO-21911


 Drive Mounting and Installation
 -------------------------------
 The RO 5000S Series disk drives may be mounted in a host system in
 any orientation. The shipping lock automatically locks the actuator
 on power down, and releases the actuator when the power is reapplied
 and the spindle motor reaches proper speed.

 When installing the drive into an enclosure, the breather holes on
 the drive top cover must not be obstructed. At least 0.1-inch clear-
 ance must be provided between the top cover and the host frame.

 There must be at least 0.1-inch clearance between the drive housing
 and the host frame to ensure functional vibration isolation.

 The drive may be mounted in either a vertical or horizontal orienta-
 tion. It is supplied complete with antivibration mounts and threaded
 mounting brackets.

 Mounting Holes: 6-32-2A (12X), screw length 0.125 max.


 Physical Description
 --------------------
 SCSI devices are daisy-chained together using a common cable. Both
 ends of the cable are terminated. All signals are common between all
 SCSI devices.

 The RO 5000S uses single-ended drivers and receivers, which allow a
 maximum cable length of 29 feet (6 meters).


 Cable Requirements
 ------------------
 A 50-conductor flat cable or 25-signal twisted pair cable shall be
 used. The maximum cable length shall be 20 feet (6 meters).

 A stub length of no more than 4 inches (0.1 meters) is allowed off
 the mainline interconnection within any connected equipment.

 A minimum conductor size of 28 AWG shall be employed to minimize
 noise effects and ensure proper distribution of optional terminator
 power.


 Connector Requirements
 ----------------------
 The drive connector is a shrouded and keyed 50-pin connector
 consisting of two rows of 25 pins each on 2.54 mm (0.1 in) centers.

 The mating cable connector shall be a 50-pin connector consiting of
 two rows of 25 female contacts on 0.1 in (2.54 mm) center. The
 Connector should have an integral polarization bar which mates with
 the polarization notch on the drive connector. The 3M P/N 3425-6600
 cable connector is recommended.

 The power connector is a 4 pin AMP Mate-N-Look P/N 350211-1 mounted
 on the reverse side of the PCB. The recommended mating connector is
 AMP P/N 1-480424-0 socket housing use in AMP pin P/N 350078-4.


 Electrical Description
 ----------------------
 All assigned signal are terminated with 220 ohms to +5V (nominal) and
 330 ohms to ground at each end of the cable. All signals use open-
 collector drivers.


 Output Characteristics
 ----------------------
 Each signal driven by the RO 5000S has the following output
 characteristics when measured at the drive's connector:

     Signal assertion               = 0.0 volts dc to 0.4 volts dc.

     Minimum driver output capacity = 48 milliamps (sinking) at 0.5
                                      volts dc.

     Signal negation                = 2.5 volts dc to 5.25 volts dc.


 Input Characteristics
 ---------------------
 Each signal received by the RO 5000S shall have the following input
 characteristics when measured at the drive's connector:

     Signal true                    = 0.0 volts dc to 0.8 volts dc.

     Maximum toatl input load       = -0.4 milliamp at 0.4 volts dc.

     Signal false                   = 2.0 volts dc to 5.25 volts dc.

     Minimum input hysteresis       = 0.2 volts dc.


 Terminator Power (Optional)
 ---------------------------
 The RO 5000S is configured to supply terminator power,(TERMPWR), with
 the following characteristics:

 VTERM = 4.0 volts dc to 5.25 volts dc.

 800 milliamps minimum source drive capability.

 1.0 milliamp maximum sink capability.


 SCSI Bus
 --------
 Communication on the SCSI bus is allowed between only two SCSI
 devices at any given time, with a maximum of eight SCSI devices.

 Sample SCSI Configuration

   +--------+        +-----+ Single Initiator, Single Target
   |Computer+--------+Drive|
   +--------+SCSI Bus+-----+


   +--------+SCSI    +-----+ Single Initiator, Multiple Target
   |Computer+-----+--+Drive|
   +--------+Bus  |  +-----+
                  |  +-----+
                  +--+Drive|
                     +-----+


   +--------+SCSI Bus+-----+ Multiple Initiator, Multiple Target
   |Computer+-+---+--+Drive|
   +--------+ |   |  +-----+
   +--------+ |   |  +-----+
   |Computer+-+   +--+Drive|
   +--------+     |  +-----+
                  |  +-----+
                  +--+Drive|
                  |  +-----+
                  |  +-----+
                  +--+Drive|
                  |  +-----+
   +--------+     |  +-----+
   |Computer+-----+--+Drive|
   +--------+        +-----+


 Radio Frequency Interference
 ----------------------------
 The drive shall not be subjected to any electrical field which
 exceeds 2 volts per meter, RMS, in the range of 1.5 Hz to 1.0 GHz.


 Magnetic Field
 --------------
 There shall be no source of constant magnetic field which yield more
 than 0.0005 Tesla measured in the location occupied by the magnetic
 heads when the drive is installed.



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
RODIME   RO 5000S SERIES DISK DRIVE  PRODUCT SPECIFICATION PRO-21911


 Product Description
 ===================

 General
 -------
 The RO 5000S disk drive is a random access storage devices which use
 four 5.25-inch magnetic disks to provide up to 178 megabytes of
 unformatted on-line storage.

 The drive communicates with a host computer system via the Small
 Computer System Interface (SCSI) bus and is fully soft sectored.


 Features
 --------
 The RO 5000S disk drive is compatible with the SCSI bus definend by
 ANSI X3T9.2/82-2 Revision 17B and Common Command Set (CCS) Revisions
 4A and 4B.

 The following features are supported:

 - a 4K byte (16K optional) dual-ported FIFO data buffer
 - 10M bits/s disk transfer rate
 - disconnected operations with airbitration for reselection
 - command linking
 - 32-bit ECC error detection and correction
 - average data transfer rate of 1.25 megabytes/second
 - 1 : 1 interleave factor with any format between 128 and 1024 bytes
   per sector.
 - operation with arbitrating and non-arbitrating hosts
 - extended SCSI command set
 - diagnostics and error reporting.



 Seek Time
 ---------
       +----------------------------------+--------+
       |                                  | RO5000S|
       +----------------------------------+--------+
       |Single cylinder        msec.      |   4    |
       +----------------------------------+--------+
       |1219 cylinders         msec. max. |  44.0  |
       +----------------------------------+--------+
       |Average cylinder seek  msec.      |  24    |
       +----------------------------------+--------+


 Defect Handling
 ---------------
 Disc defects are handled by the RO 5000S using a sector sparing
 technique. During manufacture the drive is formatted using a format
 control code of 1EH. After this format, the drive allows the
 initiator access to all physical sectors. The drive is tested in this
 mode and any defective sectors are entered into a list known as the
 Primary Defect List or P-List. The P-List is stored in sectors 0 and
 10 of the special Maintenance Track. This track is physically
 Cylinder -2, Head 0 and is NOT part of the logical address space
 normally available to the user. The P-List can only be altered or
 erased by reformatting the maintenance track (Command E1H) or re-
 formatting the entire drive (Command 04H) using format control codes
 1EH or 16H.

 P-LIST: Maximum number of defective sectors = 30.

 Defects given to the drive during a RE-ASSIGN BLOCK command are
 appended to a Growing Defect List or GLIST. The GLIST is stored in
 sectors 3 and 13 of the maintenance track. The GLIST is stored in
 physical sector format and may be displayed by the READ DEFECT DATA
 command ONLY in physical sector format. The GLIST may be used, to-
 gether with the PLIST, during the FORMAT UNIT command with control
 code 00H or 10H. In this case, the two lists are searched together.
 On tracks with a single defect, the defect is skipped, on tracks with
 multiple defects, the track is re-assigned to the next available
 spare.

 The GLIST will be deleted if:
 The FORMAT MAINTENANCE TRACKS command is issued.
 or;
 A FORMAT UNIT command with control code 018H is issued.
 or;
 The sector size is changed and the drive is reformatted using a
 FORMAT UNIT command.

 G-List: Maximum number of defective sectors = 30.
         Maximum number defective tracks (Greater than 1 flaw):

                RO 5180S = 12
                RO 5125S = 12
                RO 5075S = 12


 LED ERROR CODES
 ---------------
 The following codes are presented by a sequence of four LED flashes
 of either long (L), or short (S) duration, repeating continuously:

 +--------+-----+---------------------------------------------------+
 |SEQUENCE|CODE |DEFINITION                                         |
 +-+-+-+--+-----+---------------------------------------------------+
 |S|S|S|L | 1   |The spindle motor speed is out of tolerance (+/-5%)|
 +-+-+-+--+-----+---------------------------------------------------+
 |S|S|L|S | 2   |ROM checksum diagnostic failure                    |
 +-+-+-+--+-----+---------------------------------------------------+
 |S|S|L|L | 3   |A write unsafe condition has been detected         |
 +-+-+-+--+-----+---------------------------------------------------+
 |S|L|S|S | 4   |Drive status has gone not not ready, due to a      |
 | | | |  |     |hardware fault                                     |
 +-+-+-+--+-----+---------------------------------------------------+
 |S|L|S|L | 5   |RAM buffer memory diagnostic failure               |
 +-+-+-+--+-----+---------------------------------------------------+
 |S|L|L|S | 6   |Head arm positioner servo failure                  |
 +-+-+-+--+-----+---------------------------------------------------+
 |S|L|L|L | 7   |The spindle motor did not start                    |
 +-+-+-+--+-----+---------------------------------------------------+
 |L|S|S|S | 8   |Spindle motor failed to attain +/-1% speed lock at |
 | | | |  |     |spinup                                             |
 +-+-+-+--+-----+---------------------------------------------------+
 |L|S|S|L | 9   |Power supplies fell below acceptable limits        |
 +-+-+-+--+-----+---------------------------------------------------+

 All the above error codes are designated FATAL, and resetting of the
 drive can only be accomplished by powering off, then on again.

 If the drive has a FATAL error, it will park and lock the heads, stop
 the spindle motor, and flash the fatal error code on the SELECT LED
 on the front panel. The drive will still respond to commands sent
 across the SCSI interface, but will not execute any of them except
 TEST DRIVE READY, INQUIRY or REQUEST SENSE.


 FAST BLINK LED
 --------------
 If the RESET signal on the SCSI interface is held active (low), the
 SELECT LED will flash rapidly. Check for the following conditions:

  1. Some other device on the bus is hung up, or has been powered
     down.

  2. A cable has been incorrectly installed.


