
M 2 2 4 1 A S    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 5.25"/FH              Cylinders     754|     |     |
Capacity form/unform    21/   27 MB        Heads           4|     |     |
Seek time   / track  83.0/18.0 ms          Sector/track   17|     |     |
Controller           MFM / ST412           Precompensation 66535
Cache/Buffer               KB              Landing Zone
Data transfer rate    0.625 MB/S int       Bytes/Sector      512
                      6.250 MB/S ext
Recording method     MFM                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 45    |    -40 60
Power: sleep              W     Humidity     %        20 80    |      5 95
       standby            W     Altitude    km            3.000|        12.000
       idle               W     Shock        g         2       |     30
       seek               W     Rotation   RPM      3600
       read/write    27.0 W     Acoustic   dBA        40
       spin-up            W     ECC        Bit
                                MTBF         h      10000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


