
S T 3 2 5 3 1 A         M E D A L I S T    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 4956|  619| 1024
Capacity form/unform  2557/      MB        Heads           6|   16|     |   16
Seek time   / track  12.5/ 3.5 ms          Sector/track     |   63|   63|   63
Controller           IDE / ATA3 ENHANCED   Precompensation
Cache/Buffer           128 KB MULTI-SEGMEN Landing Zone
Data transfer rate   11.000 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method     RLL 1/7,ZBR 2/3                operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %                 |
       standby        1.0 W     Altitude    km                 |
       idle           4.5 W     Shock        g         5       |     75
       seek           5.6 W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA        34
       spin-up            W     ECC        Bit   SMART
                                MTBF         h     300000
                                Warranty Month        36
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST32531A/33240A MEDALIST 2531AT/3240AT  JUMPER SETTING

 Jumper Setting
 ==============


               J2                   5  12
  +----------------------------+--1+V--V+
  |XXXXXXXXXXXXXXXXXXXXXXXXXXXX|:::|OOOO|POWER
  +----------------------------+++++----+
   Pin 20 removed               ||+--- RESERVED
                                |+-+-- Slave Present (when Master ON)
                                |  +-- Cable Select (when Slave OFF)
            o o1                +----- Master ON, Slave OFF
            o o2
            | +-- Full capacity (as shipped from factory)
            +---- Limit capacity to 2.1 GB (4092 cylinders)


 Limit Capacity jumper sets the default cylinder translation
 to 4092 to solve issues with certain BIOS that only auto-detect.
 Total available sectors are still at full capacity as reported via
 Identify Drive data words 52-61. Third party partitioning software
 may be needed to achieve full capacity if this option jumper is used.


