
S W I F T   9 4 3 5 4 - 1 3 3    CDC
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders    1272|  636|  477|  962
Capacity form/unform   117/  133 MB        Heads           5|   10|    8|   14
Seek time   / track  15.0/ 4.0 ms          Sector/track   36|   36|   60|   17
Controller           IDE / AT              Precompensation
Cache/Buffer            32 KB SEGMENTED    Landing Zone
Data transfer rate    1.250 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL 2/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      3600
       read/write    11.0 W     Acoustic   dBA
       spin-up            W     ECC        Bit   32,56
                                MTBF         h     150000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST1156/1133/1111-A  PRODUCT DESCRIPTION

  +------------------------------------------------------+Power
  |                                                      |XXXX
  |                                                      |1234
  |                                                      |
  |                                                      |X1
  |                                                      |XX AT
  |                                                      |XX INTERFACE
  |                                                      |XX CONNECTOR
  |                                                      |XX
  |                                                      |XX
  |                                                      |XX
  |                                                      |XX
  |                                                      |XX
  |                                                      |+-1 OPTIONS
  |                                             10 or 14 || | JUMPER
  |                                             pin      || | BLOCK
  +------------------------------------------------------++-+




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST1156/1133/1111-A  PRODUCT DESCRIPTION

 Jumper setting
 --------------

 x = Jumpers set from factory

 10-pin and 14-pin version have the same pin definition for pins 1-10.
 The 14-pin version has 4 additional pins (11-14)

 Master/Slave Jumper
 -------------------
       1-2  OPEN        Master
            CLOSED      Slave

 If only one drive is installed, configure the drive as a master. If
 there are two drives installed on the bus, one must be configured as
 a master and the other as a slave. No more than two drives can be
 connected on the AT bus.
 To configure the drive as a slave, install a jumper on pins 1 and 2
 of the the 12-pin user configuration jumper block.
 To configure the drive as a master, leave pins 1 and 2 of the options
 jumper block open.


 3-4 Head Configuration
 ----------------------
       3-4  CLOSED     5 Heads
            OPEN       7/9 Heads


 Slave-Present Jumper
 --------------------
       5-6  OPEN        Slave not installed
            CLOSED      Slave installed

 If both the master and the slave are Swift AT interface drives, you
 do not need this jumper. This is because the master can detect the
 presence of the slave using the interface DASP-signal state.
 If the drives in your application do not implement the DASP-signal,
 install the jumper on the master drive only, (The slave drive ignores
 this jumper).
 To tell the master that a slave is present, install a jumper on pins
 5 and 6 of the options jumper block on the master drive.


 ECC Jumper
 ----------
       7-8  OPEN        4 ECC Bytes
            CLOSED      7 ECC Bytes

 This jumper setting selects the number of ECC bytes transferred to or
 from the host during read long and write operations. (The media
 always uses seven ECC bytes. The jumper only controls the number of
 bytes transferred.)

   - If you install a jumper on pins 7 and 8 of the options jumper
     block, seven ECC bytes are transferred.

   - If you do not install a jumper on pins 7 and 8 of the options
     jumper block, four ECC bytes are transferred.


 Factory Test Jumper
 -------------------
       9-10 OPEN        Normal Operation
            CLOSED      Factory Test

 Pins 9 and 10 are used for testing during the manufacturing process;
 they are not for field use.


 11-12/13-14  Factory Use
 ------------------------
 Some PWA's have these pins
 FACTORY USE!


 Remote LED
 ----------
      A   B
    +---+---+    Default jumper at C-D for LED mounted on drive PWA
    | * | * |    To use remote LED, remove jumper and extend B (Anode)
    +---+---+    and D (Cathode).
    | * | * |
    +---+---+
      C   D

 Swift LED kit 75912397 allows connection to a remote LED.
 Swift LED kit 95913369 has an LED for attachment to the system front
 bezel or a 5.25-inch frame kit.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
SEAGATE  ST1156/1133/1111-A  PRODUCT DESCRIPTION

 Notes on installation
 =====================

 Drive mounting
 --------------

     horizontally             vertically
   +-----------------+   +--+             +--+ +------------------+
   |                 |   |  +-----+ +-----+  | |                  | x
   |                 |   |  |     | |     |  | x+----------------+x
 +-+-----------------+-+ |  |     | |     |  | ||x              x||
 +---------------------+ |  |     | |     |  | ||  x          x  ||
                         |  |     | |     |  | ||    x      x    ||
      x           x      |  |     | |     |  | ||      x  x      ||
 +------x------x-------+ |  +-----+ +-----+  | ||       xx       ||
 +-+------x--x-------+-+ +--+             +--+ ||     x    x     ||
   |       xx        |                         ||   x        x   ||
   |     x    x      |                         || x            x ||
   +---x--------x----+                         |x                x|
     x            x                           x++----------------++x
      UNACCEPTABLE!                                UNACCEPTABLE!

 The drive may be mounted in the following positions:

  1. Horizontally, with the drive's PC board on the top drive.

  2. Horizontally, with the drive's PC board on the bottom of the
     drive.

  3. Vertically, on either side.

 Do not mount the drive vertically on either end.

 For optimum performance, format the drive in the same orientation as
 it is be mounted in the host system.

 Caution: To avoid potential service problems, observe the following
 precautions:

  - Handle the drive by the edges or frame. Do not pressure on the top
    cover or touch the circuit board.

  - Do not remove or cover factory-installed labels. They contain in-
    formation needed to service the product.

  - Do not put labels over the breather holes on the top surface of
    the drive. The breather holes must remain clear to allow air
    circulate.

 - If a label, oher than a factory-installed label, has been placed
   over the breather holes, remove it. Do not poke holes through the
   label. This damages the filter underneath, allowing contaminants to
   enter the drive.

 - Do not use solvents to remove the adhesive residue from drive
   labels. Small amounts of solvent may get into the unit and contami-
   nate the disc.

 - Do not plug a live DC power cable into the drive power connector.
   This damages the connector contacts.


 (Allready low-level formatted at the factory)


