
S T 9 1 4 0 A G    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        |  980|     |
Capacity form/unform   128/      MB        Heads           4|   15|     |
Seek time   / track  16.0/ 5.0 ms          Sector/track     |   17|     |
Controller           IDE / AT              Precompensation
Cache/Buffer           120 KB ADAPTIVE     Landing Zone
Data transfer rate    2.800 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C                 |
Power: sleep          0.1 W     Humidity     %                 |
       standby        0.1 W     Altitude    km                 |
       idle           0.6 W     Shock        g       100       |    150
       seek           1.7 W     Rotation   RPM      3545
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST9140/9550/9190/9145AG  PRODUCT SPECIFICATION

  +---------------------------------------------------------+
  |                                                         |XX
  |                                                         |XX 44-pin
  |                                                         |XX I
  |                                                         |XX N
  |                                                         |XX T
  |                                                         |XX E
  |                                                         |*X R
  |                                                         |XX F
  |                                                         |XX A
  |                                                         |XX C
  |                                                         |XX E
  |                                                         |XX1
  |                                                         |+-+
  +---------------------------------------------------------++-+
                                                            Master/
                                                            Slave




**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST9140/9550/9190/9145AG  PRODUCT SPECIFICATION

 Jumper Setting
 ==============

 Master/Slave selection
 ----------------------
    Interface                              J1      Jumper
   +-------------------------------------------+   +------+
   |o o o o o o o o o o o o o o o o o o o o o 1|   | A  C |
   |o o o o o o o o o o o o * o o o o o o o o o|   | B  D |
   44------------------------------------------+   +------+
 ---------------------------------------------------------PWA------

 Pin 41   +5VDC
 Pin 42   +5VDC
 Pin 43   GND
 Pin 44   Reserved
 Drive uses +5VDC power supplied to the drive via the interface
 connector. The drive does NOT make use of a +12VDC power line.

 Pin-20 removed for keying


   Jumper for Pins        Configuration
   A and B   C and D
   ------------------------------------------------------------------
   OPEN      OPEN       Drive is Master, no Slave present
   CLOSED    OPEN       Drive is Master, Seagate Slave drive present
   OPEN      CLOSED     Drive is Slave to another Seagate 2.5" Master
   CLOSED    CLOSED     Reserved Position (Do not use)


