
M 2 9 5 4 W S    FUJITSU
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    5713|     |     |
Capacity form/unform  4350/ 5000 MB        Heads           9|     |     |
Seek time   / track   9.0/ 1.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/WI/FAST      Precompensation
Cache/Buffer           506 KB MULTI-SEGMEN Landing Zone
Data transfer rate    9.400 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     PR4ML                          operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 50    |    -40 60
Power: sleep              W     Humidity     %        20 80    |      5 95
       standby            W     Altitude    km            3.000|        12.000
       idle               W     Shock        g         5       |     50
       seek               W     Rotation   RPM      7200
       read/write    10.0 W     Acoustic   dBA        34
       spin-up            W     ECC        Bit   ON THE FLY
                                MTBF         h    1000000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      G   E   N   E   R   A   L
**********************************************************************
NEVER








                 Announced but never produced.

                        NEVER PRODUCED!!!


