
D T C A - 2 3 2 4 0   T R A V E . 4 G T    IBM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        | 6304|     |
Capacity form/unform  3240/      MB        Heads            |   16|     |
Seek time   / track  13.0/ 4.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA3            Precompensation
Cache/Buffer            96 KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 65
Power: sleep          0.1 W     Humidity     %         8 90    |      5 95
       standby        0.3 W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle           1.9 W     Shock        g       100       |    500
       seek           2.3 W     Rotation   RPM      4000
       read/write     2.2 W     Acoustic   dBA
       spin-up            W     ECC        Bit   ENHANCED, ON THE FLY,SMART
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
IBM      DTCA-23240/24090  TRAVELSTAR 4GT



              +--------------------------------------+
              |                                      |
              |                                      |
              |                                      |
              +--------Interface-------------49------+
              |       **********************1 **47 Jumper
              |       *************x********* **48   |
              +------44----------------------50------+
              +                                      +

 Pin position 20 is left blank for secure connector insertion.








**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
IBM      DTCA-23240/24090  JUMPER SEWTTING

 Jumper Setting
 ==============

 Drive Address Setting
 ---------------------
 A jumper is available at the interface connector to determine the
 drive address.

 Using Cable Selection, the drive address depends on the condition of
 pin 28 of the AT interface cable. In the case when pin 28 is ground
 or low, the drive is a Master. If pin 28 is open or high level, the
 drive is a Slave.


