
M H A - 2 0 2 1 A T    FUJITSU
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders    6372| 4200|     |
Capacity form/unform  2160/      MB        Heads           4|   16|     |
Seek time   / track  13.0/ 2.5 ms          Sector/track     |   63|     |
Controller           IDE / ATA3            Precompensation
Cache/Buffer           128 KB              Landing Zone
Data transfer rate    6.000 MB/S int       Bytes/Sector      512
                     16.600 MB/S ext PIO4
Recording method     PR4ML                          operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 65
Power: sleep          0.2 W     Humidity     %         8 90    |      5 95
       standby        0.2 W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle           0.9 W     Shock        g       100       |    300
       seek           2.5 W     Rotation   RPM      4000
       read/write         W     Acoustic   dBA        30
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  MHA-2021/2032AT  SWITCH SETTINGS

  +---------------------------------------------------------+
  |                                                         |XX
  |                                                         |XXI
  |                                                         |XXN
  |                                                         |XXT
  |                                                         |XXE
  |                                                         |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  |                                                         |XX
  |                                                         1XX
  |                                                         |xxJumper
  +---------------------------------------------------------+





**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  MHA-2021AT/2032AT  SWITCH SETTINGS

 Jumper Setting
 ==============


  +CNH1--1-----Interface---------  MASTER
  |* *   * * * * * * * *
  |* *   * * * * * *
  +------------------


  +CNH1--1-----Interface---------  SLAVE
  |* *   * * * * * * * *
  |xxx   * * * * * *
  +B-D---2-----------


  +A-C---1-----Interface---------  CABLE SELECT
  |xxx   * * * * * * * *
  |* *   * * * * * *
  +------------------

 The CSEL setting is not depended on setting between pins B and D.


 By connecting the CSEL of the master device to the CSEL Line
 (conductor) of the cable and connecting it to ground further, the
 CSEL is set to low level.

 The device is identified as a master device. At this time, the CSEL
 of the slave device does not have a conductor. Thus, since the slave
 device is not connected to the CSEL conductor, the CSEL is set to
 high level. The device is identified as a slave device.


