
S T 3 3 2 2 0 A         M E D A L I S T    SEAGATE
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        | 6253|  751| 1024
Capacity form/unform  3227/      MB        Heads           4|   16|     |   16
Seek time   / track  12.0/ 1.1 ms          Sector/track     |   63|   63|   63
Controller           IDE / ATA3 ULTRA      Precompensation
Cache/Buffer           128 KB              Landing Zone
Data transfer rate   11.500 MB/S int       Bytes/Sector      512
                     33.300 MB/S ext UDMA2
Recording method     PRML 16/17,ZBR                 operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby        0.8 W     Altitude    km                 |
       idle           4.3 W     Shock        g        10       |     75
       seek           5.5 W     Rotation   RPM      4490
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST33220A  JUMPERSETTINGS

 Jumper Setting
 ==============

                         J2  40 pin I/O Cable Connection
                         |   pin-20 removed
                         |
              +----------|---------+-------1-+---------+    TOP (HDA)
           ---+::::::::::*::::::::1| : : : : | X X X X +----
              +--------------------+-8-+-+-+-+-5-G-G-12+    BOTTOM
                                     | | | |
              Master ON, Slave OFF --+ | | |
    Slave Present (when Master ON) ----+ | |
     Cable Select (when Slave OFF) ----+ | |
                          Reserved ------+ |
                    Limit capacity --------+

 Limit Capacity jumper sets the default cylinder translation
 to 4092 to solve issues with certain BIOS that only auto-detect.
 Total available sectors are still at full capacity as reported via
 Identify Drive data words 52-61. Third party partitioning software
 may be needed to achieve full capacity if this option jumper is used.


