
M 1 6 1 4 T A U    FUJITSU
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    4133| 2114|     |
Capacity form/unform  1091/      MB        Heads           4|   16|     |
Seek time   / track  11.0/ 3.0 ms          Sector/track     |   63|     |
Controller           IDE / ATA2 FAST/ENHA  Precompensation
Cache/Buffer            64 KB FIFO RING    Landing Zone
Data transfer rate    6.000 MB/S int       Bytes/Sector      512
                     16.700 MB/S ext PIO4
Recording method     PRML 8/9                       operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep          1.0 W     Humidity     %         8 80    |      5 95
       standby            W     Altitude    km    -0.300  3.000| -0.300 12.000
       idle           4.2 W     Shock        g         5       |     75
       seek           4.6 W     Rotation   RPM      4500
       read/write         W     Acoustic   dBA        32
       spin-up            W     ECC        Bit
                                MTBF         h     300000
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
FUJITSU  M1612/14T  JUMPER SETTING

  +---------------------------------------------------------+
  |                                                         |
  |                                                         |XXI
  |                                                         |XXN
  |                                                  CNH1   |XXT
  |                                                 5++++1  |XXE
  |                                                 6++++2  |XXR
  |                                                         |XXF
  |                                                         |XXA
  |                                                         |XXC
  |                                                         |XXE
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX +5V
  |                                                         |XX RETURN
  |                                                         |XX +12V
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
FUJITSU  M1612/M1614TAU  SWITCH AND JUMPER SETTINGS

 Jumper Setting
 ==============

 Terminal CNH1
 -------------
     +---+
   1 |* *| 2
   3 |* *| 4
   5 |* *| 6
     +---+

 Pins  |  Status  | Function
 ------+----------+--------------------------
 2-4   |  SHORT*  | Select drive as MASTER
       |  OPEN    | Select drive as SLAVE
 ------+----------+--------------------------
 4-6   |  SHORT   | CSEL selection method
       |  OPEN    | Standard selection method


 CSEL provides for an alternative method for selection of the MASTER
 and SLAVE configurations. A special cable is needed to implement
 this feature and should only be used if supported by BOTH drives.
 CSEL should only be used in conjunction with a slave and without
 ACMODE.


