
H P   D 3 5 8 1 A    HEWLETT PACKARD
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |     |     |
Capacity form/unform  1000/      MB        Heads            |     |     |
Seek time   / track  11.0/     ms          Sector/track     |     |     |
Controller           SCSI2 SI/WI/SCA/FAST  Precompensation
Cache/Buffer           512 KB WRITE CACHE  Landing Zone
Data transfer rate    7.100 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method                                    operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     800000
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
HEWLETT  HP D3583A/D3582A/D3591A NETSERVER DRIVES










     The drive configures automatically in dependence of the Slot
     position.


