
C P - 2 2 5 4    CONNER
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/HH               Cylinders    1339|  489|     |
Capacity form/unform   250/      MB        Heads           6|   16|     |
Seek time   / track      /     ms          Sector/track     |   63|     |
Controller           IDE / AT              Precompensation
Cache/Buffer               KB              Landing Zone
Data transfer rate          MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage                  Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates


**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
CONNER   QUICK INSTALLATION GUIDE L-511-1008 11/93 AT-BUS

 QUICK INSTALLATION GUIDE
 ------------------------
 AT-BUS
 ------
 Table 1
 +---------------------------------------+
 |Single Drive = Jumper ACT and C/D      |
 |Master Drive = Jumper ACT, C/D and DSP |
 |Slave Drive  = No jumpers installed    |
 +---------------------------------------+

 Table 2
 +------------------------------------+
 |Single Drive = Jumper C/D           |
 |Master Drive = Jumper C/D and E-1   |
 |Slave Drive  = No jumpers installed |
 +------------------------------------+

 Table 3
 +-----------------------------------+
 |Single Drive = Jumper E-1          |
 |Master Drive = Jumper E-1          |
 |Slave Drive  = No jumpers installed|
 +-----------------------------------+

 Table 4
 +-----------------------------------+
 |Single Drive = Jumper M/S          |
 |Master Drive = Jumper M/S          |
 |Slave Drive  = No jumpers installed|
 +-----------------------------------+

 Table 5
 +-----------------------------------+
 |Single Drive = Jumper C/D          |
 |Master Drive = Jumper C/D          |
 |Slave Drive  = No jumpers installed|
 +-----------------------------------+

 Table 6
 +-----------------------------------+
 |Single Drive = Jumper C/D          |
 |Master Drive = Jumper C/D and DSP  |
 |Slave Drive  = No jumpers installed|
 +-----------------------------------+

 Table 7
 +----------------------------------+
 |Single Drive = Jumper C/D and DSP |
 |Master Drive = Jumper C/D and DSP |
 |Slave Drive  = Jumper DSP         |
 +----------------------------------+

 Table 8
 +---------------------------------+
 |Single Drive = Jumper Pins 1-2   |
 |Master Drive = Jumper Pins 1-2   |
 |Slave Drive  = No Jumper Pins 1-2|
 +---------------------------------+


 LED Configuration Table
 -----------------------
 Letter  Connector  LED+   LED-
   A       J-4      Pin 1  Pin 2
   B       J-1      Pin 3  Pin 4
   C       J-5      Pin 3  Pin 4
   D       J-3      Pin 3  Pin 4
   E       J-7      Pin 1  Pin 2
   F       J-5      Pin 7  Pin 8


 All Conner drives are shipped with jumpers to configure the drive in
 the Single (Master) mode.

 Conner drives are low-level formatted at the factory.


