
D S P - 3 0 5 3 L R    DEC
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    3177|     |     |
Capacity form/unform   535/  684 MB        Heads           4|     |     |
Seek time   / track   9.5/ 1.0 ms          Sector/track     |     |     |
Controller           SCSI2 SI/FAST/SCA     Precompensation
Cache/Buffer           512 KB SEGMENTED    Landing Zone
Data transfer rate    4.000 MB/S int       Bytes/Sector      512
                     10.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 60
Power: sleep              W     Humidity     %        10 90    |      8 95
       standby            W     Altitude    km    -0.061  3.048|        12.192
       idle           7.5 W     Shock        g        10       |     45
       seek           9.0 W     Rotation   RPM      5400
       read/write         W     Acoustic   dBA        34
       spin-up            W     ECC        Bit   264
                                MTBF         h     500000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,FCC,TUV,UL1950,VDE



**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
DEC      DSP3000LR SERIES  PRODUCT DESCRIPTION EK-RH3CA-PD.A01

 80-pin SCSI Connector (8/16-bit) (Raid)
 ---------------------------------------
      +--------------------------------------------------+
      |       Back View                                  |
      |                                                  |
      +--------------------------------------------------+
      |   +-----------------------------------------+    |
      |   |                                         J1   |
      |   +-----------------------------------------+    |
      +----------Combination-Connector-------------------+
      +                                                  +


      +--------------------------------------------------+
      |       Front View (Bezel End)                     |
      |                                                  |
      |                                                  |
      +--------------------------------------------------+
      +--------------------------------------------------+
      |                                                  |
      +                                                  +





  +---------------------------------------------------------+
  |                                         Active     ++   |
  |                                         Termination++   |+-+
  |                                                         || |
  |                                                         || |
  |                                                         || | J1
  |                                                         || |
  |                                                         || |
  |                                                         || |
  |                                                         || |
  |                                                         || |
  |                                                         || |
  |                                                         || |
  |                                                         || |
  |                                                         || |
  |                                                         |+-+
  |                                                         |
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
DEC      DSP3000LR SERIES  INSTALLATION GUIDE EK-RH3CA-IG.A01

 Jumper Setting
 ==============

 TERMPWR (Terminator Power)
 --------------------------
 NOTE
 LR Models do not provide TERMPWR to the SCSI bus. The RAID connector
 does not accommodate this feature.


 SCSI Bus Termination
 --------------------
 Both ends of the SCSI bus cable must be terminated. One end is
 terminated at the host. The other end must be terminated by the last
 SCSI device on the SCSI bus.


 Drive Termination
 -----------------
 DSP3000L Series drives contain internal components to provide active
 termination of the SCSI bus.

 When this drive is the last device on the SCSI bus, configure the
 drive to enable active termination. Do so by installing a shunt
 jumper at the drive's active termination header. If active
 termination is not required for this drive, make sure that the
 jumper is not installed.


 Active Termination - LR Models
 ------------------------------

                        |
                    xxx |Install shunt jumper to enable active
      ---------------+--+termination
        -------------+
        80-pin connector



 SCSI ID (Address) Selection
 ---------------------------
 Each device on the SCSI bus must have a unique SCSI ID number
 assigned to it.

 ID number for L/LD models (8-bit SCSI) range from 0 through 7. For
 LW/LWD models (16-bit SCSI), the numbers range from 0 through 15.

 SCSI ID numbers for LR models range from 0 through 7 for 8-bit
 configurations and from 0 through 15 for 16-bit configurations.

 Configure the SCSI ID of L/LD/LW/LWD models by installing jumper
 across the indicated Option connector pins. For LR versions, provide
 the proper open or ground signal input to the referenced pins of the
 drive's 80-pin RAID connector.


 SCSI ID - LR Models
 -------------------

   +----------+-------------------+  Combination Connector (J1) Pin 79
   | SCSI ID  |  Jumper Location  | +---------------------------+---+
   |          | ID3| ID2| ID1| ID0| |  xxxxxxxxxxxxxxxxxxxxxxxxxx80 |
   |          | P80| P40| P79| P39| |  xxxxxxxxxxxxxxxxxxxxxxxxxx40 |
   +----------+----+----+----+----+ +---------------------------+---+
   |    0     | 0  | 0  | 0  | 0  |                             Pin 39
   |    1     | 0  | 0  | 0  | 1  |
   |    2     | 0  | 0  | 1  | 0  |
   |    3     | 0  | 0  | 1  | 1  |
   |    4     | 0  | 1  | 0  | 0  |
   |    5     | 0  | 1  | 0  | 1  |
   |    6     | 0  | 1  | 1  | 0  |
   |    7     | 0  | 1  | 1  | 1  |
   |    8*    | 1  | 0  | 0  | 0  |
   |    9*    | 1  | 0  | 0  | 1  |
   |   10*    | 1  | 0  | 1  | 0  |
   |   11*    | 1  | 0  | 1  | 1  |
   |   12*    | 1  | 1  | 0  | 0  |
   |   13*    | 1  | 1  | 0  | 1  |
   |   14*    | 1  | 1  | 1  | 0  |
   |   15*    | 1  | 1  | 1  | 1  |
   +----------+----+----+----+----+

 1 = GND, -0.5V to +0.4V
 0 = OPEN CKT, +0.5V to 2.4V

 * SCSI ID 8-15 only on 16-bit SCSI


 Configure Optional Features
 ---------------------------
 CAUTION
 The 5-volt signals of two or more drives should not be connected
 together or to any other current source by using the Option
 connector. Doing so may cause drive malfunction or component damage.

 Except when connecting several drives together for a spindle
 synchronization application, do not connect the ground signals of two
 or more drives together or to any other current source using the
 Option connector. Doing so may introduce ground loop problems.

 The following optional features can be configured according to your
 system requirements. These features (model-dependent) include:

 - Notification of AC power failure (not currently supported by LR
   models. SCSI RST may be used instead.)

 - Spindle synchronization

 - Write protection (not currently supported by LR models)

 - Spin delay


 AC Failure Notification
 -----------------------
 The AC Low connection (AC_LOW L) is not currently supported on LR
 models, SCSI Bus Reset provides the alternative to the AC Low
 warning.


 Spindle Synchronization
 -----------------------
 DSP3000L Series drives support synchronized spindle operation. Master
 or slave synchronized operation is set through a SCSI Mode Select
 Page.

 When the drive operates as a Master, it generates a spindle
 synchronization reference signal (SPINDLE_SYNC_REF L). When operating
 as a slave, the drive synchronizes its spindle according to the
 SPINDLE_SYNC_REF L input reference. The drive always maintains local
 speed regulation when no reference signal is applied.

 NOTE
 The reference signal must originate from drives with the same
 electronics modules. Fo example, connect Model DSP3107L only with
 another DSP3107L drive. Do not connect the SPINDLE_SYNC_REF L signal
 so that of any other model disk drive. Otherwise, the drive may mal-
 function.

 When connecting multiple drives together for spindle synchronization,
 be sure to use proper cabling techniques to avoid ground loop
 problems.


 Spindle Sync Connection
 -----------------------
                    Combination Connector
    DSP3053LR      +-------------------------------+
    DSP3107LR      |  xxxxxxxxxxxxxxxxxxxxxxxxxx   |
    DSP3133LR      |  xxxxxxxxxxxxxxxxxxxxxxxxxx   |
                   +-------------------------+-----+
                                             Pin 37
                                             Spindle Sync

 Spin Delay
 ----------
 The method for establishing spin-up characteristics is dependent upon
 the drive model.

 Spin Delay - LR Models
 ----------------------
 Spin delay (spin-up) characteristics for LR models are determined by
 the state of the RMT_START (pin 38) and DLYD_START (pin 78) inputs to
 the 80-pin RAID connector. The states of these signals are set by
 using either hard-wired connections at the backplane or backplane
 logic.

 Spin-up characteristics are configured to provide one of the follo-
 wing options.

 - Spin-up at drive power on (Option 1)

 - Spin-up upon receipt of SCSI Start command (Option 2)

 - Spin-up after a predetermined delay following power up. Delay is
   equal to 12 seconds (typical) times the drive's numeric SCSI ID
   (Option 3)

 NOTE
 LR models that do not implement any of the listed spin delay options
 should be configured for Option 2.


 The following chart describes spin-up characteristics for LR model
 drives:

             Combination Connector +----- Pin 78
           +-----------------------+--+   DLYD_START
           | xxxxxxxxxxxxxxxxxxxxxxxx |
           | xxxxxxxxxxxxxxxxxxxxxxxx |
           +-----------------------+--+
                                   +----- Pin 38
                                          RMT_START
      +---------+-----------+----------+
      |Option   | DLYD_START| RMT_START|
      |         | Pin 78    | Pin 38   |
      +---------+-----------+----------+
      |Option 1 | OPEN      | OPEN     |
      +---------+-----------+----------+
      |Option 2 | OPEN      | GROUND   |
      +---------+-----------+----------+
      |Option 3 | GROUND    | OPEN     |
      +---------+-----------+----------+


 Remote Features
 ---------------
 DSP3000L Series drives support the following remote features, which
 can be configured at the drive's Option connector or RAID backplane:

  - Remote SCSI ID selection
  - Remote LED status display


 Remote SCSI ID Selection
 ------------------------
 SCSI ID can be set remotely from an external (remote) switch or
 control panel. For L/LD/LW/LWD models, this is accomplished using the
 Option connector. For LR models, the output of the remote or external
 ID switches takes the place of jumpers or circuits at the RAID system
 backplane.

 To configure LR models, connect the output of the remote or external
 switch to the RAID backplane instead of using backplane jumpers or
 circuits.

 Remote LED Status Display
 -------------------------
 LR models provide the ACTIVITY LED OUT signal which can be used to
 drive a user-supplied remote LED.


 ACTIVITY LED OUT signal - LR Models
 -----------------------------------
 LR models do not contain a busy or fault LED. Rather, they provide an
 output to drive a user-supplied activity LED.

 The ACTIVITY LED OUT signal indicates the drive is performing a SCSI
 operation. Connect the cathode of the user-supplied LED to the
 ACTIVITY LED OUT connection. The LED anode must be attached to the
 proper +5 VDC supply through an appropriate current-limiting
 resistor.

               Combination Connector   +- ACTIVITY LED OUT (Pin 77)
   DSP3053LR   +-----------------------+--+
   DSP3107LR   | xxxxxxxxxxxxxxxxxxxxxxxx |
   DSP3133LR   | xxxxxxxxxxxxxxxxxxxxxxxx |
               +--------------------------+



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
DEC      DSP3000L SERIES  INSTALLATION GUIDE EK-RH3CA-IG.A01

 Notes on installation
 =====================

 Drive mounting
 --------------

     horizontally             vertically
   +-----------------+   +--+             +--+ +------------------+
   |                 |   |  +-----+ +-----+  | |                  |
   |                 |   |  |     | |     |  | |+----------------+|
 +-+-----------------+-+ |  |     | |     |  | ||                ||
 +---------------------+ |  |     | |     |  | ||                ||
                         |  |     | |     |  | ||                ||
                         |  |     | |     |  | ||                ||
 +---------------------+ |  +-----+ +-----+  | ||                ||
 +-+-----------------+-+ +--+             +--+ ||                ||
   |                 |                         ||                ||
   |                 |                         ||                ||
   +-----------------+                         ||                ||
                                               ++----------------++

 You can mount the disk drive in any position. LR models mount in RAID
 storage subsystems. The drive (with bezel) attaches to the system bay
 and accept #6-32 screws. Screws should not exceed 0.25 inch
 (6.25 millimeters) in length, otherwise damage to the PCB may result.


 Mounting and Bezel Options
 --------------------------
 Bezels and mounting brackets are available from Digital Equipment
 Corporation for mounting the drive in either 3.5-inch or 5.25-inch
 form factor bays.


 Combination Connector - L/LD Models
 -----------------------------------
  +-----------------+-----------------------------------------------+
  | Part Number     | Vendor                                        |
  +-----------------+-----------------------------------------------+
  | 12-36486-01     | Digital Equipment Corp.                       |
  +-----------------+-----------------------------------------------+
  | 89331-001       | Berg Electronics (formerly Dupont Electronics)|
  +-----------------+-----------------------------------------------+
  | CWN-710-54-0119 | C.W. Industries                               |
  +-----------------+-----------------------------------------------+
  | DA-2339-25      | Methode Electronics                           |
  +-----------------+-----------------------------------------------+
    Includes 0.1-in pitch, 50-pin SCSI connector and 4-pin power
    connector.


 Combination Connector - LW/LWD Models
 -------------------------------------
  +-----------------+-----------------------------------------------+
  | Part Number     | Vendor                                        |
  +-----------------+-----------------------------------------------+
  | 12-40413-01     | Digital Equipment Corp.                       |
  +-----------------+-----------------------------------------------+
  | 92-1814-12-1    | AMP, Inc.                                     |
  +-----------------+-----------------------------------------------+
    Includes 68-pin SCSI connector, 4-pin power connector, and a
    2-mm pitch, 12-pin (2x6) Option connector.


 Option Connector - L/LD Models
 ------------------------------
  +-----------------+-----------------------------------------------+
  | Part Number     | Vendor                                        |
  +-----------------+-----------------------------------------------+
  | 12-36484-02     | Digital Equipment Corp.                       |
  +-----------------+-----------------------------------------------+
  | 90516-003       | Berg Electronics (formerly Dupont Electronics)|
  +-----------------+-----------------------------------------------+
  | 3-176837-3      | AMP, Inc.                                     |
  +-----------------+-----------------------------------------------+
  | 87049-2091      | Molex, Inc.                                   |
  +-----------------+-----------------------------------------------+
    A 2-mm pitch, 19-pin (2x10) keyed (missing pin) connector


 Secondary Option Connector - LW/LWD Models
 ------------------------------------------
  +-----------------+-----------------------------------------------+
  | Part Number     | Vendor                                        |
  +-----------------+-----------------------------------------------+
  | 12-36484-05     | Digital Equipment Corp.                       |
  +-----------------+-----------------------------------------------+
    A 2-mm pitch, 5-pin (2x3) keyed (missing pin) connector


 Shunt Jumper - All Models
 -------------------------
  +-----------------+-----------------------------------------------+
  | Part Number     | Vendor                                        |
  +-----------------+-----------------------------------------------+
  | 12-36482-01     | Digital Equipment Corp.                       |
  +-----------------+-----------------------------------------------+
  | 86730-001       | Berg Electronics (formerly Dupont Electronics)|
  +-----------------+-----------------------------------------------+
  | LPC-SPG         | Honda                                         |
  +-----------------+-----------------------------------------------+
    A 2-mm pitch shunt for configuring termination characteristics


 RAID Connector - LR Models
 --------------------------
  +-----------------+-----------------------------------------------+
  | Part Number     | Vendor                                        |
  +-----------------+-----------------------------------------------+
  | TBS             | Digital Equipment Corp.                       |
  +-----------------+-----------------------------------------------+


 DC Power and pin connector assignments
 --------------------------------------
      +------------+   pin 1    +12 VDC
      | 4  3  2  1 |   pin 2    +12 Volts Return GROUND
      +------------+   pin 3    + 5 Volts Return GROUND
                       pin 4    + 5 VDC



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
DEC      DSP3000L SERIES  INSTALLATION GUIDE EK-RH3CA-IG.A01

 Product Summary
 ---------------
 DSP3000L Series 3.5-inch Disk Drives are high-performance, high
 capacity drives, designed and manufactures by Digital Equipment
 Corporation.


 Features
 --------
 Features of the DSP3000L Series drives include the following:

 - Formatted capacity ranging from 535 MB to 1,377.5 MB, depending
   upon model

 - 1 millisecond track-to-track seek time

 - 512 KB segmented cache buffer

 - End-to-end Error Detection Code/Parity on cache RAM

 - Four headers per sector

 - Embedded quadrature servo

 - Self-diagnostics

 - Down-loadable SCSI firmware

 - Tagged command queuing

 - Seek ordering

 - Automatic block realloction

 - Glitch-free power on/off operation

 - Synchronized spindle operation

 - Low power consumption


 Power-On Tests
 --------------
 After power is applied, and before spin-up is completed, the drive
 performs self-test diagnostics prior to making itself visible on the
 SCSI bus. These intitial self-test check most of the electronics that
 control HDA, but not the SCSI transceiver or SCSI connector.

 After spin-up, additional tests complete self-test coverage of the
 electronics module and the HDA. The unit appears not ready to the
 host between completion of the initial self-tests and completion of
 the drive's post spin-up tests.


 Seek Time
 ---------
       +----------------------------------+--------+--------+--------+
       |                                  |DSP3053L|DSP3107L|DSP3133L|
       +----------------------------------+--------+--------+--------+
       |Track-to-Track         msec. typ. |   1    |   1    |   1    |
       +----------------------------------+--------+--------+--------+
       |Average                msec. typ. |   9.5  |   9.5  |   9.5  |
       |                       msec. max. |  20    |  20    |  20    |
       +----------------------------------+--------+--------+--------+
       |Latency                msec. avg. |   5.6  |   5.6  |   5.6  |
       +----------------------------------+--------+--------+--------+


 LED Indicators
 --------------
 The green Busy LED illuminates to signify the drive is working on a
 SCSI command. The amber Fault LED indicates a fault status.

 Both the Busy and Fault indicators light briefly during power up.
 This serves as a hardware and lamp test.

 During a calibration operation, the Busy LED is illuminated and the
 Fault LED flashes. Calibrations occur following some firmware up-
 grades. Generally, calibration periods last only about five minutes,
 after which the drive comes on-line and both indicators go out.

 If the Fault indicator lights at any other time, the drive has failed
 and likely requires service (unless the Fault LED was turned on by
 means of a MODE SELECT command).

 Remote Busy and Fault indicators can be connected to the Option
 connector to provide status display at a remote location or panel.


