
S T 3 2 4 3 0 W D       H A W K   2 L P    SEAGATE
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders    3898|     |     |
Capacity form/unform  2147/ 2600 MB        Heads           9|     |     |
Seek time   / track   9.8/ 1.5 ms          Sector/track     |     |     |
Controller           SCSI2 DI/WI/FAST      Precompensation
Cache/Buffer           512 KB LOOK-AHEAD   Landing Zone
Data transfer rate    5.000 MB/S int       Bytes/Sector      512
                     20.000 MB/S ext SYNC
Recording method     RLL 1/7                        operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C         5 55    |    -40 70
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle           6.5 W     Shock        g                 |
       seek               W     Rotation   RPM      5411
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     800000
                                Warranty Month        60
Lift/Lock/Park     YES          Certificates


**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
SEAGATE  ST32430W/3620W  PRODUCT DESCRIPTION

  +---------------------------------------------------------+
  |                                                         |XX1
  |                                                         |XXPower
  |                                                         |1-+
  |                                                         || J5
 ++LED                                                      || |
 ++                                                         |+-+
  |                                                         |+1+
  |                                                         ||X|I/O
  |                                                         ||X|
  |                                                         ||X|
  |                                                         ||X|J1
  |                                                         ||X|
  |+-+                                                      ||X|
  || |J6                                                    ||X|
  |+-1                                8--------1            ||X|
  |                                   +--------+J2          |+-+
  +---------------------------------------------------------+



**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
SEAGATE  ST32430W/3620W  PRODUCT DESCRIPTION

 Jumper Setting
 ==============



   REAR VIEW                             +------ 5V
                                         | +---- GND
     (TOP)                               | | +-- GND
      34                   1         1   | | | + 12V
      +---------------------+  +-J5---+ +-------+
  ----+|||||||||||||||||||||+--+::::::+-+O O O O+-
      +---------------------+  +------+ +-------+
      68pin I/O Cable           ||||||    Power   SCSI ID = 0 (none)
      Connection                |||||+----------- SCSI ID = 1
                                ||||+------------ SCSI ID = 2
                                |||+---------+--- SCSI ID = 4 or pin-6
                                |||          +--- REFIND+
                                ||+-------------- SCSI ID = 8
                                |+--------------- pin-10 GND
                                +---------------- pin-11 +5V

 J5  SCSI ID
 -----------
   +----------+-------------------------------+
   | SCSI ID  |       Jumper Location         |
   |          |             PINS              |
   |          |  7-8  |  5-6  |  3-4  |  1-2  |
   +----------+-------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |    2     | OPEN  | OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |    3     | OPEN  | OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |    4     | OPEN  | CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    5     | OPEN  | CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |    6     | OPEN  | CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |    7     | OPEN  | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |    8     | CLOSED| OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    9     | CLOSED| OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |   10     | CLOSED| OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |   11     | CLOSED| OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |   12     | CLOSED| CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |   13     | CLOSED| CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |   14     | CLOSED| CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |   15     | CLOSED| CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+


 RIGHT SIDE VIEW

   +-J1                                  TOP (HDA)
   |X+------------+--------+-----PWA--------------------Front of drive
   +-+            |12345678|J2
                  +--------+
  +Terminator PWR -+||||||+- RESERVED
  +Terminator PWR --+||||+-- Start Delay (12 secs * ID)
  |  Enable T-Res ---+||+--- Motor Start
  | Parity Enable ----++---- Write Protect
  |
  |
  Terminator Power-source Table
  -----------------------------
  1 2             1 2             1 2
 +----           +----           +----
 |X o            |o X            |o o
 |X o            |o X            |xxx
 +------         +------         +-------
 Drive Supplies  Drive Supplies  Bus Supplies
 Bus             Own             Drive


 FRONT VIEW                                   J6
                TOP (HDA)                  +-----1+
 -------PWA--------------------------------+::::::+---
              ++                           +------+  SCSI ID = 0 none
              ++LED            pin-11 +5V --+||||+-- SCSI ID = 1
                               pin-10 GND ---+||+--- SCSI ID = 2
                           SCSI ID = 8 or -+--++--+- SCSI ID = 4 or
                           pin-8 BUSY     -+      +- pin-6 REFIND+

 NOTE
 If these ID jumper are used, the ID jumpers J5 ARE NOT USED!!!!!

 J6  SCSI ID
 -----------
   +----------+-------------------------------+
   | SCSI ID  |       Jumper Location         |
   |          |             PINS              |
   |          |  7-8  |  5-6  |  3-4  |  1-2  |
   +----------+-------+-------+-------+-------+
   |    0     | OPEN  | OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    1     | OPEN  | OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |    2     | OPEN  | OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |    3     | OPEN  | OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |    4     | OPEN  | CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    5     | OPEN  | CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |    6     | OPEN  | CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |    7     | OPEN  | CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |    8     | CLOSED| OPEN  | OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |    9     | CLOSED| OPEN  | OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |   10     | CLOSED| OPEN  | CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |   11     | CLOSED| OPEN  | CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+
   |   12     | CLOSED| CLOSED| OPEN  | OPEN  |
   +----------+-------+-------+-------+-------+
   |   13     | CLOSED| CLOSED| OPEN  | CLOSED|
   +----------+-------+-------+-------+-------+
   |   14     | CLOSED| CLOSED| CLOSED| OPEN  |
   +----------+-------+-------+-------+-------+
   |   15     | CLOSED| CLOSED| CLOSED| CLOSED|
   +----------+-------+-------+-------+-------+



**********************************************************************
                      F   E   A   T   U   R   E  S
**********************************************************************
SEAGATE  ST32430W/WD/WC/DC/31230W/WD/WC/DC  INSTALL. GUIDE 77767478

 Before you begin
 ----------------
 Verify that the system is switched off and disconnected from main
 power before any installation is attempted.

 Protect yourself, the drive, and your  valuable programs and data by
 reading the following cautions and warnings.

 - Do not tamper with sealed top cover. Doing so voids your warranty.
   The drive contains no user serviceable components. See Product
   Repair section for more information.

 - Visually inspect the shipping container for any obvious damage.

 - Verify all parts listed on shipping bill are received with the
   equipment. Discrepancies or damage should be reported to the
   shipping company.

 - Inspect drive for possible shipping damage. All claims of this type
   should be filed promptly with the transporter involved. Save
   original packing materials to be used when reshipping.

 - When transporting or shipping a drive or system, please ensure that
   they are correctly packed in original Seagate approved (or
   equivalent) container and shipped via an airride carrier
   experienced in handling computer equipment.

 - Do not unpack drive from its static shielded bag until you are
   ready to install it in the system.

 -  Always handle the drive by the frame or casting.

 - Do not touch Printed Circuit Board (PCB) or the I/O connector pins.

 - Never apply pressure to the PCB or to the drive top cover.

 Caution. The circuit assemblies and components contained in this
 equipment can be degraded or destroyed by Electrostatic Overstress
 (EOS) or by Electrostatic Discharge (ESD).

 Static electrical charges can accumulate quickly on personnel,
 clothing and synthetic materials. The electrostatic fields due to
 these charges when brought in close proximity to susceptible circuit
 assemblies and components, can result in degraded reliability or
 immediate failure of the affected component or assembly.

 To insure optimum reliable equipment operation, it is required that
 technical support personnel discharge themselves by wearing a
 grounding strap around the wrist and be connected to a grounding
 terminal while working in the vicinity of, and while handling EOS/
 ESD susceptible assemblies/parts. If unavailable, ground yourself
 frequently by touching the metal chassis of the system before
 handling any components (this helps only if the system is connected
 to a ground). Avoid static-inducing carpeted areas. This procedure
 is especially important when handling printed circuit boards (PCB's).


 Safety instructions
 -------------------
 1. The disc drive(s) are to be installed in a customer supplied
    enclosure where the surrounding air does not exceed 50 o C.
 2. Four (4) 6-32 UNC-2A screws are required for installation. Maximum
    screw length into side of drive is 0.15 inches (3.81 mm). Maximum
    screw length into bottom is 0.20 in. (5.08 mm). Maximum screw
    tightening torque is 6.0 in-lb (.675 NM) with minimum thread
    engagement of 0.12 in (3.05 mm).
 3. The power requirements are shown in the Product Information
    section.
 4. The power supply must satisfy the safety requirements for SELV
    (Safety Extra Low Voltage) cir-cuits.
 5. Service is to be provided by trained Seagate service personnel.
 6. The incorporation of the disc drives listed in this guide into a
    customer enclosure must meet the appropriate safety requirements
    of the country in which it is used (e.g. UL 1950, CAN/CSA-C22.2
    No. 950-M89, DIN VDE 0805:1993 and EN60950: 1992 (IEC 950).
    Note. Power must be off when connecting or disconnecting.

 - CMOS configuration: SCSI drives should not be defined in the CMOS.
   The SCSI host adapter uses its own BIOS to handle the Input/Output
   procedures.

 The CMOS setting for SCSI drive is either drive type zero, or the no
 drive installed option.


 Low-Level formatting: All Hawk 2LP wide family drive models are
 low-level formatted at the factory and do not require this step
 during installation. If an installed drive is low-level formatted,
 all user data will be lost.

 Note: Seagate Technology assumes no liability for lost user data.

 Partitioning and high level formatting: A drive can be subdivided
 into "partitions" which behave as individual drives within the
 system. Consult the system documentation for instructions on
 partitioning and high level formatting. Information is also available
 in bookstores and libraries.


 Product repair information
 --------------------------
 Service requirements
 The special facilities required for the manufacture of these drives
 generally prohibit repair in the field. If problems occur during
 installation, please contact your supplier for assistance. Do not
 attempt to disassemble or repair. Drives should be sent to the repair
 depot through the purchase source, if possible. Please observe
 the following cautions.

 Caution!
 - Handle drive with care. Do not drop, or bump hard.
 - Never remove the cover of these disc drives. Servicing items in the
   sealed HDA (heads, media, actuator, etc.) require special
   facilities. The drive contains no user purchasable parts or PCBs.
 - Opening the sealed HDA voids the drive warranty.
 - Applying a soldering device to the components on the PCB voids the
   drive warranty.
 - Do not connect or disconnect cables without first removing power
   from the drive.
 - Place drive on a flat, static dissipative surface and handle with
   extreme care. Always follow all EOS/ESD precautions to avoid
   damage to the electrical assemblies.

 Shipping
 When transporting or shipping a drive, a Seagate approved container
 must be used. Keep your original box. They are easily identified by
 the Seagate Approved Package label. Shipping a drive in a
 non-approved container voids the drive warranty.

 Seagate repair centers may refuse receipt of components improperly
 packaged or obviously damaged in transit. Contact your Authorized
 Seagate Distributor to purchase additional boxes. Seagate recommends
 shipping by an air-ride carrier experienced in handling computer
 equipment.


 Initial setup information
 -------------------------
 For the initial setup connect the cables or plug into a mounted
 connector (if applicable), set the drive ID on the bus and enable or
 disable the I/O line terminator resistor packs (Hawk 2LP family "W"
 models only).

 These procedures are described in paragraphs following.
 Note whether drive model number ends in W, WD, WC or DC.


 Write precompensation and reduced write current
 -----------------------------------------------
 Not required on Seagate SCSI Interface drives covered by this manual.


 Do not power up the host system until the drive is mounted and the
 system cover is replaced.

 Connect DC power connector to the drive ("W/WD" models only).

 Replace the Host System cover.

 Turn on DC power.

 Boot the system from the floppy drive or from a previously installed
 hard-drive if there is one.

 Proceed with drive setup of the new hard drive.


 SCSI interface drives
 ---------------------
 The SCSI interface handles both drive geometry and defect management
 internally. The "no drive installed" option is selected for systems
 with SCSI drives.

 All SCSI interface drives are low-level formatted at the factory. You
 may wish to low-level format the drive to optimize its performance
 for your system. Consult the controller documentation for information
 on low-level formatting. Partitioning and high-level formatting can
 be done through DOS by way of the FDISK utility for partitioning, and
 FORMAT for high-level formatting.

 Consult your DOS manual for FORMAT and FDISK command options.


