
P R O D R I V E   L P S   1 2 7   A T    QUANTUM
NO MORE PRODUCED                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 3.5"/SLIMLINE         Cylinders        |  919|     |
Capacity form/unform   127/      MB        Heads            |   16|     |
Seek time   / track  14.0/     ms          Sector/track     |   17|     |
Controller           IDE / AT              Precompensation
Cache/Buffer           128 KB              Landing Zone
Data transfer rate    1.250 MB/S int       Bytes/Sector      512
                            MB/S ext
Recording method     RLL                            operating  | non-operating
                                                  -------------+--------------
Supply voltage     5/12 V       Temperature *C                 |
Power: sleep              W     Humidity     %                 |
       standby            W     Altitude    km                 |
       idle               W     Shock        g                 |
       seek               W     Rotation   RPM
       read/write         W     Acoustic   dBA
       spin-up            W     ECC        Bit
                                MTBF         h     350000
                                Warranty Month
Lift/Lock/Park     YES          Certificates     CSA,TUV,UL1950,VDE           

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
QUANTUM  PRODRIVE LPS 127/170/340 AT  UNIVERSAL CONFIGURATION CARD


  +---------------------------------------------------------+
  |                                             JP1+-+-+-+  |XX
  |                                                +-+-+-+  |XX
  |                                                SP DS CS |XX
  |                                                         |XX
  |                                                         |XX AT-Bus
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |XX
  |                                                         |
  |                                                         |
  +---------------------------------------------------------+





**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
QUANTUM  PRODRIVE LPS 127/170/340 AT  UNIVERSAL CONFIGURATION CARD

 Jumper setting
 ==============


 JP1  Drive Select/Cable Select/Slave Present
 --------------------------------------------
   +------+------+------+--------------------------------------------+
   |DS    |CS    |SP    | Description                                |
   +------+------+------+--------------------------------------------+
   |OPEN  |OPEN  |OPEN  | Slave Drive                                |
   |      |      |      | Compatible with drive using PDIAG- line to |
   |      |      |      | handle Master/Slave communications         |
   +------+------+------+--------------------------------------------+
   |OPEN  |OPEN  |CLOSED| Slave Drive                                |
   |      |      |      | The PDIAG- and DASP- lines are not driven  |
   +------+------+------+--------------------------------------------+
   |CLOSED|OPEN  |OPEN  | Master Drive                               |
   |      |      |      | Uses DASP- to check for the presence of a  |
   |      |      |      | Slave                                      |
   +------+------+------+--------------------------------------------+
   |CLOSED|OPEN  |CLOSED| Master Drive                               |
   |      |      |      | Uses the SP jumper to determine whether a  |
   |      |      |      | Slave is present, without checking PDIAG-  |
   |      |      |      | or DASP-                                   |
   +------+------+------+--------------------------------------------+
   |OPEN  |CLOSED|   X  | Slave or Master Drive, depending on the    |
   |      |      |      | state of the Quantum Cable Select signal   |
   |      |      |      | (pin 28) at the IDE-bus interface          |
   |      |      |      | connector.                                 |
   |      |      |      | If the signal state is set to OPEN         |
   |      |      |      | (grounded) then the drive is configured a  |
   |      |      |      | if DS were CLOSED, described above. If the |
   |      |      |      | Cable Select signal is set to CLOSED       |
   |      |      |      | (high), then the drive is configured as if |
   |      |      |      | DS were OPEN, described above.             |
   +------+------+------+--------------------------------------------+

 X indicates the jumper setting does not matter.

 Caution: The CS and DS jumpers should never be installed at the same
          time.


 DS  Drive Select Jumper
 -----------------------
 You can configure two drives on the ATA Interface as Master (Drive 0)
 and Slave (Drive 1) using the DS jumpers. Set the CS jumpers to OPEN
 for each drive. Then, set the DS Jumper to CLOSED on one drive to
 configure that drive as Master. Set the DS jumper to OPEN on the
 other drive to configure as Slave.

 Note: For drives configured using the DS jumper, the order in which
       drives are connected in a daisy chain has no significance.


 CS  Cable Select Jumper
 -----------------------
 When two ProDrive LPS 127/170/340AT hard disk drives are daisy-
 chained together, they can be configured as Master and Slave by using
 the CS jumper or by using the DS jumper - BUT NOT BOTH. To configure
 the two drives using the CS jumper, set the CS jumper to CLOSED and
 the DS jumper to OPEN on each drive.

 Once you install the CS jumper, the drive is configured as a Master
 or Slave by state of the Cable Select signal, which is pin 28 at the
 IDE-bus interface connector. Quantum uses pin 28 as a vendor-specific
 pin; it does NOT conform to the function normally allocated for this
 pin according to the ATA (AT Attachment).

 Pin 28 is grounded - that is, set to OPEN - on the cable coming from
 the host. This configures the first drive as Master. Then, pin 28 on
 the connector at the second drive should be made an open circuit by a
 cut in signal line 28 in the cable from the first drive, so it
 becomes high - that is, set to CLOSED - due to a pull-up in the
 second drive. This configures the second drive as a Slave.


 SP  Slave Present Jumper
 ------------------------
 The SP jumper normally is not needed. However, when the ProDrive LPS
 127/170/340AT is configured as Master and is connected to a Slave
 drive that does not implement the Drive Active/Slave Present (DASP-)
 signal, it is necessary to set the SP jumper to CLOSED on the
 ProDrive LPS 127/170/340AT.


