
D C X A - 2 1 0 0 0 0           1 0 G T    IBM
                                                      Native|  Translation
                                                      ------+-----+-----+-----
Form                 2.5"/SUPERSLIMLINE    Cylinders        |16383|     |
Capacity form/unform 10050/      MB        Heads            |   16|     |
Seek time   / track  12.0/     ms          Sector/track     |   63|     |
Controller           IDE / ATA ENHANCED    Precompensation
Cache/Buffer           460 KB SEGMENTED    Landing Zone
Data transfer rate   12.500 MB/S int       Bytes/Sector      512
                     33.300 MB/S ext UDMA2
Recording method     PRML                           operating  | non-operating
                                                  -------------+--------------
Supply voltage     5 V          Temperature *C         5 55    |    -40 65
Power: sleep          0.1 W     Humidity     %         8 90    |      5 95
       standby        0.3 W     Altitude    km    -0.300  3.048| -0.300 12.192
       idle           0.7 W     Shock        g       125       |    600
       seek           2.3 W     Rotation   RPM      4200
       read/write     2.1 W     Acoustic   dBA
       spin-up        4.7 W     ECC        Bit   ENHANCED, ON THE FLY,SMART
                                MTBF         h
                                Warranty Month
Lift/Lock/Park     YES          Certificates                                  

**********************************************************************
                        L   A   Y   O   U   T
**********************************************************************
IBM      DCXA-210000/208100 TRAVELSTAR 10GT  INSTALLATION GUIDE


              +--------------------------------------+
              |                                      |
              |                                      |
              |                                      |
              +--------Interface-------------49------+
              |     43**********************1 **47 Jumper
              |     44*************x********* **48   |
              +------------------------------50------+
              +                                      +

 Pin position 20 is left blank for correct connector insertion.

 Pin position 47 through 50 are used for drive address setting.







**********************************************************************
                      J   U   M   P   E   R   S
**********************************************************************
IBM      DCXA-210000/208100  TRAVELSTAR 10GT  INSTALLATIONS

 Jumper Setting
 ==============

 Master/Slave Drive Address Setting
 ----------------------------------
 A jumper is available at the interface connector to determine the
 drive address.

   ---49--47+
    *   * X | Slave
    *   * X |
   ---50--48+


   ---49--47+
    *   * * | Master
    *   * * |
   ---50--48+


   ---49--47+
    *   * * | Cable Selection
    *   xxx |
   ---50--48+


   ---49--47+
    *   xxx |
    *   * * | RESERVED Never attach a jumper here!
   ---50--48+


   ---49--47+
    *   X * | NEVER ATTACH A JUMPER HERE!!!
    *   X * |
   ---50--48+


 Cable Selection
 ---------------
 Using Cable Selection, the drive address depends on the condition of
 pin 28 of the AT interface cable. In the case when pin 28 is ground
 or low, the drive is a Master. If pin 28 is open or high level, the
 drive is a Slave.


 Cabling
 -------
 The maximum cable length from the host system to the HDD plus circuit
 pattern in the host system shall not exceed 18 inches.


 AT Signal Connector
 -------------------
 The AT signal connector is designed to mate with Dupont part number
 69764-044 or equivalent.



**********************************************************************
                      I   N   S   T   A   L   L
**********************************************************************
IBM      DCXA-210000/208100  TRAVELSTAR 10GT  JUMPER SETTINGS

 Notes on installation
 =====================

 Installation direction
 ----------------------

     horizontally                           vertically
   +-----------------+             +--+                       +--+
   |                 |             |  +-----+           +-----+  |
   |                 |             |  |     |           |     |  |
 +-+-----------------+-+           |  |     |           |     |  |
 +---------------------+           |  |     |           |     |  |
                                   |  |     |           |     |  |
                                   |  |     |           |     |  |
 +---------------------+           |  +-----+           +-----+  |
 +-+-----------------+-+           +--+                       +--+
   |                 |
   |                 |
   +-----------------+

 The drive will operate in all axis (6 directions).

 Performance and error rate will stay within specification limits if
 the drive is operated in the other permissible orientations from
 which it was formatted. Thus a drive formatted in a horizontal
 orientation will be able to run vertically and vice versa.

 The drive must be securely mounted in the system to prevent motion or
 vibration during a seek operation or spindle rotation using
 appropriate screws or equivalent mounting hardware.

 The recommended mounting screw torque is 3.0   0.5 kgf.cm.

 The recommended mounting screw depth is 3.0   0.3mm for bottom and
 3.5   0.5mm for horizontal mounting.


 Air Cooling Requirement
 -----------------------
 The host system must provide sufficient air flow across the drive to
 maintain the temperature at less than 60*C (measured at the centre of
 the files top cover).


